<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.7.0">
<drawing>
<schematic>
<libraries>
<library name="fab">
<packages>
<package name="SOIC14">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="QFN/MLF20">
<description>&lt;b&gt;HP-VFQFP-N20&lt;/b&gt; Micro Lead Frame package (MLF)</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT 23&lt;/b&gt;</description>
</package>
<package name="EFOBM">
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R1206W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="R1206FAB">
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1206K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1206 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 3216</description>
</package>
<package name="C1206FAB">
</package>
<package name="2X03SMD">
</package>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="LED1206">
<description>LED 1206 pads (standard pattern)</description>
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="5MM">
<description>5mm round through hole part.</description>
</package>
<package name="SPDTSWITCH">
</package>
</packages>
<symbols>
<symbol name="ATTINY24/44/84">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="(PCINT7/ICP/OC0B/ADC7)PA7"/>
<pin name="(PCINT6/OC1A/SDA/MOSI/ADC6)PA6"/>
<pin name="(PCINT5/OC1B/MISO/DO/ADC5)PA5"/>
<pin name="(PCINT4/T1/SCL/USCK/ADC4)PA4"/>
<pin name="(PCINT3/T0/ADC3)PA3"/>
<pin name="(PCINT2/AIN1/ADC2)PA2"/>
<pin name="(PCINT1/AIN0/ADC1)PA1"/>
<pin name="(PCINT0/AREF/ADC0)PA0"/>
<pin name="(PCINT11/RESET/DW)PB3"/>
<pin name="(PCINT10/INT0/OC0A/CKOUT)PB2"/>
<pin name="(PCINT9/XTAL2)PB1"/>
<pin name="(PCINT8/XTAL1/CLKI)PB0"/>
</symbol>
<symbol name="REGULATOR">
<pin name="IN"/>
<pin name="GND"/>
<pin name="OUT"/>
</symbol>
<symbol name="CERAMIC_RESONATOR">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="R-US">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="C-US">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="AVRISP">
<pin name="MISO" direction="pas" function="dot"/>
<pin name="VCC" direction="pas" function="dot"/>
<pin name="SCK" direction="pas" function="dot"/>
<pin name="MOSI" direction="pas" function="dot"/>
<pin name="RST" direction="pas" function="dot"/>
<pin name="GND" direction="pas" function="dot"/>
</symbol>
<symbol name="LED">
<description>LED</description>
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="SPDTSWITCH">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ATTINY44" prefix="IC">
<gates>
<gate name="1" symbol="ATTINY24/44/84"/>
</gates>
<devices>
<device name="-SSU" package="SOIC14">
<connects>
<connect gate="1" pin="(PCINT0/AREF/ADC0)PA0" pad="13"/>
<connect gate="1" pin="(PCINT1/AIN0/ADC1)PA1" pad="12"/>
<connect gate="1" pin="(PCINT10/INT0/OC0A/CKOUT)PB2" pad="5"/>
<connect gate="1" pin="(PCINT11/RESET/DW)PB3" pad="4"/>
<connect gate="1" pin="(PCINT2/AIN1/ADC2)PA2" pad="11"/>
<connect gate="1" pin="(PCINT3/T0/ADC3)PA3" pad="10"/>
<connect gate="1" pin="(PCINT4/T1/SCL/USCK/ADC4)PA4" pad="9"/>
<connect gate="1" pin="(PCINT5/OC1B/MISO/DO/ADC5)PA5" pad="8"/>
<connect gate="1" pin="(PCINT6/OC1A/SDA/MOSI/ADC6)PA6" pad="7"/>
<connect gate="1" pin="(PCINT7/ICP/OC0B/ADC7)PA7" pad="6"/>
<connect gate="1" pin="(PCINT8/XTAL1/CLKI)PB0" pad="2"/>
<connect gate="1" pin="(PCINT9/XTAL2)PB1" pad="3"/>
<connect gate="1" pin="GND" pad="14"/>
<connect gate="1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-PU" package="DIL14">
<connects>
<connect gate="1" pin="(PCINT0/AREF/ADC0)PA0" pad="13"/>
<connect gate="1" pin="(PCINT1/AIN0/ADC1)PA1" pad="12"/>
<connect gate="1" pin="(PCINT10/INT0/OC0A/CKOUT)PB2" pad="5"/>
<connect gate="1" pin="(PCINT11/RESET/DW)PB3" pad="4"/>
<connect gate="1" pin="(PCINT2/AIN1/ADC2)PA2" pad="11"/>
<connect gate="1" pin="(PCINT3/T0/ADC3)PA3" pad="10"/>
<connect gate="1" pin="(PCINT4/T1/SCL/USCK/ADC4)PA4" pad="9"/>
<connect gate="1" pin="(PCINT5/OC1B/MISO/DO/ADC5)PA5" pad="8"/>
<connect gate="1" pin="(PCINT6/OC1A/SDA/MOSI/ADC6)PA6" pad="7"/>
<connect gate="1" pin="(PCINT7/ICP/OC0B/ADC7)PA7" pad="6"/>
<connect gate="1" pin="(PCINT8/XTAL1/CLKI)PB0" pad="2"/>
<connect gate="1" pin="(PCINT9/XTAL2)PB1" pad="3"/>
<connect gate="1" pin="GND" pad="14"/>
<connect gate="1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MU" package="QFN/MLF20">
<connects>
<connect gate="1" pin="(PCINT0/AREF/ADC0)PA0" pad="5"/>
<connect gate="1" pin="(PCINT1/AIN0/ADC1)PA1" pad="4"/>
<connect gate="1" pin="(PCINT10/INT0/OC0A/CKOUT)PB2" pad="14"/>
<connect gate="1" pin="(PCINT11/RESET/DW)PB3" pad="13"/>
<connect gate="1" pin="(PCINT2/AIN1/ADC2)PA2" pad="3"/>
<connect gate="1" pin="(PCINT3/T0/ADC3)PA3" pad="2"/>
<connect gate="1" pin="(PCINT4/T1/SCL/USCK/ADC4)PA4" pad="1"/>
<connect gate="1" pin="(PCINT5/OC1B/MISO/DO/ADC5)PA5" pad="20"/>
<connect gate="1" pin="(PCINT6/OC1A/SDA/MOSI/ADC6)PA6" pad="16"/>
<connect gate="1" pin="(PCINT7/ICP/OC0B/ADC7)PA7" pad="15"/>
<connect gate="1" pin="(PCINT8/XTAL1/CLKI)PB0" pad="11"/>
<connect gate="1" pin="(PCINT9/XTAL2)PB1" pad="12"/>
<connect gate="1" pin="GND" pad="8"/>
<connect gate="1" pin="VCC" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="REGULATOR" prefix="IC" uservalue="yes">
<gates>
<gate name="G$1" symbol="REGULATOR"/>
</gates>
<devices>
<device name="SOT23" package="SOT23">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RESONATOR">
<gates>
<gate name="G$1" symbol="CERAMIC_RESONATOR"/>
</gates>
<devices>
<device name="" package="EFOBM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RES-US" prefix="R" uservalue="yes">
<description>&lt;b&gt;Resistor (US Symbol)&lt;/b&gt;
&lt;p&gt;
Variants with postfix FAB are widened to allow the routing of internal traces</description>
<gates>
<gate name="G$1" symbol="R-US"/>
</gates>
<devices>
<device name="1206" package="R1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206W" package="R1206W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206FAB" package="R1206FAB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAP-US" prefix="C">
<gates>
<gate name="G$1" symbol="C-US"/>
</gates>
<devices>
<device name="1206" package="C1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206K" package="C1206K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206FAB" package="C1206FAB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AVRISP">
<gates>
<gate name="G$1" symbol="AVRISP"/>
</gates>
<devices>
<device name="SMD" package="2X03SMD">
<connects>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="MISO" pad="1"/>
<connect gate="G$1" pin="MOSI" pad="4"/>
<connect gate="G$1" pin="RST" pad="5"/>
<connect gate="G$1" pin="SCK" pad="3"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="2X03">
<connects>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="MISO" pad="1"/>
<connect gate="G$1" pin="MOSI" pad="4"/>
<connect gate="G$1" pin="RST" pad="5"/>
<connect gate="G$1" pin="SCK" pad="3"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED">
<description>LED</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="LED1206">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FAB1206" package="LED1206FAB">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5MM" package="5MM">
<connects>
<connect gate="G$1" pin="A" pad="IN"/>
<connect gate="G$1" pin="C" pad="OUT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPDTSWITCH">
<gates>
<gate name="G$1" symbol="SPDTSWITCH"/>
</gates>
<devices>
<device name="" package="SPDTSWITCH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X16">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X16/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="PINHD16">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="PINHD-1X16" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD16"/>
</gates>
<devices>
<device name="" package="1X16">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X16/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="fab2">
<packages>
<package name="3.5MMTERM">
</package>
<package name="ED555DS-2DS">
</package>
</packages>
<symbols>
<symbol name="1X2">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="TERM-1X02" prefix="J">
<description>3.5mm terminal block, 2 positions ED555-2DS as found in the fablab inventory. 
&lt;p&gt;Stolen from &lt;a href="http://www.ladyada.net/library/pcb/eaglelibrary.html"&gt;Adafruit&lt;/a&gt;, adapted by Zaerc.</description>
<gates>
<gate name="G$1" symbol="1X2"/>
</gates>
<devices>
<device name="-ADAFRUIT" package="3.5MMTERM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-FABLAB" package="ED555DS-2DS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<parts>
<part name="IC1" library="fab" deviceset="ATTINY44" device="-SSU"/>
<part name="IC2" library="fab" deviceset="REGULATOR" device="SOT23"/>
<part name="U$1" library="fab" deviceset="RESONATOR" device="" value="20mhz"/>
<part name="C1" library="fab" deviceset="CAP-US" device="1206FAB" value="0.1uF"/>
<part name="U$4" library="fab" deviceset="AVRISP" device="SMD"/>
<part name="U$6" library="fab" deviceset="LED" device="FAB1206"/>
<part name="R5" library="fab" deviceset="RES-US" device="1206FAB" value="499"/>
<part name="C2" library="fab" deviceset="CAP-US" device="1206FAB"/>
<part name="JP2" library="pinhead" deviceset="PINHD-1X16" device=""/>
<part name="R2" library="fab" deviceset="RES-US" device="1206FAB" value="1K"/>
<part name="U$5" library="fab" deviceset="SPDTSWITCH" device=""/>
<part name="J1" library="fab2" deviceset="TERM-1X02" device="-ADAFRUIT"/>
</parts>
<sheets>
<sheet>
<plain>
</plain>
<busses>
</busses>
<nets>
<net name="N$1">
<segment>
<pinref part="IC1" gate="1" pin="(PCINT11/RESET/DW)PB3"/>
<pinref part="U$4" gate="G$1" pin="RST"/>
</segment>
</net>
<net name="VCC">
<segment>
<pinref part="U$4" gate="G$1" pin="VCC"/>
</segment>
<segment>
<pinref part="R5" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="IC1" gate="1" pin="VCC"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="OUT"/>
<pinref part="C1" gate="G$1" pin="2"/>
<pinref part="U$5" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="JP2" gate="A" pin="2"/>
</segment>
<segment>
<pinref part="U$5" gate="G$1" pin="1"/>
</segment>
</net>
<net name="MOSI">
<segment>
<pinref part="U$4" gate="G$1" pin="MOSI"/>
</segment>
<segment>
<pinref part="IC1" gate="1" pin="(PCINT6/OC1A/SDA/MOSI/ADC6)PA6"/>
</segment>
</net>
<net name="GND">
<segment>
<pinref part="U$4" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="IC1" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="U$6" gate="G$1" pin="C"/>
</segment>
<segment>
<pinref part="U$1" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="GND"/>
<pinref part="C2" gate="G$1" pin="2"/>
<pinref part="C1" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="JP2" gate="A" pin="5"/>
</segment>
<segment>
<pinref part="R2" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="JP2" gate="A" pin="1"/>
</segment>
<segment>
<pinref part="J1" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$2">
<segment>
<pinref part="R5" gate="G$1" pin="1"/>
<pinref part="U$6" gate="G$1" pin="A"/>
</segment>
</net>
<net name="PB0">
<segment>
<pinref part="IC1" gate="1" pin="(PCINT8/XTAL1/CLKI)PB0"/>
</segment>
<segment>
<pinref part="U$1" gate="G$1" pin="3"/>
</segment>
</net>
<net name="PB1">
<segment>
<pinref part="IC1" gate="1" pin="(PCINT9/XTAL2)PB1"/>
</segment>
<segment>
<pinref part="U$1" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$8">
<segment>
<pinref part="IC2" gate="G$1" pin="IN"/>
<pinref part="C2" gate="G$1" pin="1"/>
<pinref part="J1" gate="G$1" pin="2"/>
</segment>
</net>
<net name="PA5">
<segment>
<pinref part="IC1" gate="1" pin="(PCINT5/OC1B/MISO/DO/ADC5)PA5"/>
</segment>
<segment>
<pinref part="U$4" gate="G$1" pin="MISO"/>
</segment>
<segment>
<pinref part="JP2" gate="A" pin="4"/>
</segment>
</net>
<net name="PA4">
<segment>
<pinref part="IC1" gate="1" pin="(PCINT4/T1/SCL/USCK/ADC4)PA4"/>
</segment>
<segment>
<pinref part="U$4" gate="G$1" pin="SCK"/>
</segment>
<segment>
<pinref part="JP2" gate="A" pin="6"/>
</segment>
</net>
<net name="PA3">
<segment>
<pinref part="IC1" gate="1" pin="(PCINT3/T0/ADC3)PA3"/>
</segment>
<segment>
<pinref part="JP2" gate="A" pin="11"/>
</segment>
</net>
<net name="PA2">
<segment>
<pinref part="IC1" gate="1" pin="(PCINT2/AIN1/ADC2)PA2"/>
</segment>
<segment>
<pinref part="JP2" gate="A" pin="12"/>
</segment>
</net>
<net name="PA1">
<segment>
<pinref part="IC1" gate="1" pin="(PCINT1/AIN0/ADC1)PA1"/>
</segment>
<segment>
<pinref part="JP2" gate="A" pin="13"/>
</segment>
</net>
<net name="PA0">
<segment>
<pinref part="IC1" gate="1" pin="(PCINT0/AREF/ADC0)PA0"/>
</segment>
<segment>
<pinref part="JP2" gate="A" pin="14"/>
</segment>
</net>
<net name="N$4">
<segment>
<pinref part="JP2" gate="A" pin="3"/>
<pinref part="R2" gate="G$1" pin="1"/>
</segment>
</net>
</nets>
</sheet>
</sheets>
</schematic>
</drawing>
</eagle>
