<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<schematic>
<libraries>
<library name="fab">
<packages>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1206FAB">
</package>
<package name="C2220">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R1206W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="R1206FAB">
</package>
<package name="LED1206">
<description>LED 1206 pads (standard pattern)</description>
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="5MM">
<description>5mm round through hole part.</description>
</package>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
<package name="SOIC14">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="QFN/MLF20">
<description>&lt;b&gt;HP-VFQFP-N20&lt;/b&gt; Micro Lead Frame package (MLF)</description>
</package>
<package name="EFOBM">
</package>
</packages>
<symbols>
<symbol name="CAP-NONPOLARIZED">
<description>non-polarized capacitor</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="R-US">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="LED">
<description>LED</description>
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="REGULATOR_SOT223">
<pin name="IN"/>
<pin name="GND"/>
<pin name="OUT1"/>
<pin name="OUT2"/>
</symbol>
<symbol name="ATTINY24/44/84">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="(PCINT7/ICP/OC0B/ADC7)PA7"/>
<pin name="(PCINT6/OC1A/SDA/MOSI/ADC6)PA6"/>
<pin name="(PCINT5/OC1B/MISO/DO/ADC5)PA5"/>
<pin name="(PCINT4/T1/SCL/USCK/ADC4)PA4"/>
<pin name="(PCINT3/T0/ADC3)PA3"/>
<pin name="(PCINT2/AIN1/ADC2)PA2"/>
<pin name="(PCINT1/AIN0/ADC1)PA1"/>
<pin name="(PCINT0/AREF/ADC0)PA0"/>
<pin name="(PCINT11/RESET/DW)PB3"/>
<pin name="(PCINT10/INT0/OC0A/CKOUT)PB2"/>
<pin name="(PCINT9/XTAL2)PB1"/>
<pin name="(PCINT8/XTAL1/CLKI)PB0"/>
</symbol>
<symbol name="CERAMIC_RESONATOR">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="CAP-UNPOLARIZED" prefix="C" uservalue="yes">
<gates>
<gate name="&gt;NAME" symbol="CAP-NONPOLARIZED"/>
</gates>
<devices>
<device name="" package="C1206">
<connects>
<connect gate="&gt;NAME" pin="1" pad="1"/>
<connect gate="&gt;NAME" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FAB" package="C1206FAB">
<connects>
<connect gate="&gt;NAME" pin="1" pad="1"/>
<connect gate="&gt;NAME" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2220" package="C2220">
<connects>
<connect gate="&gt;NAME" pin="1" pad="1"/>
<connect gate="&gt;NAME" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RES-US" prefix="R" uservalue="yes">
<description>&lt;b&gt;Resistor (US Symbol)&lt;/b&gt;
&lt;p&gt;
Variants with postfix FAB are widened to allow the routing of internal traces</description>
<gates>
<gate name="G$1" symbol="R-US"/>
</gates>
<devices>
<device name="1206" package="R1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206W" package="R1206W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206FAB" package="R1206FAB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED">
<description>LED</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="LED1206">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FAB1206" package="LED1206FAB">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5MM" package="5MM">
<connects>
<connect gate="G$1" pin="A" pad="IN"/>
<connect gate="G$1" pin="C" pad="OUT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="REGULATOR_SOT223" prefix="U">
<gates>
<gate name="G$1" symbol="REGULATOR_SOT223"/>
</gates>
<devices>
<device name="" package="SOT223">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT1" pad="2"/>
<connect gate="G$1" pin="OUT2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY44" prefix="IC">
<gates>
<gate name="1" symbol="ATTINY24/44/84"/>
</gates>
<devices>
<device name="-SSU" package="SOIC14">
<connects>
<connect gate="1" pin="(PCINT0/AREF/ADC0)PA0" pad="13"/>
<connect gate="1" pin="(PCINT1/AIN0/ADC1)PA1" pad="12"/>
<connect gate="1" pin="(PCINT10/INT0/OC0A/CKOUT)PB2" pad="5"/>
<connect gate="1" pin="(PCINT11/RESET/DW)PB3" pad="4"/>
<connect gate="1" pin="(PCINT2/AIN1/ADC2)PA2" pad="11"/>
<connect gate="1" pin="(PCINT3/T0/ADC3)PA3" pad="10"/>
<connect gate="1" pin="(PCINT4/T1/SCL/USCK/ADC4)PA4" pad="9"/>
<connect gate="1" pin="(PCINT5/OC1B/MISO/DO/ADC5)PA5" pad="8"/>
<connect gate="1" pin="(PCINT6/OC1A/SDA/MOSI/ADC6)PA6" pad="7"/>
<connect gate="1" pin="(PCINT7/ICP/OC0B/ADC7)PA7" pad="6"/>
<connect gate="1" pin="(PCINT8/XTAL1/CLKI)PB0" pad="2"/>
<connect gate="1" pin="(PCINT9/XTAL2)PB1" pad="3"/>
<connect gate="1" pin="GND" pad="14"/>
<connect gate="1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-PU" package="DIL14">
<connects>
<connect gate="1" pin="(PCINT0/AREF/ADC0)PA0" pad="13"/>
<connect gate="1" pin="(PCINT1/AIN0/ADC1)PA1" pad="12"/>
<connect gate="1" pin="(PCINT10/INT0/OC0A/CKOUT)PB2" pad="5"/>
<connect gate="1" pin="(PCINT11/RESET/DW)PB3" pad="4"/>
<connect gate="1" pin="(PCINT2/AIN1/ADC2)PA2" pad="11"/>
<connect gate="1" pin="(PCINT3/T0/ADC3)PA3" pad="10"/>
<connect gate="1" pin="(PCINT4/T1/SCL/USCK/ADC4)PA4" pad="9"/>
<connect gate="1" pin="(PCINT5/OC1B/MISO/DO/ADC5)PA5" pad="8"/>
<connect gate="1" pin="(PCINT6/OC1A/SDA/MOSI/ADC6)PA6" pad="7"/>
<connect gate="1" pin="(PCINT7/ICP/OC0B/ADC7)PA7" pad="6"/>
<connect gate="1" pin="(PCINT8/XTAL1/CLKI)PB0" pad="2"/>
<connect gate="1" pin="(PCINT9/XTAL2)PB1" pad="3"/>
<connect gate="1" pin="GND" pad="14"/>
<connect gate="1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MU" package="QFN/MLF20">
<connects>
<connect gate="1" pin="(PCINT0/AREF/ADC0)PA0" pad="5"/>
<connect gate="1" pin="(PCINT1/AIN0/ADC1)PA1" pad="4"/>
<connect gate="1" pin="(PCINT10/INT0/OC0A/CKOUT)PB2" pad="14"/>
<connect gate="1" pin="(PCINT11/RESET/DW)PB3" pad="13"/>
<connect gate="1" pin="(PCINT2/AIN1/ADC2)PA2" pad="3"/>
<connect gate="1" pin="(PCINT3/T0/ADC3)PA3" pad="2"/>
<connect gate="1" pin="(PCINT4/T1/SCL/USCK/ADC4)PA4" pad="1"/>
<connect gate="1" pin="(PCINT5/OC1B/MISO/DO/ADC5)PA5" pad="20"/>
<connect gate="1" pin="(PCINT6/OC1A/SDA/MOSI/ADC6)PA6" pad="16"/>
<connect gate="1" pin="(PCINT7/ICP/OC0B/ADC7)PA7" pad="15"/>
<connect gate="1" pin="(PCINT8/XTAL1/CLKI)PB0" pad="11"/>
<connect gate="1" pin="(PCINT9/XTAL2)PB1" pad="12"/>
<connect gate="1" pin="GND" pad="8"/>
<connect gate="1" pin="VCC" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RESONATOR">
<gates>
<gate name="G$1" symbol="CERAMIC_RESONATOR"/>
</gates>
<devices>
<device name="" package="EFOBM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X02/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X06/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X01">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X03/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="PINHD2">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD6">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD1">
<pin name="1" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD3">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="PINHD-1X2" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PINHD2"/>
</gates>
<devices>
<device name="" package="1X02">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X02/90">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X6" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD6"/>
</gates>
<devices>
<device name="" package="1X06">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X06/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X1" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PINHD1"/>
</gates>
<devices>
<device name="" package="1X01">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X3" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD3"/>
</gates>
<devices>
<device name="" package="1X03">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X03/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="supply1">
<description>&lt;b&gt;Supply Symbols&lt;/b&gt;&lt;p&gt;
 GND, VCC, 0V, +5V, -5V, etc.&lt;p&gt;
 Please keep in mind, that these devices are necessary for the
 automatic wiring of the supply signals.&lt;p&gt;
 The pin name defined in the symbol is identical to the net which is to be wired automatically.&lt;p&gt;
 In this library the device names are the same as the pin names of the symbols, therefore the correct signal names appear next to the supply symbols in the schematic.&lt;p&gt;
 &lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
</packages>
<symbols>
<symbol name="+5V">
<pin name="+5V" direction="sup"/>
</symbol>
<symbol name="GND">
<pin name="GND" direction="sup"/>
</symbol>
<symbol name="+12V">
<pin name="+12V" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="+5V" prefix="P+">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="+5V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GND" prefix="GND">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="GND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="+12V" prefix="P+">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="+12V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="con-wago-500">
<description>&lt;b&gt;Wago Screw Clamps&lt;/b&gt;&lt;p&gt;
Grid 5.00 mm&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="W237-102">
<description>&lt;b&gt;WAGO SCREW CLAMP&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="KL">
<pin name="KL" direction="pas"/>
</symbol>
<symbol name="KL+V">
<pin name="KL" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="W237-102" prefix="X" uservalue="yes">
<description>&lt;b&gt;WAGO SCREW CLAMP&lt;/b&gt;</description>
<gates>
<gate name="-1" symbol="KL"/>
<gate name="-2" symbol="KL+V"/>
</gates>
<devices>
<device name="" package="W237-102">
<connects>
<connect gate="-1" pin="KL" pad="1"/>
<connect gate="-2" pin="KL" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="237-102"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="70K9898"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DO41-10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2.54 mm, horizontal, grid 10.16 mm</description>
</package>
</packages>
<symbols>
<symbol name="D">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="1N4004" prefix="D">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
general purpose rectifier, 1 A</description>
<gates>
<gate name="1" symbol="D"/>
</gates>
<devices>
<device name="" package="DO41-10">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="relay">
<description>&lt;b&gt;Relays&lt;/b&gt;&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;Eichhoff
&lt;li&gt;Finder
&lt;li&gt;Fujitsu
&lt;li&gt;HAMLIN
&lt;li&gt;OMRON
&lt;li&gt;Matsushita
&lt;li&gt;NAiS
&lt;li&gt;Siemens
&lt;li&gt;Schrack
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="ZF112">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x switch</description>
</package>
</packages>
<symbols>
<symbol name="K">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="U">
<pin name="O" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="P" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ZF112" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x switch</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="" package="ZF112">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="O" pad="O"/>
<connect gate="2" pin="P" pad="P"/>
<connect gate="2" pin="S" pad="S"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="transistor-npn">
<description>&lt;b&gt;NPN Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="NPN">
<pin name="B" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="2N3904" prefix="Q">
<description>&lt;b&gt;NPN Transistor&lt;/b&gt;</description>
<gates>
<gate name="G1" symbol="NPN"/>
</gates>
<devices>
<device name="" package="TO92">
<connects>
<connect gate="G1" pin="B" pad="2"/>
<connect gate="G1" pin="C" pad="1"/>
<connect gate="G1" pin="E" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<parts>
<part name="R2" library="fab" deviceset="RES-US" device="1206FAB"/>
<part name="U$2" library="fab" deviceset="LED" device="FAB1206"/>
<part name="C4" library="fab" deviceset="CAP-UNPOLARIZED" device="FAB"/>
<part name="U1" library="fab" deviceset="REGULATOR_SOT223" device=""/>
<part name="JP3" library="pinhead" deviceset="PINHD-1X2" device=""/>
<part name="P+4" library="supply1" deviceset="+5V" device=""/>
<part name="GND2" library="supply1" deviceset="GND" device=""/>
<part name="P+5" library="supply1" deviceset="+5V" device=""/>
<part name="GND4" library="supply1" deviceset="GND" device=""/>
<part name="GND5" library="supply1" deviceset="GND" device=""/>
<part name="C5" library="fab" deviceset="CAP-UNPOLARIZED" device="FAB"/>
<part name="P+6" library="supply1" deviceset="+5V" device=""/>
<part name="P+7" library="supply1" deviceset="+5V" device=""/>
<part name="GND6" library="supply1" deviceset="GND" device=""/>
<part name="IC1" library="fab" deviceset="ATTINY44" device="-SSU"/>
<part name="P+1" library="supply1" deviceset="+5V" device=""/>
<part name="GND1" library="supply1" deviceset="GND" device=""/>
<part name="JP2" library="pinhead" deviceset="PINHD-1X6" device=""/>
<part name="X1" library="con-wago-500" deviceset="W237-102" device=""/>
<part name="P+2" library="supply1" deviceset="+5V" device=""/>
<part name="P+3" library="supply1" deviceset="+5V" device=""/>
<part name="R1" library="fab" deviceset="RES-US" device="1206FAB"/>
<part name="R3" library="fab" deviceset="RES-US" device="1206FAB"/>
<part name="GND3" library="supply1" deviceset="GND" device=""/>
<part name="GND7" library="supply1" deviceset="GND" device=""/>
<part name="X2" library="con-wago-500" deviceset="W237-102" device=""/>
<part name="U$1" library="fab" deviceset="RESONATOR" device=""/>
<part name="GND8" library="supply1" deviceset="GND" device=""/>
<part name="P+8" library="supply1" deviceset="+5V" device=""/>
<part name="R4" library="fab" deviceset="RES-US" device="1206FAB"/>
<part name="GND9" library="supply1" deviceset="GND" device=""/>
<part name="X3" library="con-wago-500" deviceset="W237-102" device=""/>
<part name="D1" library="diode" deviceset="1N4004" device=""/>
<part name="K1" library="relay" deviceset="ZF112" device=""/>
<part name="Q1" library="transistor-npn" deviceset="2N3904" device=""/>
<part name="R5" library="fab" deviceset="RES-US" device="1206FAB"/>
<part name="GND10" library="supply1" deviceset="GND" device=""/>
<part name="P+9" library="supply1" deviceset="+12V" device=""/>
<part name="P+10" library="supply1" deviceset="+12V" device=""/>
<part name="P+11" library="supply1" deviceset="+12V" device=""/>
<part name="X4" library="con-wago-500" deviceset="W237-102" device=""/>
<part name="GND11" library="supply1" deviceset="GND" device=""/>
<part name="R6" library="fab" deviceset="RES-US" device="1206FAB"/>
<part name="P+12" library="supply1" deviceset="+5V" device=""/>
<part name="JP6" library="pinhead" deviceset="PINHD-1X1" device=""/>
<part name="JP4" library="pinhead" deviceset="PINHD-1X3" device=""/>
</parts>
<sheets>
<sheet>
<plain>
</plain>
<busses>
</busses>
<nets>
<net name="+5V">
<segment>
<pinref part="C4" gate="&gt;NAME" pin="2"/>
<pinref part="P+4" gate="1" pin="+5V"/>
</segment>
<segment>
<pinref part="R2" gate="G$1" pin="2"/>
<pinref part="P+5" gate="1" pin="+5V"/>
</segment>
<segment>
<pinref part="U1" gate="G$1" pin="OUT1"/>
<pinref part="P+6" gate="1" pin="+5V"/>
</segment>
<segment>
<pinref part="P+7" gate="1" pin="+5V"/>
<pinref part="JP2" gate="A" pin="3"/>
<pinref part="JP2" gate="A" pin="2"/>
<pinref part="JP2" gate="A" pin="1"/>
</segment>
<segment>
<pinref part="IC1" gate="1" pin="VCC"/>
<pinref part="P+1" gate="1" pin="+5V"/>
</segment>
<segment>
<pinref part="X1" gate="-1" pin="KL"/>
<pinref part="P+2" gate="1" pin="+5V"/>
</segment>
<segment>
<pinref part="X2" gate="-1" pin="KL"/>
<pinref part="P+3" gate="1" pin="+5V"/>
</segment>
<segment>
<pinref part="X3" gate="-1" pin="KL"/>
<pinref part="P+8" gate="1" pin="+5V"/>
</segment>
<segment>
<pinref part="R6" gate="G$1" pin="2"/>
<pinref part="P+12" gate="1" pin="+5V"/>
</segment>
</net>
<net name="GND">
<segment>
<pinref part="C4" gate="&gt;NAME" pin="1"/>
<pinref part="GND2" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="U$2" gate="G$1" pin="C"/>
<pinref part="GND4" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="C5" gate="&gt;NAME" pin="1"/>
<pinref part="U1" gate="G$1" pin="GND"/>
<pinref part="GND5" gate="1" pin="GND"/>
<pinref part="JP3" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="GND6" gate="1" pin="GND"/>
<pinref part="JP2" gate="A" pin="4"/>
<pinref part="JP2" gate="A" pin="5"/>
<pinref part="JP2" gate="A" pin="6"/>
</segment>
<segment>
<pinref part="IC1" gate="1" pin="GND"/>
<pinref part="GND1" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="R1" gate="G$1" pin="1"/>
<pinref part="GND3" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="R3" gate="G$1" pin="1"/>
<pinref part="GND7" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="U$1" gate="G$1" pin="2"/>
<pinref part="GND8" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="R4" gate="G$1" pin="1"/>
<pinref part="GND9" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="Q1" gate="G1" pin="E"/>
<pinref part="GND10" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="X4" gate="-2" pin="KL"/>
<pinref part="GND11" gate="1" pin="GND"/>
</segment>
</net>
<net name="N$5">
<segment>
<pinref part="U$2" gate="G$1" pin="A"/>
<pinref part="R2" gate="G$1" pin="1"/>
</segment>
</net>
<net name="MOSI">
<segment>
<pinref part="IC1" gate="1" pin="(PCINT6/OC1A/SDA/MOSI/ADC6)PA6"/>
<pinref part="JP4" gate="A" pin="1"/>
</segment>
</net>
<net name="MISO">
<segment>
<pinref part="IC1" gate="1" pin="(PCINT5/OC1B/MISO/DO/ADC5)PA5"/>
<pinref part="JP4" gate="A" pin="2"/>
</segment>
</net>
<net name="SCK">
<segment>
<pinref part="IC1" gate="1" pin="(PCINT4/T1/SCL/USCK/ADC4)PA4"/>
<pinref part="JP4" gate="A" pin="3"/>
</segment>
</net>
<net name="RST">
<segment>
<pinref part="IC1" gate="1" pin="(PCINT11/RESET/DW)PB3"/>
<pinref part="R6" gate="G$1" pin="1"/>
<pinref part="JP6" gate="G$1" pin="1"/>
</segment>
</net>
<net name="STATE1">
<segment>
<pinref part="X1" gate="-2" pin="KL"/>
<pinref part="R1" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="IC1" gate="1" pin="(PCINT1/AIN0/ADC1)PA1"/>
</segment>
</net>
<net name="STATE2">
<segment>
<pinref part="R3" gate="G$1" pin="2"/>
<pinref part="X2" gate="-2" pin="KL"/>
</segment>
<segment>
<pinref part="IC1" gate="1" pin="(PCINT0/AREF/ADC0)PA0"/>
</segment>
</net>
<net name="N$1">
<segment>
<pinref part="IC1" gate="1" pin="(PCINT9/XTAL2)PB1"/>
<pinref part="U$1" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$2">
<segment>
<pinref part="IC1" gate="1" pin="(PCINT8/XTAL1/CLKI)PB0"/>
<pinref part="U$1" gate="G$1" pin="3"/>
</segment>
</net>
<net name="PUL">
<segment>
<pinref part="R4" gate="G$1" pin="2"/>
<pinref part="X3" gate="-2" pin="KL"/>
</segment>
<segment>
<pinref part="IC1" gate="1" pin="(PCINT2/AIN1/ADC2)PA2"/>
</segment>
</net>
<net name="RELE">
<segment>
<pinref part="R5" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="IC1" gate="1" pin="(PCINT3/T0/ADC3)PA3"/>
</segment>
</net>
<net name="N$3">
<segment>
<pinref part="Q1" gate="G1" pin="B"/>
<pinref part="R5" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$4">
<segment>
<pinref part="Q1" gate="G1" pin="C"/>
<pinref part="K1" gate="1" pin="2"/>
<pinref part="D1" gate="1" pin="A"/>
</segment>
</net>
<net name="+12V">
<segment>
<pinref part="JP3" gate="G$1" pin="2"/>
<pinref part="U1" gate="G$1" pin="IN"/>
<pinref part="C5" gate="&gt;NAME" pin="2"/>
<pinref part="P+9" gate="1" pin="+12V"/>
</segment>
<segment>
<pinref part="D1" gate="1" pin="C"/>
<pinref part="K1" gate="1" pin="1"/>
<pinref part="P+10" gate="1" pin="+12V"/>
</segment>
<segment>
<pinref part="K1" gate="2" pin="S"/>
<pinref part="P+11" gate="1" pin="+12V"/>
</segment>
</net>
<net name="N$6">
<segment>
<pinref part="X4" gate="-1" pin="KL"/>
<pinref part="K1" gate="2" pin="P"/>
</segment>
</net>
</nets>
</sheet>
</sheets>
</schematic>
</drawing>
</eagle>
