<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.2">
<drawing>
<schematic>
<libraries>
<library name="fab">
<packages>
<package name="TQFP32-08THIN">
</package>
<package name="2-SMD-5X3MM">
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1206FAB">
</package>
<package name="C2220">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R1206W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="R1206FAB">
</package>
<package name="LED1206">
<description>LED 1206 pads (standard pattern)</description>
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="5MM">
<description>5mm round through hole part.</description>
</package>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="23-I/O">
<pin name="PB5(SCK)"/>
<pin name="PB7(XTAL2/TOSC2)"/>
<pin name="PB6(XTAL1/TOSC1)"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="AVCC" direction="pwr"/>
<pin name="PB4(MISO)"/>
<pin name="PB3(MOSI/OC2)"/>
<pin name="PB2(SS/OC1B)"/>
<pin name="PB1(OC1A)"/>
<pin name="PB0(ICP)"/>
<pin name="PD7(AIN1)"/>
<pin name="PD6(AIN0)"/>
<pin name="PD5(T1)"/>
<pin name="PD4(XCK/T0)"/>
<pin name="PD3(INT1)"/>
<pin name="PD2(INT0)"/>
<pin name="PD1(TXD)"/>
<pin name="PD0(RXD)"/>
<pin name="ADC7"/>
<pin name="ADC6"/>
<pin name="PC5(ADC5/SCL)"/>
<pin name="PC4(ADC4/SDA)"/>
<pin name="PC3(ADC3)"/>
<pin name="PC2(ADC2)"/>
<pin name="PC1(ADC1)"/>
<pin name="PC0(ADC0)"/>
<pin name="PC6(/RESET)" function="dot"/>
</symbol>
<symbol name="CRYSTAL">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="CAP-NONPOLARIZED">
<description>non-polarized capacitor</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="R-US">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="LED">
<description>LED</description>
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="REGULATOR_SOT223">
<pin name="IN"/>
<pin name="GND"/>
<pin name="OUT1"/>
<pin name="OUT2"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ATMEGA88-THIN" prefix="IC">
<gates>
<gate name="G$1" symbol="23-I/O"/>
</gates>
<devices>
<device name="" package="TQFP32-08THIN">
<connects>
<connect gate="G$1" pin="ADC6" pad="19"/>
<connect gate="G$1" pin="ADC7" pad="22"/>
<connect gate="G$1" pin="AREF" pad="20"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND" pad="21"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="PB0(ICP)" pad="12"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="13"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="14"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="15"/>
<connect gate="G$1" pin="PB4(MISO)" pad="16"/>
<connect gate="G$1" pin="PB5(SCK)" pad="17"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="7"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="8"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="29"/>
<connect gate="G$1" pin="PD0(RXD)" pad="30"/>
<connect gate="G$1" pin="PD1(TXD)" pad="31"/>
<connect gate="G$1" pin="PD2(INT0)" pad="32"/>
<connect gate="G$1" pin="PD3(INT1)" pad="1"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="2"/>
<connect gate="G$1" pin="PD5(T1)" pad="9"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="10"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="11"/>
<connect gate="G$1" pin="VCC@1" pad="4"/>
<connect gate="G$1" pin="VCC@2" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CRYSTAL">
<gates>
<gate name="G$1" symbol="CRYSTAL"/>
</gates>
<devices>
<device name="" package="2-SMD-5X3MM">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAP-UNPOLARIZED" prefix="C" uservalue="yes">
<gates>
<gate name="&gt;NAME" symbol="CAP-NONPOLARIZED"/>
</gates>
<devices>
<device name="" package="C1206">
<connects>
<connect gate="&gt;NAME" pin="1" pad="1"/>
<connect gate="&gt;NAME" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FAB" package="C1206FAB">
<connects>
<connect gate="&gt;NAME" pin="1" pad="1"/>
<connect gate="&gt;NAME" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2220" package="C2220">
<connects>
<connect gate="&gt;NAME" pin="1" pad="1"/>
<connect gate="&gt;NAME" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RES-US" prefix="R" uservalue="yes">
<description>&lt;b&gt;Resistor (US Symbol)&lt;/b&gt;
&lt;p&gt;
Variants with postfix FAB are widened to allow the routing of internal traces</description>
<gates>
<gate name="G$1" symbol="R-US"/>
</gates>
<devices>
<device name="1206" package="R1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206W" package="R1206W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206FAB" package="R1206FAB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED">
<description>LED</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="LED1206">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FAB1206" package="LED1206FAB">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5MM" package="5MM">
<connects>
<connect gate="G$1" pin="A" pad="IN"/>
<connect gate="G$1" pin="C" pad="OUT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="REGULATOR_SOT223" prefix="U">
<gates>
<gate name="G$1" symbol="REGULATOR_SOT223"/>
</gates>
<devices>
<device name="" package="SOT223">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT1" pad="2"/>
<connect gate="G$1" pin="OUT2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X02/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X03/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X06/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X04/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="PINHD2">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD3">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD6">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD4">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="PINHD-1X2" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PINHD2"/>
</gates>
<devices>
<device name="" package="1X02">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X02/90">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X3" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD3"/>
</gates>
<devices>
<device name="" package="1X03">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X03/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X6" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD6"/>
</gates>
<devices>
<device name="" package="1X06">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X06/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X4" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD4"/>
</gates>
<devices>
<device name="" package="1X04">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X04/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="supply1">
<description>&lt;b&gt;Supply Symbols&lt;/b&gt;&lt;p&gt;
 GND, VCC, 0V, +5V, -5V, etc.&lt;p&gt;
 Please keep in mind, that these devices are necessary for the
 automatic wiring of the supply signals.&lt;p&gt;
 The pin name defined in the symbol is identical to the net which is to be wired automatically.&lt;p&gt;
 In this library the device names are the same as the pin names of the symbols, therefore the correct signal names appear next to the supply symbols in the schematic.&lt;p&gt;
 &lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
</packages>
<symbols>
<symbol name="+5V">
<pin name="+5V" direction="sup"/>
</symbol>
<symbol name="GND">
<pin name="GND" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="+5V" prefix="P+">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="+5V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GND" prefix="GND">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="GND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X01">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="PINHD1">
<pin name="1" direction="pas" function="dot"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="PINHD-1X1" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PINHD1"/>
</gates>
<devices>
<device name="" package="1X01">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<parts>
<part name="IC1" library="fab" deviceset="ATMEGA88-THIN" device=""/>
<part name="U$1" library="fab" deviceset="CRYSTAL" device=""/>
<part name="C1" library="fab" deviceset="CAP-UNPOLARIZED" device="FAB"/>
<part name="C2" library="fab" deviceset="CAP-UNPOLARIZED" device="FAB"/>
<part name="C3" library="fab" deviceset="CAP-UNPOLARIZED" device="FAB"/>
<part name="R1" library="fab" deviceset="RES-US" device="1206FAB"/>
<part name="R2" library="fab" deviceset="RES-US" device="1206FAB"/>
<part name="U$2" library="fab" deviceset="LED" device="FAB1206"/>
<part name="C4" library="fab" deviceset="CAP-UNPOLARIZED" device="FAB"/>
<part name="GND1" library="supply1" deviceset="GND" device=""/>
<part name="U1" library="fab" deviceset="REGULATOR_SOT223" device=""/>
<part name="JP3" library="pinhead" deviceset="PINHD-1X2" device=""/>
<part name="P+3" library="supply1" deviceset="+5V" device=""/>
<part name="P+4" library="supply1" deviceset="+5V" device=""/>
<part name="GND2" library="supply1" deviceset="GND" device=""/>
<part name="GND3" library="supply1" deviceset="GND" device=""/>
<part name="P+5" library="supply1" deviceset="+5V" device=""/>
<part name="GND4" library="supply1" deviceset="GND" device=""/>
<part name="GND5" library="supply1" deviceset="GND" device=""/>
<part name="C5" library="fab" deviceset="CAP-UNPOLARIZED" device="FAB"/>
<part name="P+6" library="supply1" deviceset="+5V" device=""/>
<part name="P+7" library="supply1" deviceset="+5V" device=""/>
<part name="GND6" library="supply1" deviceset="GND" device=""/>
<part name="JP4" library="pinhead" deviceset="PINHD-1X3" device=""/>
<part name="JP1" library="pinhead" deviceset="PINHD-1X6" device=""/>
<part name="JP5" library="pinhead" deviceset="PINHD-1X4" device=""/>
<part name="JP2" library="pinhead" deviceset="PINHD-1X1" device=""/>
</parts>
<sheets>
<sheet>
<plain>
</plain>
<busses>
</busses>
<nets>
<net name="+5V">
<segment>
<pinref part="R1" gate="G$1" pin="1"/>
<pinref part="P+3" gate="1" pin="+5V"/>
<pinref part="C3" gate="&gt;NAME" pin="2"/>
<pinref part="IC1" gate="G$1" pin="AVCC"/>
<pinref part="IC1" gate="G$1" pin="VCC@1"/>
<pinref part="IC1" gate="G$1" pin="VCC@2"/>
</segment>
<segment>
<pinref part="C4" gate="&gt;NAME" pin="2"/>
<pinref part="P+4" gate="1" pin="+5V"/>
</segment>
<segment>
<pinref part="R2" gate="G$1" pin="2"/>
<pinref part="P+5" gate="1" pin="+5V"/>
</segment>
<segment>
<pinref part="U1" gate="G$1" pin="OUT1"/>
<pinref part="P+6" gate="1" pin="+5V"/>
</segment>
<segment>
<pinref part="P+7" gate="1" pin="+5V"/>
<pinref part="JP1" gate="A" pin="2"/>
<pinref part="JP1" gate="A" pin="3"/>
<pinref part="JP1" gate="A" pin="1"/>
</segment>
</net>
<net name="N$2">
<segment>
<pinref part="IC1" gate="G$1" pin="AREF"/>
<pinref part="C3" gate="&gt;NAME" pin="1"/>
</segment>
</net>
<net name="N$3">
<segment>
<pinref part="U$1" gate="G$1" pin="2"/>
<pinref part="IC1" gate="G$1" pin="PB6(XTAL1/TOSC1)"/>
<pinref part="C1" gate="&gt;NAME" pin="1"/>
</segment>
</net>
<net name="N$4">
<segment>
<pinref part="U$1" gate="G$1" pin="1"/>
<pinref part="IC1" gate="G$1" pin="PB7(XTAL2/TOSC2)"/>
<pinref part="C2" gate="&gt;NAME" pin="1"/>
</segment>
</net>
<net name="GND">
<segment>
<pinref part="C2" gate="&gt;NAME" pin="2"/>
<pinref part="C1" gate="&gt;NAME" pin="2"/>
<pinref part="GND1" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="C4" gate="&gt;NAME" pin="1"/>
<pinref part="GND2" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="GND"/>
<pinref part="GND3" gate="1" pin="GND"/>
<pinref part="IC1" gate="G$1" pin="GND@1"/>
<pinref part="IC1" gate="G$1" pin="GND@2"/>
</segment>
<segment>
<pinref part="U$2" gate="G$1" pin="C"/>
<pinref part="GND4" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="C5" gate="&gt;NAME" pin="1"/>
<pinref part="U1" gate="G$1" pin="GND"/>
<pinref part="GND5" gate="1" pin="GND"/>
<pinref part="JP3" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="GND6" gate="1" pin="GND"/>
<pinref part="JP1" gate="A" pin="4"/>
<pinref part="JP1" gate="A" pin="5"/>
<pinref part="JP1" gate="A" pin="6"/>
</segment>
</net>
<net name="N$5">
<segment>
<pinref part="U$2" gate="G$1" pin="A"/>
<pinref part="R2" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$6">
<segment>
<pinref part="JP3" gate="G$1" pin="2"/>
<pinref part="U1" gate="G$1" pin="IN"/>
<pinref part="C5" gate="&gt;NAME" pin="2"/>
</segment>
</net>
<net name="N$7">
<segment>
<pinref part="IC1" gate="G$1" pin="PB3(MOSI/OC2)"/>
<pinref part="JP4" gate="A" pin="1"/>
</segment>
</net>
<net name="N$8">
<segment>
<pinref part="IC1" gate="G$1" pin="PB4(MISO)"/>
<pinref part="JP4" gate="A" pin="2"/>
</segment>
</net>
<net name="N$9">
<segment>
<pinref part="IC1" gate="G$1" pin="PB5(SCK)"/>
<pinref part="JP4" gate="A" pin="3"/>
</segment>
</net>
<net name="TEMP">
<segment>
<pinref part="IC1" gate="G$1" pin="PD2(INT0)"/>
<pinref part="JP2" gate="G$1" pin="1"/>
</segment>
</net>
<net name="SDA">
<segment>
<pinref part="IC1" gate="G$1" pin="PC4(ADC4/SDA)"/>
<pinref part="JP5" gate="A" pin="2"/>
</segment>
</net>
<net name="SCL">
<segment>
<pinref part="IC1" gate="G$1" pin="PC5(ADC5/SCL)"/>
<pinref part="JP5" gate="A" pin="3"/>
</segment>
</net>
<net name="POT">
<segment>
<pinref part="IC1" gate="G$1" pin="PC3(ADC3)"/>
<pinref part="JP5" gate="A" pin="1"/>
</segment>
</net>
<net name="RST">
<segment>
<pinref part="JP5" gate="A" pin="4"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PC6(/RESET)"/>
<pinref part="R1" gate="G$1" pin="2"/>
</segment>
</net>
</nets>
</sheet>
</sheets>
</schematic>
</drawing>
</eagle>
