<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="46.99" x2="35.23" y2="46.99" width="0" layer="20"/>
<wire x1="35.23" y1="46.99" x2="35.23" y2="85.08" width="0" layer="20"/>
<wire x1="35.23" y1="85.08" x2="0" y2="85.08" width="0" layer="20"/>
<wire x1="0" y1="85.08" x2="0" y2="46.99" width="0" layer="20"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
<package name="C1206FAB">
</package>
<package name="R1206FAB">
</package>
</packages>
</library>
<library name="pinhead+">
<packages>
<package name="1X04_SMT">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="fab" package="SOIC8" value="A4953-H-BRIDGE-MOTOR-DRIVER">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="fab" package="SOIC8" value="A4953-H-BRIDGE-MOTOR-DRIVER">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="fab" package="C1206FAB" value="1uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="pinhead+" package="1X04_SMT" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="pinhead+" package="1X04_SMT" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="pinhead+" package="1X04_SMT" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="fab" package="C1206FAB" value="10uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="fab" package="C1206FAB" value="10uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="fab" package="C1206FAB" value="1uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="pinhead+" package="1X04_SMT" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="fab" package="R1206FAB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="JP1" pad="2"/>
<contactref element="U$1" pad="5"/>
<contactref element="U$2" pad="5"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="GND">
<contactref element="JP1" pad="4"/>
<contactref element="U$1" pad="1"/>
<contactref element="U$2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="U$1" pad="7"/>
<contactref element="U$2" pad="7"/>
<contactref element="JP4" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="JP2" pad="1"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="N$5">
<contactref element="JP2" pad="2"/>
<contactref element="U$1" pad="8"/>
</signal>
<signal name="N$6">
<contactref element="JP2" pad="3"/>
<contactref element="U$2" pad="6"/>
</signal>
<signal name="N$7">
<contactref element="U$2" pad="8"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="IN1">
<contactref element="JP3" pad="1"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="IN2">
<contactref element="JP3" pad="2"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="IN3">
<contactref element="JP3" pad="3"/>
<contactref element="U$2" pad="3"/>
<contactref element="R1" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="IN4">
<contactref element="JP3" pad="4"/>
<contactref element="U$2" pad="2"/>
</signal>
<signal name="V">
<contactref element="U$1" pad="4"/>
<contactref element="U$2" pad="4"/>
<contactref element="JP4" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
