<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<schematic>
<libraries>
<library name="esp12e">
<packages>
<package name="ESP8266-ESP12E">
<description>
&lt;b&gt;ESP8266-12E Library for Eagle CAD&lt;/b&gt;&lt;p&gt;
The author not responsible for any damages or errors!.&lt;p&gt;
&lt;author&gt;Created by Suhail jr.lt;/author&gt;
</description>
</package>
</packages>
<symbols>
<symbol name="ESP12E">
<description>
&lt;b&gt;ESP8266-12E Library for Eagle CAD&lt;/b&gt;&lt;p&gt;
The author not responsible for any damages or errors!.&lt;p&gt;
&lt;author&gt;Created by Suhail jr.lt;/author&gt;
</description>
<pin name="GND"/>
<pin name="GPIO15"/>
<pin name="GPIO2"/>
<pin name="GPIO0"/>
<pin name="GPIO4"/>
<pin name="GPIO5"/>
<pin name="RXD"/>
<pin name="TXD"/>
<pin name="REST"/>
<pin name="ADC"/>
<pin name="CH_PD"/>
<pin name="GPIO16"/>
<pin name="GPIO14"/>
<pin name="GPIO12"/>
<pin name="GPIO13"/>
<pin name="VCC"/>
<pin name="CS0"/>
<pin name="MISO"/>
<pin name="GPIO9"/>
<pin name="GPIO10"/>
<pin name="MOSI"/>
<pin name="SCLK"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ESP8266-12E" prefix="SJR" uservalue="yes">
<description>
&lt;b&gt;ESP8266-12E Library for Eagle CAD&lt;/b&gt;&lt;p&gt;
The author not responsible for any damages or errors!.&lt;p&gt;
&lt;author&gt;Created by Suhail jr.lt;/author&gt;
</description>
<gates>
<gate name="G$1" symbol="ESP12E"/>
</gates>
<devices>
<device name="ESP12E" package="ESP8266-ESP12E">
<connects>
<connect gate="G$1" pin="ADC" pad="2"/>
<connect gate="G$1" pin="CH_PD" pad="3"/>
<connect gate="G$1" pin="CS0" pad="17"/>
<connect gate="G$1" pin="GND" pad="9"/>
<connect gate="G$1" pin="GPIO0" pad="12"/>
<connect gate="G$1" pin="GPIO10" pad="20"/>
<connect gate="G$1" pin="GPIO12" pad="6"/>
<connect gate="G$1" pin="GPIO13" pad="7"/>
<connect gate="G$1" pin="GPIO14" pad="5"/>
<connect gate="G$1" pin="GPIO15" pad="10"/>
<connect gate="G$1" pin="GPIO16" pad="4"/>
<connect gate="G$1" pin="GPIO2" pad="11"/>
<connect gate="G$1" pin="GPIO4" pad="13"/>
<connect gate="G$1" pin="GPIO5" pad="14"/>
<connect gate="G$1" pin="GPIO9" pad="19"/>
<connect gate="G$1" pin="MISO" pad="18"/>
<connect gate="G$1" pin="MOSI" pad="21"/>
<connect gate="G$1" pin="REST" pad="1"/>
<connect gate="G$1" pin="RXD" pad="15"/>
<connect gate="G$1" pin="SCLK" pad="22"/>
<connect gate="G$1" pin="TXD" pad="16"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="fab">
<packages>
<package name="1X06SMD">
</package>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT 23&lt;/b&gt;</description>
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1206K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1206 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 3216</description>
</package>
<package name="C1206FAB">
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R1206W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="R1206FAB">
</package>
<package name="SOT-23">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="TO252">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
TS-003</description>
</package>
<package name="JACK_2.1MM">
</package>
<package name="JACK_.65MM">
</package>
<package name="LED1206">
<description>LED 1206 pads (standard pattern)</description>
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="5MM">
<description>5mm round through hole part.</description>
</package>
</packages>
<symbols>
<symbol name="FTDI">
<pin name="GND"/>
<pin name="CTS"/>
<pin name="VCC"/>
<pin name="TXD"/>
<pin name="RXD"/>
<pin name="RTS"/>
</symbol>
<symbol name="TS2">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="P1" direction="pas"/>
</symbol>
<symbol name="REGULATOR">
<pin name="IN"/>
<pin name="GND"/>
<pin name="OUT"/>
</symbol>
<symbol name="C-US">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="R-US">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="N_MOSFET">
<pin name="D" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="G" direction="pas"/>
</symbol>
<symbol name="JACK">
<pin name="PIN"/>
<pin name="CONTACT"/>
<pin name="SHUNT"/>
</symbol>
<symbol name="LED">
<description>LED</description>
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="FTDI-SMD-HEADER">
<gates>
<gate name="G$1" symbol="FTDI"/>
</gates>
<devices>
<device name="" package="1X06SMD">
<connects>
<connect gate="G$1" pin="CTS" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="RTS" pad="6"/>
<connect gate="G$1" pin="RXD" pad="5"/>
<connect gate="G$1" pin="TXD" pad="4"/>
<connect gate="G$1" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6MM_SWITCH" prefix="S" uservalue="yes">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
<gates>
<gate name="2" symbol="TS2"/>
</gates>
<devices>
<device name="6MM_SWITCH" package="6MM_SWITCH">
<connects>
<connect gate="2" pin="P" pad="1"/>
<connect gate="2" pin="P1" pad="2"/>
<connect gate="2" pin="S" pad="3"/>
<connect gate="2" pin="S1" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="REGULATOR" prefix="IC" uservalue="yes">
<gates>
<gate name="G$1" symbol="REGULATOR"/>
</gates>
<devices>
<device name="SOT23" package="SOT23">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAP-US" prefix="C">
<gates>
<gate name="G$1" symbol="C-US"/>
</gates>
<devices>
<device name="1206" package="C1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206K" package="C1206K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206FAB" package="C1206FAB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RES-US" prefix="R" uservalue="yes">
<description>&lt;b&gt;Resistor (US Symbol)&lt;/b&gt;
&lt;p&gt;
Variants with postfix FAB are widened to allow the routing of internal traces</description>
<gates>
<gate name="G$1" symbol="R-US"/>
</gates>
<devices>
<device name="1206" package="R1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206W" package="R1206W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206FAB" package="R1206FAB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NMOSFET" prefix="T" uservalue="yes">
<description>&lt;b&gt;MOS FET&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="N_MOSFET"/>
</gates>
<devices>
<device name="SOT23" package="SOT-23">
<connects>
<connect gate="A" pin="D" pad="1"/>
<connect gate="A" pin="G" pad="3"/>
<connect gate="A" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO252" package="TO252">
<connects>
<connect gate="A" pin="D" pad="3"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JACK" prefix="J">
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="2.1MM" package="JACK_2.1MM">
<connects>
<connect gate="G$1" pin="CONTACT" pad="CONTACT"/>
<connect gate="G$1" pin="PIN" pad="PIN"/>
<connect gate="G$1" pin="SHUNT" pad="SHUNT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name=".65MM" package="JACK_.65MM">
<connects>
<connect gate="G$1" pin="CONTACT" pad="SHUNT"/>
<connect gate="G$1" pin="PIN" pad="PIN"/>
<connect gate="G$1" pin="SHUNT" pad="CONTACT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED">
<description>LED</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="LED1206">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FAB1206" package="LED1206FAB">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5MM" package="5MM">
<connects>
<connect gate="G$1" pin="A" pad="IN"/>
<connect gate="G$1" pin="C" pad="OUT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="Seeed-OPL-Relay">
<packages>
<package name="REY5-19.0X15.0X15.0MM">
</package>
</packages>
<symbols>
<symbol name="RELAY-HLS8L-DC5V-S-C">
<pin name="V+"/>
<pin name="V-"/>
<pin name="NO"/>
<pin name="NC"/>
<pin name="COM"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="RELAY-HLS8L-DC5V-S-C(5P-19X15MM)" prefix="K" uservalue="yes">
<description>315030000</description>
<gates>
<gate name="G$1" symbol="RELAY-HLS8L-DC5V-S-C"/>
</gates>
<devices>
<device name="" package="REY5-19.0X15.0X15.0MM">
<connects>
<connect gate="G$1" pin="COM" pad="1"/>
<connect gate="G$1" pin="NC" pad="5"/>
<connect gate="G$1" pin="NO" pad="4"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="HLS8L-DC5V-S-C"/>
<attribute name="VALUE" value="HLS8L-DC5V-S-C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="FAB_Hello">
<packages>
</packages>
<symbols>
<symbol name="GND-1">
<pin name="GND" direction="sup"/>
</symbol>
<symbol name="VCC">
<pin name="VCC" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="GND" prefix="GND">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="GND-1"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VCC" prefix="P+">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="VCC" symbol="VCC"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
</package>
<package name="MOLEX-1X2">
</package>
<package name="SCREWTERMINAL-3.5MM-2">
</package>
<package name="JST-2-SMD">
<description>2mm SMD side-entry connector. tDocu layer indicates the actual physical plastic housing. +/- indicate SparkFun standard batteries and wiring.</description>
</package>
<package name="1X02_BIG">
</package>
<package name="JST-2-SMD-VERT">
</package>
<package name="R_SW_TH">
</package>
<package name="SCREWTERMINAL-5MM-2">
</package>
<package name="1X02_LOCK">
</package>
<package name="MOLEX-1X2_LOCK">
</package>
<package name="1X02_LOCK_LONGPADS">
<description>This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place.  
You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  
This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" 
to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers.
Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,
if you push a header all the way into place, it is covered up entirely on the bottom side.  This idea of altering the position of holes to aid alignment 
will be further integrated into the Sparkfun Library for other footprints.  It can help hold any component with 3 or more connection pins.</description>
</package>
<package name="SCREWTERMINAL-3.5MM-2_LOCK">
</package>
<package name="1X02_LONGPADS">
</package>
<package name="1X02_NO_SILK">
</package>
<package name="JST-2-PTH">
</package>
<package name="1X02_XTRA_BIG">
</package>
<package name="1X02_PP_HOLES_ONLY">
</package>
<package name="SCREWTERMINAL-3.5MM-2-NS">
</package>
<package name="JST-2-PTH-NS">
</package>
<package name="JST-2-PTH-KIT">
<description>&lt;H3&gt;JST-2-PTH-KIT&lt;/h3&gt;
2-Pin JST, through-hole connector&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.</description>
</package>
<package name="SPRINGTERMINAL-2.54MM-2">
</package>
<package name="1X02_2.54_SCREWTERM">
</package>
<package name="JST-2-PTH-VERT">
</package>
</packages>
<symbols>
<symbol name="M02">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="M02" prefix="J" uservalue="yes">
<description>Standard 2-pin 0.1" header. Use with &lt;br&gt;
- straight break away headers ( PRT-00116)&lt;br&gt;
- right angle break away headers (PRT-00553)&lt;br&gt;
- swiss pins (PRT-00743)&lt;br&gt;
- machine pins (PRT-00117)&lt;br&gt;
- female headers (PRT-00115)&lt;br&gt;&lt;br&gt;

 Molex polarized connector foot print use with: PRT-08233 with associated crimp pins and housings.&lt;br&gt;&lt;br&gt;

2.54_SCREWTERM for use with  PRT-10571.&lt;br&gt;&lt;br&gt;

3.5mm Screw Terminal footprints for  PRT-08084&lt;br&gt;&lt;br&gt;

5mm Screw Terminal footprints for use with PRT-08432</description>
<gates>
<gate name="G$1" symbol="M02"/>
</gates>
<devices>
<device name="PTH" package="1X02">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR" package="MOLEX-1X2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.5MM" package="SCREWTERMINAL-3.5MM-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08399"/>
</technology>
</technologies>
</device>
<device name="-JST-2MM-SMT" package="JST-2-SMD">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-11443"/>
</technology>
</technologies>
</device>
<device name="PTH2" package="1X02_BIG">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="4UCON-15767" package="JST-2-SMD-VERT">
<connects>
<connect gate="G$1" pin="1" pad="GND"/>
<connect gate="G$1" pin="2" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ROCKER" package="R_SW_TH">
<connects>
<connect gate="G$1" pin="1" pad="P$3"/>
<connect gate="G$1" pin="2" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5MM" package="SCREWTERMINAL-5MM-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="STOREFRONT_ID" value="PRT-08432"/>
</technology>
</technologies>
</device>
<device name="LOCK" package="1X02_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR_LOCK" package="MOLEX-1X2_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X02_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.5MM_LOCK" package="SCREWTERMINAL-3.5MM-2_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08399"/>
</technology>
</technologies>
</device>
<device name="PTH3" package="1X02_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1X02_NO_SILK" package="1X02_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-PTH-2" package="JST-2-PTH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09863"/>
<attribute name="SKU" value="PRT-09914"/>
</technology>
</technologies>
</device>
<device name="PTH4" package="1X02_XTRA_BIG">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POGO_PIN_HOLES_ONLY" package="1X02_PP_HOLES_ONLY">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.5MM-NO_SILK" package="SCREWTERMINAL-3.5MM-2-NS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08399"/>
</technology>
</technologies>
</device>
<device name="-JST-2-PTH-NO_SILK" package="JST-2-PTH-NS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-PTH-2-KIT" package="JST-2-PTH-KIT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SPRING-2.54-RA" package="SPRINGTERMINAL-2.54MM-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2.54MM_SCREWTERM" package="1X02_2.54_SCREWTERM">
<connects>
<connect gate="G$1" pin="1" pad="P1"/>
<connect gate="G$1" pin="2" pad="P2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-PTH-VERT" package="JST-2-PTH-VERT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="con-amp-quick">
<description>&lt;b&gt;AMP Connectors, Type QUICK&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="03P">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="M03">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="M03" prefix="SL" uservalue="yes">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="M03"/>
</gates>
<devices>
<device name="" package="03P">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="v-reg">
<description>&lt;b&gt;Voltage Regulators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DPACK">
<description>&lt;b&gt;DPAK&lt;/b&gt;&lt;p&gt;
PLASTIC PACKAGE CASE 369C-01&lt;br&gt;
Source: http://www.onsemi.co.jp .. LM317M-D.PDF</description>
</package>
<package name="TO220L1">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
<package name="SOT223">
<description>&lt;b&gt;Small Outline Transistor 223&lt;/b&gt;&lt;p&gt;
PLASTIC PACKAGE CASE 318E-04&lt;br&gt;
Source: http://www.onsemi.co.jp .. LM137M-D.PDF</description>
</package>
<package name="D2PACK">
<description>&lt;b&gt;D2PACK&lt;/b&gt;&lt;p&gt;
INTERNATIONAL RECTIFIER, irg4bc15ud-s.pdf</description>
</package>
</packages>
<symbols>
<symbol name="78ADJ">
<pin name="IN" direction="in"/>
<pin name="ADJ" direction="in"/>
<pin name="OUT" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="LD117A?*" prefix="IC">
<description>&lt;b&gt;Low drop fixed and adjustable positive voltage regulators&lt;/b&gt; 1 A&lt;p&gt;
Source: http://www.st.com/stonline/products/literature/ds/7194/ld1117axx.pdf</description>
<gates>
<gate name="G$1" symbol="78ADJ"/>
</gates>
<devices>
<device name="DT" package="DPACK">
<connects>
<connect gate="G$1" pin="ADJ" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="4"/>
</connects>
<technologies>
<technology name="-TR"/>
<technology name="12TR"/>
<technology name="18TR"/>
<technology name="25TR"/>
<technology name="28TR"/>
<technology name="33TR"/>
<technology name="50TR"/>
</technologies>
</device>
<device name="V" package="TO220L1">
<connects>
<connect gate="G$1" pin="ADJ" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
<technology name="12"/>
<technology name="18"/>
<technology name="25"/>
<technology name="28"/>
<technology name="33"/>
<technology name="50"/>
</technologies>
</device>
<device name="S" package="SOT223">
<connects>
<connect gate="G$1" pin="ADJ" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="4"/>
</connects>
<technologies>
<technology name="12TR"/>
<technology name="18TR"/>
<technology name="25TR"/>
<technology name="28TR"/>
<technology name="33TR"/>
<technology name="50TR"/>
<technology name="TR"/>
</technologies>
</device>
<device name="D2MTR" package="D2PACK">
<connects>
<connect gate="G$1" pin="ADJ" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<parts>
<part name="SJR1" library="esp12e" deviceset="ESP8266-12E" device="ESP12E"/>
<part name="U$7" library="fab" deviceset="FTDI-SMD-HEADER" device=""/>
<part name="S1" library="fab" deviceset="6MM_SWITCH" device="6MM_SWITCH"/>
<part name="IC1" library="fab" deviceset="REGULATOR" device="SOT23"/>
<part name="S2" library="fab" deviceset="6MM_SWITCH" device="6MM_SWITCH"/>
<part name="C1" library="fab" deviceset="CAP-US" device="1206FAB" value="10uf"/>
<part name="R7" library="fab" deviceset="RES-US" device="1206FAB" value="10k"/>
<part name="R8" library="fab" deviceset="RES-US" device="1206FAB" value="10k"/>
<part name="R1" library="fab" deviceset="RES-US" device="1206FAB"/>
<part name="K1" library="Seeed-OPL-Relay" deviceset="RELAY-HLS8L-DC5V-S-C(5P-19X15MM)" device="" value="HLS8L-DC5V-S-C"/>
<part name="GND1" library="FAB_Hello" deviceset="GND" device=""/>
<part name="P+1" library="FAB_Hello" deviceset="VCC" device=""/>
<part name="J1" library="SparkFun-Connectors" deviceset="M02" device="POLAR_LOCK"/>
<part name="T1" library="fab" deviceset="NMOSFET" device="SOT23"/>
<part name="R2" library="fab" deviceset="RES-US" device="1206FAB"/>
<part name="K2" library="Seeed-OPL-Relay" deviceset="RELAY-HLS8L-DC5V-S-C(5P-19X15MM)" device="" value="HLS8L-DC5V-S-C"/>
<part name="GND2" library="FAB_Hello" deviceset="GND" device=""/>
<part name="P+2" library="FAB_Hello" deviceset="VCC" device=""/>
<part name="J2" library="SparkFun-Connectors" deviceset="M02" device="POLAR_LOCK"/>
<part name="T2" library="fab" deviceset="NMOSFET" device="SOT23"/>
<part name="J4" library="fab" deviceset="JACK" device="2.1MM"/>
<part name="R3" library="fab" deviceset="RES-US" device="1206FAB" value="10k"/>
<part name="R4" library="fab" deviceset="RES-US" device="1206FAB" value="10k"/>
<part name="SL1" library="con-amp-quick" deviceset="M03" device=""/>
<part name="R5" library="fab" deviceset="RES-US" device="1206FAB"/>
<part name="IC2" library="v-reg" deviceset="LD117A?*" device="S" technology="12TR"/>
<part name="U$1" library="fab" deviceset="LED" device="FAB1206"/>
<part name="U$2" library="fab" deviceset="LED" device="FAB1206"/>
<part name="R6" library="fab" deviceset="RES-US" device="1206FAB" value="0"/>
<part name="R9" library="fab" deviceset="RES-US" device="1206FAB" value="0"/>
<part name="R10" library="fab" deviceset="RES-US" device="1206FAB" value="0"/>
<part name="R11" library="fab" deviceset="RES-US" device="1206FAB" value="0"/>
<part name="R12" library="fab" deviceset="RES-US" device="1206FAB" value="0"/>
<part name="R13" library="fab" deviceset="RES-US" device="1206FAB" value="0"/>
<part name="R14" library="fab" deviceset="RES-US" device="1206FAB" value="0"/>
</parts>
<sheets>
<sheet>
<plain>
</plain>
<busses>
</busses>
<nets>
<net name="GND">
<segment>
<pinref part="SJR1" gate="G$1" pin="GND"/>
<pinref part="R8" gate="G$1" pin="2"/>
<pinref part="S1" gate="2" pin="S1"/>
<pinref part="S1" gate="2" pin="S"/>
</segment>
<segment>
<pinref part="U$7" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="S2" gate="2" pin="P"/>
<pinref part="S2" gate="2" pin="P1"/>
<pinref part="C1" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="T1" gate="A" pin="S"/>
<pinref part="GND1" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="T2" gate="A" pin="S"/>
<pinref part="GND2" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="J4" gate="G$1" pin="CONTACT"/>
</segment>
<segment>
<pinref part="SL1" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="ADJ"/>
</segment>
</net>
<net name="N$3">
<segment>
<pinref part="SJR1" gate="G$1" pin="TXD"/>
<pinref part="U$7" gate="G$1" pin="RXD"/>
</segment>
</net>
<net name="N$4">
<segment>
<pinref part="SJR1" gate="G$1" pin="RXD"/>
<pinref part="U$7" gate="G$1" pin="TXD"/>
</segment>
</net>
<net name="N$8">
<segment>
<pinref part="S1" gate="2" pin="P"/>
<pinref part="SJR1" gate="G$1" pin="GPIO0"/>
<pinref part="S1" gate="2" pin="P1"/>
<pinref part="R3" gate="G$1" pin="2"/>
</segment>
</net>
<net name="3V3">
<segment>
<pinref part="R7" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="OUT"/>
<pinref part="SJR1" gate="G$1" pin="VCC"/>
<pinref part="R4" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="R3" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$11">
<segment>
<pinref part="S2" gate="2" pin="S"/>
<pinref part="S2" gate="2" pin="S1"/>
<pinref part="C1" gate="G$1" pin="1"/>
<pinref part="R7" gate="G$1" pin="2"/>
<pinref part="SJR1" gate="G$1" pin="REST"/>
</segment>
</net>
<net name="N$5">
<segment>
<pinref part="R8" gate="G$1" pin="1"/>
<pinref part="SJR1" gate="G$1" pin="GPIO15"/>
</segment>
</net>
<net name="N$2">
<segment>
<pinref part="K1" gate="G$1" pin="V-"/>
<pinref part="T1" gate="A" pin="D"/>
<pinref part="U$1" gate="G$1" pin="A"/>
</segment>
</net>
<net name="VCC">
<segment>
<pinref part="P+1" gate="VCC" pin="VCC"/>
<pinref part="K1" gate="G$1" pin="V+"/>
<pinref part="U$1" gate="G$1" pin="C"/>
</segment>
<segment>
<pinref part="U$7" gate="G$1" pin="VCC"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="IN"/>
</segment>
<segment>
<pinref part="K2" gate="G$1" pin="V+"/>
<pinref part="P+2" gate="VCC" pin="VCC"/>
<pinref part="U$2" gate="G$1" pin="C"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="OUT"/>
</segment>
</net>
<net name="N$1">
<segment>
<pinref part="R1" gate="G$1" pin="2"/>
<pinref part="T1" gate="A" pin="G"/>
</segment>
</net>
<net name="CONTROL">
<segment>
<pinref part="R2" gate="G$1" pin="1"/>
<pinref part="SJR1" gate="G$1" pin="GPIO5"/>
</segment>
</net>
<net name="N$6">
<segment>
<pinref part="K1" gate="G$1" pin="NO"/>
<pinref part="J1" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$7">
<segment>
<pinref part="K1" gate="G$1" pin="COM"/>
<pinref part="J1" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$10">
<segment>
<pinref part="K2" gate="G$1" pin="V-"/>
<pinref part="T2" gate="A" pin="D"/>
<pinref part="U$2" gate="G$1" pin="A"/>
</segment>
</net>
<net name="N$12">
<segment>
<pinref part="R2" gate="G$1" pin="2"/>
<pinref part="T2" gate="A" pin="G"/>
</segment>
</net>
<net name="N$13">
<segment>
<pinref part="K2" gate="G$1" pin="NO"/>
<pinref part="J2" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$14">
<segment>
<pinref part="K2" gate="G$1" pin="COM"/>
<pinref part="J2" gate="G$1" pin="1"/>
</segment>
</net>
<net name="12V">
<segment>
<pinref part="J4" gate="G$1" pin="PIN"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="IN"/>
</segment>
<segment>
<pinref part="SL1" gate="G$1" pin="3"/>
</segment>
</net>
<net name="CONTROL02">
<segment>
<pinref part="R1" gate="G$1" pin="1"/>
<pinref part="SJR1" gate="G$1" pin="GPIO4"/>
</segment>
</net>
<net name="N$15">
<segment>
<pinref part="SJR1" gate="G$1" pin="CH_PD"/>
<pinref part="R4" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$9">
<segment>
<pinref part="SJR1" gate="G$1" pin="GPIO14"/>
<pinref part="R5" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$17">
<segment>
<pinref part="R5" gate="G$1" pin="1"/>
<pinref part="SL1" gate="G$1" pin="2"/>
</segment>
</net>
</nets>
</sheet>
</sheets>
</schematic>
</drawing>
</eagle>
