<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<board>
<plain>
<wire x1="24.13" y1="21.59" x2="114.28" y2="21.59" width="0" layer="20"/>
<wire x1="114.28" y1="21.59" x2="114.28" y2="88.57" width="0" layer="20"/>
<wire x1="114.28" y1="88.57" x2="24.13" y2="88.57" width="0" layer="20"/>
<wire x1="24.13" y1="88.57" x2="24.13" y2="21.59" width="0" layer="20"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="C1206FAB">
</package>
<package name="1X06SMD">
</package>
<package name="2X03SMD">
</package>
<package name="R1206FAB">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X04/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X03/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="atmega8">
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="crystal">
<description>&lt;b&gt;Crystals and Crystal Resonators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="CSM-7X-DU">
<description>&lt;b&gt;SMD CRYSTAL&lt;/b&gt;&lt;p&gt;
Source: www.ecsxtal.com .. Crystal 3.6864MHz CSM_7X_DU.PDF</description>
</package>
</packages>
</library>
<library name="01_SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="fab" package="C1206FAB" value="22 pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="fab" package="C1206FAB" value="22 pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="DHT22" library="pinhead" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FTDI" library="fab" package="1X06SMD" value="FTDI-SMD-HEADER">
<attribute name="FTDI" value=""/>
<attribute name="NAME"/>
</element>
<element name="ISP" library="fab" package="2X03SMD" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LCDI2C" library="pinhead" package="1X04/90" value="">
<attribute name="LCD" value=""/>
<attribute name="VALUE"/>
</element>
<element name="MICRO" library="atmega8" package="TQFP32-08" value="ATMEGA328P-AU">
<attribute name="VALUE"/>
</element>
<element name="POWER" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="fab" package="R1206FAB" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="fab" package="R1206FAB" value="10 K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="REDLED" library="fab" package="LED1206FAB" value="RED LED">
<attribute name="VALUE"/>
</element>
<element name="RELAY1" library="pinhead" package="1X03/90" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RESET" library="fab" package="6MM_SWITCH" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CRYSTAL" library="crystal" package="CSM-7X-DU" value="16Mhz">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="01_SparkFun" package="1206" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="01_SparkFun" package="1206" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="01_SparkFun" package="1206" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="fab" package="C1206FAB" value="100 nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="P7">
<contactref element="MICRO" pad="7"/>
<contactref element="C1" pad="2"/>
<contactref element="CRYSTAL" pad="2"/>
</signal>
<signal name="P8">
<contactref element="MICRO" pad="8"/>
<contactref element="C2" pad="2"/>
<contactref element="CRYSTAL" pad="1"/>
</signal>
<signal name="GND">
<contactref element="MICRO" pad="3"/>
<contactref element="MICRO" pad="5"/>
<contactref element="MICRO" pad="21"/>
<contactref element="REDLED" pad="2"/>
<contactref element="FTDI" pad="1"/>
<contactref element="RESET" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="ISP" pad="6"/>
<contactref element="RELAY1" pad="3"/>
<contactref element="LCDI2C" pad="1"/>
<contactref element="POWER" pad="2"/>
<contactref element="DHT22" pad="3"/>
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="RESET" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="FTDI" pad="3"/>
<contactref element="RELAY1" pad="2"/>
<contactref element="LCDI2C" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="MICRO" pad="6"/>
<contactref element="MICRO" pad="4"/>
<contactref element="MICRO" pad="18"/>
<contactref element="R2" pad="1"/>
<contactref element="POWER" pad="1"/>
<contactref element="ISP" pad="2"/>
<contactref element="DHT22" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="29">
<contactref element="MICRO" pad="29"/>
<contactref element="R2" pad="2"/>
<contactref element="RESET" pad="4"/>
<contactref element="C3" pad="1"/>
<contactref element="ISP" pad="5"/>
<contactref element="RESET" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="REDLED" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="27">
<contactref element="MICRO" pad="27"/>
<contactref element="LCDI2C" pad="3"/>
</signal>
<signal name="28">
<contactref element="MICRO" pad="28"/>
<contactref element="LCDI2C" pad="4"/>
</signal>
<signal name="31">
<contactref element="FTDI" pad="4"/>
<contactref element="MICRO" pad="30"/>
</signal>
<signal name="30">
<contactref element="FTDI" pad="5"/>
<contactref element="MICRO" pad="31"/>
</signal>
<signal name="15">
<contactref element="ISP" pad="4"/>
<contactref element="MICRO" pad="15"/>
</signal>
<signal name="16">
<contactref element="MICRO" pad="16"/>
<contactref element="ISP" pad="1"/>
</signal>
<signal name="17">
<contactref element="ISP" pad="3"/>
<contactref element="MICRO" pad="17"/>
</signal>
<signal name="P1">
<contactref element="MICRO" pad="1"/>
<contactref element="DHT22" pad="2"/>
</signal>
<signal name="P14">
<contactref element="MICRO" pad="14"/>
<contactref element="RELAY1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="C3" pad="2"/>
<contactref element="FTDI" pad="6"/>
</signal>
<signal name="OUTLINE">
</signal>
</signals>
</board>
</drawing>
</eagle>
