<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.2">
<drawing>
<schematic>
<libraries>
<library name="fab">
<packages>
<package name="SOIC14">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="QFN/MLF20">
<description>&lt;b&gt;HP-VFQFP-N20&lt;/b&gt; Micro Lead Frame package (MLF)</description>
</package>
<package name="1X06SMD">
</package>
<package name="EFOBM">
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R1206W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="R1206FAB">
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1206FAB">
</package>
<package name="C2220">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="2X03SMD">
</package>
<package name="OP1206">
</package>
</packages>
<symbols>
<symbol name="ATTINY24/44/84">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="(PCINT7/ICP/OC0B/ADC7)PA7"/>
<pin name="(PCINT6/OC1A/SDA/MOSI/ADC6)PA6"/>
<pin name="(PCINT5/OC1B/MISO/DO/ADC5)PA5"/>
<pin name="(PCINT4/T1/SCL/USCK/ADC4)PA4"/>
<pin name="(PCINT3/T0/ADC3)PA3"/>
<pin name="(PCINT2/AIN1/ADC2)PA2"/>
<pin name="(PCINT1/AIN0/ADC1)PA1"/>
<pin name="(PCINT0/AREF/ADC0)PA0"/>
<pin name="(PCINT11/RESET/DW)PB3"/>
<pin name="(PCINT10/INT0/OC0A/CKOUT)PB2"/>
<pin name="(PCINT9/XTAL2)PB1"/>
<pin name="(PCINT8/XTAL1/CLKI)PB0"/>
</symbol>
<symbol name="FTDI">
<pin name="GND"/>
<pin name="CTS"/>
<pin name="VCC"/>
<pin name="TXD"/>
<pin name="RXD"/>
<pin name="RTS"/>
</symbol>
<symbol name="CERAMIC_RESONATOR">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="R-US">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="CAP-NONPOLARIZED">
<description>non-polarized capacitor</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="PINH2X3">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
</symbol>
<symbol name="PHOTOTRANSISTOR">
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ATTINY44" prefix="IC">
<gates>
<gate name="1" symbol="ATTINY24/44/84"/>
</gates>
<devices>
<device name="-SSU" package="SOIC14">
<connects>
<connect gate="1" pin="(PCINT0/AREF/ADC0)PA0" pad="13"/>
<connect gate="1" pin="(PCINT1/AIN0/ADC1)PA1" pad="12"/>
<connect gate="1" pin="(PCINT10/INT0/OC0A/CKOUT)PB2" pad="5"/>
<connect gate="1" pin="(PCINT11/RESET/DW)PB3" pad="4"/>
<connect gate="1" pin="(PCINT2/AIN1/ADC2)PA2" pad="11"/>
<connect gate="1" pin="(PCINT3/T0/ADC3)PA3" pad="10"/>
<connect gate="1" pin="(PCINT4/T1/SCL/USCK/ADC4)PA4" pad="9"/>
<connect gate="1" pin="(PCINT5/OC1B/MISO/DO/ADC5)PA5" pad="8"/>
<connect gate="1" pin="(PCINT6/OC1A/SDA/MOSI/ADC6)PA6" pad="7"/>
<connect gate="1" pin="(PCINT7/ICP/OC0B/ADC7)PA7" pad="6"/>
<connect gate="1" pin="(PCINT8/XTAL1/CLKI)PB0" pad="2"/>
<connect gate="1" pin="(PCINT9/XTAL2)PB1" pad="3"/>
<connect gate="1" pin="GND" pad="14"/>
<connect gate="1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-PU" package="DIL14">
<connects>
<connect gate="1" pin="(PCINT0/AREF/ADC0)PA0" pad="13"/>
<connect gate="1" pin="(PCINT1/AIN0/ADC1)PA1" pad="12"/>
<connect gate="1" pin="(PCINT10/INT0/OC0A/CKOUT)PB2" pad="5"/>
<connect gate="1" pin="(PCINT11/RESET/DW)PB3" pad="4"/>
<connect gate="1" pin="(PCINT2/AIN1/ADC2)PA2" pad="11"/>
<connect gate="1" pin="(PCINT3/T0/ADC3)PA3" pad="10"/>
<connect gate="1" pin="(PCINT4/T1/SCL/USCK/ADC4)PA4" pad="9"/>
<connect gate="1" pin="(PCINT5/OC1B/MISO/DO/ADC5)PA5" pad="8"/>
<connect gate="1" pin="(PCINT6/OC1A/SDA/MOSI/ADC6)PA6" pad="7"/>
<connect gate="1" pin="(PCINT7/ICP/OC0B/ADC7)PA7" pad="6"/>
<connect gate="1" pin="(PCINT8/XTAL1/CLKI)PB0" pad="2"/>
<connect gate="1" pin="(PCINT9/XTAL2)PB1" pad="3"/>
<connect gate="1" pin="GND" pad="14"/>
<connect gate="1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MU" package="QFN/MLF20">
<connects>
<connect gate="1" pin="(PCINT0/AREF/ADC0)PA0" pad="5"/>
<connect gate="1" pin="(PCINT1/AIN0/ADC1)PA1" pad="4"/>
<connect gate="1" pin="(PCINT10/INT0/OC0A/CKOUT)PB2" pad="14"/>
<connect gate="1" pin="(PCINT11/RESET/DW)PB3" pad="13"/>
<connect gate="1" pin="(PCINT2/AIN1/ADC2)PA2" pad="3"/>
<connect gate="1" pin="(PCINT3/T0/ADC3)PA3" pad="2"/>
<connect gate="1" pin="(PCINT4/T1/SCL/USCK/ADC4)PA4" pad="1"/>
<connect gate="1" pin="(PCINT5/OC1B/MISO/DO/ADC5)PA5" pad="20"/>
<connect gate="1" pin="(PCINT6/OC1A/SDA/MOSI/ADC6)PA6" pad="16"/>
<connect gate="1" pin="(PCINT7/ICP/OC0B/ADC7)PA7" pad="15"/>
<connect gate="1" pin="(PCINT8/XTAL1/CLKI)PB0" pad="11"/>
<connect gate="1" pin="(PCINT9/XTAL2)PB1" pad="12"/>
<connect gate="1" pin="GND" pad="8"/>
<connect gate="1" pin="VCC" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FTDI-SMD-HEADER">
<gates>
<gate name="G$1" symbol="FTDI"/>
</gates>
<devices>
<device name="" package="1X06SMD">
<connects>
<connect gate="G$1" pin="CTS" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="RTS" pad="6"/>
<connect gate="G$1" pin="RXD" pad="5"/>
<connect gate="G$1" pin="TXD" pad="4"/>
<connect gate="G$1" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RESONATOR">
<gates>
<gate name="G$1" symbol="CERAMIC_RESONATOR"/>
</gates>
<devices>
<device name="" package="EFOBM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RES-US" prefix="R" uservalue="yes">
<description>&lt;b&gt;Resistor (US Symbol)&lt;/b&gt;
&lt;p&gt;
Variants with postfix FAB are widened to allow the routing of internal traces</description>
<gates>
<gate name="G$1" symbol="R-US"/>
</gates>
<devices>
<device name="1206" package="R1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206W" package="R1206W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206FAB" package="R1206FAB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAP-UNPOLARIZED" prefix="C" uservalue="yes">
<gates>
<gate name="&gt;NAME" symbol="CAP-NONPOLARIZED"/>
</gates>
<devices>
<device name="" package="C1206">
<connects>
<connect gate="&gt;NAME" pin="1" pad="1"/>
<connect gate="&gt;NAME" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FAB" package="C1206FAB">
<connects>
<connect gate="&gt;NAME" pin="1" pad="1"/>
<connect gate="&gt;NAME" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2220" package="C2220">
<connects>
<connect gate="&gt;NAME" pin="1" pad="1"/>
<connect gate="&gt;NAME" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X3-SMD" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X3"/>
</gates>
<devices>
<device name="" package="2X03SMD">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PHOTOTRANSISTOR-NPN">
<gates>
<gate name="G$1" symbol="PHOTOTRANSISTOR"/>
</gates>
<devices>
<device name="1206" package="OP1206">
<connects>
<connect gate="G$1" pin="C" pad="COLLECTOR"/>
<connect gate="G$1" pin="E" pad="EMITTER"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="supply1">
<description>&lt;b&gt;Supply Symbols&lt;/b&gt;&lt;p&gt;
 GND, VCC, 0V, +5V, -5V, etc.&lt;p&gt;
 Please keep in mind, that these devices are necessary for the
 automatic wiring of the supply signals.&lt;p&gt;
 The pin name defined in the symbol is identical to the net which is to be wired automatically.&lt;p&gt;
 In this library the device names are the same as the pin names of the symbols, therefore the correct signal names appear next to the supply symbols in the schematic.&lt;p&gt;
 &lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
</packages>
<symbols>
<symbol name="GND">
<pin name="GND" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="GND" prefix="GND">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="GND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="ADXL343BCCZ">
<packages>
<package name="LGA_CC-14-1-M">
</package>
<package name="LGA_CC-14-1-L">
</package>
<package name="LGA_CC-14-1">
</package>
</packages>
<symbols>
<symbol name="ADXL343BCCZ">
<pin name="VDD_I/O" direction="pas"/>
<pin name="VS" direction="pas"/>
<pin name="INT1" direction="pas"/>
<pin name="INT2" direction="pas"/>
<pin name="!CS" direction="pas"/>
<pin name="SCL/SCLK" direction="pas"/>
<pin name="SDA/SDI/SDIO" direction="pas"/>
<pin name="SDO/ALT_ADDRESS" direction="pas"/>
<pin name="RESERVED_2" direction="pas"/>
<pin name="RESERVED" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NC" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ADXL343BCCZ" prefix="U">
<gates>
<gate name="A" symbol="ADXL343BCCZ"/>
</gates>
<devices>
<device name="" package="LGA_CC-14-1">
<connects>
<connect gate="A" pin="!CS" pad="7"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="GND_2" pad="2"/>
<connect gate="A" pin="GND_3" pad="4"/>
<connect gate="A" pin="INT1" pad="8"/>
<connect gate="A" pin="INT2" pad="9"/>
<connect gate="A" pin="NC" pad="10"/>
<connect gate="A" pin="RESERVED" pad="11"/>
<connect gate="A" pin="RESERVED_2" pad="3"/>
<connect gate="A" pin="SCL/SCLK" pad="14"/>
<connect gate="A" pin="SDA/SDI/SDIO" pad="13"/>
<connect gate="A" pin="SDO/ALT_ADDRESS" pad="12"/>
<connect gate="A" pin="VDD_I/O" pad="1"/>
<connect gate="A" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER_PART_NUMBER" value="ADXL343BCCZ"/>
<attribute name="VENDOR" value="Analog Devices Inc"/>
</technology>
</technologies>
</device>
<device name="LGA_CC-14-1-M" package="LGA_CC-14-1-M">
<connects>
<connect gate="A" pin="!CS" pad="7"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="GND_2" pad="2"/>
<connect gate="A" pin="GND_3" pad="4"/>
<connect gate="A" pin="INT1" pad="8"/>
<connect gate="A" pin="INT2" pad="9"/>
<connect gate="A" pin="NC" pad="10"/>
<connect gate="A" pin="RESERVED" pad="11"/>
<connect gate="A" pin="RESERVED_2" pad="3"/>
<connect gate="A" pin="SCL/SCLK" pad="14"/>
<connect gate="A" pin="SDA/SDI/SDIO" pad="13"/>
<connect gate="A" pin="SDO/ALT_ADDRESS" pad="12"/>
<connect gate="A" pin="VDD_I/O" pad="1"/>
<connect gate="A" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER_PART_NUMBER" value="ADXL343BCCZ"/>
<attribute name="VENDOR" value="Analog Devices Inc"/>
</technology>
</technologies>
</device>
<device name="LGA_CC-14-1-L" package="LGA_CC-14-1-L">
<connects>
<connect gate="A" pin="!CS" pad="7"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="GND_2" pad="2"/>
<connect gate="A" pin="GND_3" pad="4"/>
<connect gate="A" pin="INT1" pad="8"/>
<connect gate="A" pin="INT2" pad="9"/>
<connect gate="A" pin="NC" pad="10"/>
<connect gate="A" pin="RESERVED" pad="11"/>
<connect gate="A" pin="RESERVED_2" pad="3"/>
<connect gate="A" pin="SCL/SCLK" pad="14"/>
<connect gate="A" pin="SDA/SDI/SDIO" pad="13"/>
<connect gate="A" pin="SDO/ALT_ADDRESS" pad="12"/>
<connect gate="A" pin="VDD_I/O" pad="1"/>
<connect gate="A" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER_PART_NUMBER" value="ADXL343BCCZ"/>
<attribute name="VENDOR" value="Analog Devices Inc"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<parts>
<part name="IC1" library="fab" deviceset="ATTINY44" device="-SSU"/>
<part name="U$1" library="fab" deviceset="FTDI-SMD-HEADER" device=""/>
<part name="U$2" library="fab" deviceset="RESONATOR" device="" value="20MHz"/>
<part name="R1" library="fab" deviceset="RES-US" device="1206FAB" value="10k"/>
<part name="C1" library="fab" deviceset="CAP-UNPOLARIZED" device="FAB" value="1uF"/>
<part name="GND1" library="supply1" deviceset="GND" device=""/>
<part name="GND2" library="supply1" deviceset="GND" device=""/>
<part name="JP1" library="fab" deviceset="PINHD-2X3-SMD" device="" value="J1"/>
<part name="GND4" library="supply1" deviceset="GND" device=""/>
<part name="U1" library="ADXL343BCCZ" deviceset="ADXL343BCCZ" device="" value="ADXL343BCCZ"/>
<part name="R2" library="fab" deviceset="RES-US" device="1206FAB" value="10K"/>
<part name="R3" library="fab" deviceset="RES-US" device="1206FAB" value="10K"/>
<part name="GND3" library="supply1" deviceset="GND" device=""/>
<part name="C3" library="fab" deviceset="CAP-UNPOLARIZED" device="FAB" value="1uF"/>
<part name="GND6" library="supply1" deviceset="GND" device=""/>
<part name="U$3" library="fab" deviceset="PHOTOTRANSISTOR-NPN" device="1206"/>
<part name="GND7" library="supply1" deviceset="GND" device=""/>
<part name="GND8" library="supply1" deviceset="GND" device=""/>
<part name="R4" library="fab" deviceset="RES-US" device="1206FAB" value="0ohm"/>
<part name="R5" library="fab" deviceset="RES-US" device="1206FAB" value="0ohm"/>
<part name="GND9" library="supply1" deviceset="GND" device=""/>
<part name="R6" library="fab" deviceset="RES-US" device="1206FAB" value="10K"/>
</parts>
<sheets>
<sheet>
<plain>
</plain>
<busses>
</busses>
<nets>
<net name="XTAL1">
<segment>
<pinref part="IC1" gate="1" pin="(PCINT8/XTAL1/CLKI)PB0"/>
</segment>
<segment>
<pinref part="U$2" gate="G$1" pin="3"/>
</segment>
</net>
<net name="XTAL2">
<segment>
<pinref part="IC1" gate="1" pin="(PCINT9/XTAL2)PB1"/>
</segment>
<segment>
<pinref part="U$2" gate="G$1" pin="1"/>
</segment>
</net>
<net name="GND">
<segment>
<pinref part="C1" gate="&gt;NAME" pin="1"/>
<pinref part="GND2" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="IC1" gate="1" pin="GND"/>
<pinref part="GND1" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="JP1" gate="A" pin="1"/>
<pinref part="GND4" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="U1" gate="A" pin="GND"/>
</segment>
<segment>
<pinref part="U1" gate="A" pin="GND_3"/>
</segment>
<segment>
<pinref part="U1" gate="A" pin="GND_2"/>
</segment>
<segment>
<pinref part="U$1" gate="G$1" pin="GND"/>
<pinref part="GND3" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="C3" gate="&gt;NAME" pin="1"/>
<pinref part="GND6" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="U$3" gate="G$1" pin="C"/>
<pinref part="GND7" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="U1" gate="A" pin="NC"/>
</segment>
<segment>
<pinref part="U1" gate="A" pin="SDO/ALT_ADDRESS"/>
</segment>
<segment>
<pinref part="U$2" gate="G$1" pin="2"/>
<pinref part="GND8" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="R4" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="R5" gate="G$1" pin="2"/>
<pinref part="GND9" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="R4" gate="G$1" pin="2"/>
<pinref part="R5" gate="G$1" pin="1"/>
</segment>
</net>
<net name="PA0">
<segment>
<pinref part="IC1" gate="1" pin="(PCINT0/AREF/ADC0)PA0"/>
</segment>
<segment>
<pinref part="U$1" gate="G$1" pin="TXD"/>
</segment>
</net>
<net name="PA1">
<segment>
<pinref part="IC1" gate="1" pin="(PCINT1/AIN0/ADC1)PA1"/>
</segment>
<segment>
<pinref part="U$1" gate="G$1" pin="RXD"/>
</segment>
</net>
<net name="MOSI">
<segment>
<pinref part="IC1" gate="1" pin="(PCINT6/OC1A/SDA/MOSI/ADC6)PA6"/>
</segment>
<segment>
<pinref part="JP1" gate="A" pin="3"/>
</segment>
</net>
<net name="MISO">
<segment>
<pinref part="IC1" gate="1" pin="(PCINT5/OC1B/MISO/DO/ADC5)PA5"/>
</segment>
<segment>
<pinref part="JP1" gate="A" pin="6"/>
</segment>
</net>
<net name="SCK">
<segment>
<pinref part="IC1" gate="1" pin="(PCINT4/T1/SCL/USCK/ADC4)PA4"/>
</segment>
<segment>
<pinref part="JP1" gate="A" pin="4"/>
</segment>
</net>
<net name="RST">
<segment>
<pinref part="JP1" gate="A" pin="2"/>
</segment>
<segment>
<pinref part="IC1" gate="1" pin="(PCINT11/RESET/DW)PB3"/>
<pinref part="R1" gate="G$1" pin="1"/>
</segment>
</net>
<net name="OUT">
<segment>
<pinref part="R2" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="R3" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="U1" gate="A" pin="VDD_I/O"/>
</segment>
<segment>
<pinref part="U1" gate="A" pin="VS"/>
</segment>
<segment>
<pinref part="R1" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="C1" gate="&gt;NAME" pin="2"/>
</segment>
<segment>
<pinref part="IC1" gate="1" pin="VCC"/>
</segment>
<segment>
<pinref part="JP1" gate="A" pin="5"/>
</segment>
<segment>
<pinref part="U1" gate="A" pin="!CS"/>
</segment>
<segment>
<pinref part="C3" gate="&gt;NAME" pin="2"/>
</segment>
<segment>
<pinref part="R6" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="U$1" gate="G$1" pin="VCC"/>
</segment>
</net>
<net name="PA3">
<segment>
<pinref part="IC1" gate="1" pin="(PCINT3/T0/ADC3)PA3"/>
</segment>
<segment>
<pinref part="U1" gate="A" pin="SCL/SCLK"/>
</segment>
<segment>
<pinref part="R2" gate="G$1" pin="1"/>
</segment>
</net>
<net name="PA2">
<segment>
<pinref part="IC1" gate="1" pin="(PCINT2/AIN1/ADC2)PA2"/>
</segment>
<segment>
<pinref part="U1" gate="A" pin="SDA/SDI/SDIO"/>
</segment>
<segment>
<pinref part="R3" gate="G$1" pin="1"/>
</segment>
</net>
<net name="PA7">
<segment>
<pinref part="IC1" gate="1" pin="(PCINT7/ICP/OC0B/ADC7)PA7"/>
</segment>
<segment>
<pinref part="U$3" gate="G$1" pin="E"/>
</segment>
<segment>
<pinref part="R6" gate="G$1" pin="1"/>
</segment>
</net>
</nets>
</sheet>
</sheets>
</schematic>
</drawing>
</eagle>
