<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.2">
<drawing>
<schematic>
<libraries>
<library name="microbuilder">
<description>&lt;h2&gt;&lt;b&gt;microBuilder.eu&lt;/b&gt; Eagle Footprint Library&lt;/h2&gt;

&lt;p&gt;Footprints for common components used in our projects and products.  This is the same library that we use internally, and it is regularly updated.  The newest version can always be found at &lt;b&gt;www.microBuilder.eu&lt;/b&gt;.  If you find this library useful, please feel free to purchase something from our online store. Please also note that all holes are optimised for metric drill bits!&lt;/p&gt;

&lt;h3&gt;Obligatory Warning&lt;/h3&gt;
&lt;p&gt;While it probably goes without saying, there are no guarantees that the footprints or schematic symbols in this library are flawless, and we make no promises of fitness for production, prototyping or any other purpose. These libraries are provided for information puposes only, and are used at your own discretion.  While we make every effort to produce accurate footprints, and many of the items found in this library have be proven in production, we can't make any promises of suitability for a specific purpose. If you do find any errors, though, please feel free to contact us at www.microbuilder.eu to let us know about it so that we can update the library accordingly!&lt;/p&gt;

&lt;h3&gt;License&lt;/h3&gt;
&lt;p&gt;This work is placed in the public domain, and may be freely used for commercial and non-commercial work with the following conditions:&lt;/p&gt;
&lt;p&gt;THIS SOFTWARE IS PROVIDED ''AS IS'' AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED.  IN NO EVENT SHALL THE INSTITUTE OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING,  BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
&lt;/p&gt;</description>
<packages>
<package name="CC3000MOD">
<description>&lt;p&gt;CC3000MOD Wireless Module&lt;/p&gt;
&lt;p&gt;Source: http://www.ti.com/lit/ds/symlink/cc3000.pdf&lt;/p&gt;</description>
</package>
<package name="TESTPOINT_SMT">
<description>Surface Mount Test Point - Compact SMT</description>
</package>
<package name="TESTPOINT_PAD_2MM">
<description>Testpoint - Pad</description>
</package>
<package name="TESTPOINT_ROUND_2MM">
<description>Testpoint - Round 2mm</description>
</package>
<package name="1X01_ROUND">
</package>
<package name="PAD-1.5X2.0">
<description>1.5 x 2.0mm SMT pad (no solder paste)</description>
</package>
<package name="TESTPOINT_ROUND_1MM">
</package>
<package name="TESTPOINT_ROUND_0.5MM">
</package>
<package name="TESTPOINT_PAD_1MM">
</package>
<package name="1X03_OVAL">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X03_ROUND">
</package>
<package name="1X03_SMT">
<description>&lt;p&gt;&lt;b&gt;Pin Headers&lt;/b&gt;&lt;br/&gt;
2 Pin, 0.1"/2.54mm pitch, SMT&lt;/p&gt;</description>
</package>
<package name="1X03_1.0MM">
</package>
<package name="1X03_ROUND_76">
</package>
<package name="SOT223-R">
<description>&lt;b&gt;SOT223&lt;/b&gt; - Reflow soldering</description>
</package>
<package name="1X09_OVAL">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X09_ROUND_76">
</package>
<package name="1X09_ROUND_70">
</package>
</packages>
<symbols>
<symbol name="CC3000MOD">
<pin name="GND@1" direction="pwr"/>
<pin name="RESERVED_1"/>
<pin name="NC@1" direction="nc"/>
<pin name="RESERVED_2"/>
<pin name="WL_EN2" direction="in"/>
<pin name="WL_RS232_TX" direction="out"/>
<pin name="WL_EN1" direction="in"/>
<pin name="WL_RS232_RX" direction="in"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="SPI_CS" direction="in"/>
<pin name="SPI_DOUT" direction="out"/>
<pin name="SPI_IRQ" direction="out"/>
<pin name="SPI_DIN" direction="in"/>
<pin name="GND@5" direction="pwr"/>
<pin name="SPI_CLK" direction="in"/>
<pin name="GND@6" direction="pwr"/>
<pin name="VBAT_IN" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="EXT_32K"/>
<pin name="GND@8" direction="pwr"/>
<pin name="VIO_HOST" direction="pwr"/>
<pin name="RESERVED_3"/>
<pin name="GND@9" direction="pwr"/>
<pin name="VBAT_SW_EN" direction="in"/>
<pin name="SDA_EEPROM"/>
<pin name="SDA_CC3000"/>
<pin name="SCL_EEPROM"/>
<pin name="SCL_CC3000"/>
<pin name="GND@10" direction="pwr"/>
<pin name="GND@11" direction="pwr"/>
<pin name="GND@12" direction="pwr"/>
<pin name="GND@13" direction="pwr"/>
<pin name="RF_ANT"/>
<pin name="GND@14" direction="pwr"/>
<pin name="GND@15" direction="pwr"/>
<pin name="GND@16" direction="pwr"/>
<pin name="GND@17" direction="pwr"/>
<pin name="GND@18" direction="pwr"/>
<pin name="GND@19" direction="pwr"/>
<pin name="GND@20" direction="pwr"/>
<pin name="GND@21" direction="pwr"/>
<pin name="GND@22" direction="pwr"/>
<pin name="GND@23" direction="pwr"/>
<pin name="GND@24" direction="pwr"/>
</symbol>
<symbol name="GND">
<pin name="GND" direction="sup"/>
</symbol>
<symbol name="TESTPOINT">
<pin name="P$1"/>
</symbol>
<symbol name="PINHD3">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
</symbol>
<symbol name="VBAT">
<pin name="VBAT" direction="sup"/>
</symbol>
<symbol name="VIN">
<pin name="VIN" direction="sup"/>
</symbol>
<symbol name="VREG_SOT223_FIXED">
<pin name="IN" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="OUT" direction="pwr"/>
</symbol>
<symbol name="PINHD9">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="CC3000MOD" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;CC3000MOD Wifi Module&lt;/b&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CC3000MOD"/>
</gates>
<devices>
<device name="" package="CC3000MOD">
<connects>
<connect gate="G$1" pin="EXT_32K" pad="21"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@10" pad="31"/>
<connect gate="G$1" pin="GND@11" pad="32"/>
<connect gate="G$1" pin="GND@12" pad="33"/>
<connect gate="G$1" pin="GND@13" pad="34"/>
<connect gate="G$1" pin="GND@14" pad="36"/>
<connect gate="G$1" pin="GND@15" pad="37"/>
<connect gate="G$1" pin="GND@16" pad="38"/>
<connect gate="G$1" pin="GND@17" pad="39"/>
<connect gate="G$1" pin="GND@18" pad="40"/>
<connect gate="G$1" pin="GND@19" pad="41"/>
<connect gate="G$1" pin="GND@2" pad="9"/>
<connect gate="G$1" pin="GND@20" pad="42"/>
<connect gate="G$1" pin="GND@21" pad="43"/>
<connect gate="G$1" pin="GND@22" pad="44"/>
<connect gate="G$1" pin="GND@23" pad="45"/>
<connect gate="G$1" pin="GND@24" pad="46"/>
<connect gate="G$1" pin="GND@3" pad="10"/>
<connect gate="G$1" pin="GND@4" pad="11"/>
<connect gate="G$1" pin="GND@5" pad="16"/>
<connect gate="G$1" pin="GND@6" pad="18"/>
<connect gate="G$1" pin="GND@7" pad="20"/>
<connect gate="G$1" pin="GND@8" pad="22"/>
<connect gate="G$1" pin="GND@9" pad="25"/>
<connect gate="G$1" pin="NC@1" pad="3"/>
<connect gate="G$1" pin="RESERVED_1" pad="2"/>
<connect gate="G$1" pin="RESERVED_2" pad="4"/>
<connect gate="G$1" pin="RESERVED_3" pad="24"/>
<connect gate="G$1" pin="RF_ANT" pad="35"/>
<connect gate="G$1" pin="SCL_CC3000" pad="30"/>
<connect gate="G$1" pin="SCL_EEPROM" pad="29"/>
<connect gate="G$1" pin="SDA_CC3000" pad="28"/>
<connect gate="G$1" pin="SDA_EEPROM" pad="27"/>
<connect gate="G$1" pin="SPI_CLK" pad="17"/>
<connect gate="G$1" pin="SPI_CS" pad="12"/>
<connect gate="G$1" pin="SPI_DIN" pad="15"/>
<connect gate="G$1" pin="SPI_DOUT" pad="13"/>
<connect gate="G$1" pin="SPI_IRQ" pad="14"/>
<connect gate="G$1" pin="VBAT_IN" pad="19"/>
<connect gate="G$1" pin="VBAT_SW_EN" pad="26"/>
<connect gate="G$1" pin="VIO_HOST" pad="23"/>
<connect gate="G$1" pin="WL_EN1" pad="7"/>
<connect gate="G$1" pin="WL_EN2" pad="5"/>
<connect gate="G$1" pin="WL_RS232_RX" pad="8"/>
<connect gate="G$1" pin="WL_RS232_TX" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GND">
<description>&lt;b&gt;GND&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="GND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TESTPOINT" prefix="TP" uservalue="yes">
<description>&lt;b&gt;Test Point&lt;/b&gt;
&lt;p&gt;Various test points for characterisation and PCB testing&lt;/p&gt;
&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;&lt;b&gt;TESTPOINT_SMT&lt;/b&gt; - Compact Surface Mount Test Point [Digikey: 5016KTR-ND]&lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TESTPOINT"/>
</gates>
<devices>
<device name="" package="TESTPOINT_SMT">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PAD2MM" package="TESTPOINT_PAD_2MM">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ROUND2MM" package="TESTPOINT_ROUND_2MM">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0.1&quot;" package="1X01_ROUND">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="BOM" value="EXCLUDE"/>
</technology>
</technologies>
</device>
<device name="1.5X2.0MM_NOCREAM" package="PAD-1.5X2.0">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ROUND1MM" package="TESTPOINT_ROUND_1MM">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ROUND0.5MM" package="TESTPOINT_ROUND_0.5MM">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PAD1MM" package="TESTPOINT_PAD_1MM">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-1X3" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD3"/>
</gates>
<devices>
<device name="" package="1X03_OVAL">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ROUND" package="1X03_ROUND">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMT" package="1X03_SMT">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1MMPADS" package="1X03_1.0MM">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="76MIL" package="1X03_ROUND_76">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VBAT">
<description>VBAT Supply Sumbol</description>
<gates>
<gate name="G$1" symbol="VBAT"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VIN">
<description>VIN Supply Symbol</description>
<gates>
<gate name="G$1" symbol="VIN"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VREG_SOT223" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;SOT-223 Fixed Voltage Regulators&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;&lt;/p&gt;
&lt;table width="700"&gt;
&lt;tr bgcolor="#EEEEEE" &gt;
&lt;td&gt;&lt;b&gt;Part&lt;/b&gt;&lt;/td&gt;
&lt;td&gt;&lt;b&gt;Current Out&lt;/b&gt;&lt;/td&gt;
&lt;td&gt;&lt;b&gt;V Out&lt;/b&gt;&lt;/td&gt;
&lt;td&gt;&lt;b&gt;V In&lt;/b&gt;&lt;/td&gt;
&lt;td&gt;&lt;b&gt;V Dropout&lt;/b&gt;&lt;/td&gt;
&lt;td&gt;&lt;b&gt;θJA (°C/W)&lt;/b&gt;&lt;/td&gt;
&lt;td&gt;&lt;b&gt;TJ (°C)&lt;/b&gt;&lt;/td&gt;
&lt;td&gt;&lt;b&gt;Operating Temp&lt;/b&gt;&lt;/td&gt;
&lt;td&gt;&lt;b&gt;Digikey Part No.&lt;/b&gt;&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;AP1117&lt;/td&gt;
  &lt;td&gt;1A&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;3.3V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;18V&lt;/td&gt;
  &lt;td&gt;1.1V@500mA, 1.3V@1A&lt;/td&gt;
  &lt;td&gt;107°C/W&lt;/td&gt;
  &lt;td&gt;150°C&lt;/td&gt;
  &lt;td&gt;-40°C-125°C&lt;/td&gt;
  &lt;td&gt;AP1117IE33G-13DICT-ND&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
&lt;/tr&gt;

&lt;/table&gt;
&lt;p&gt;Max operating temp can be calculated using θJA, TJ (max junction temperature), and power in watts.  Set the "Maximum Ambient Temperature" until it reaches TJ ("Max Junction Temperature"), which is the absolute limit for safe use of the regulator: &lt;a href="http://www.daycounter.com/Calculators/Heat-Sink-Temperature-Calculator.phtml"&gt;Heat Sink Temperature Calculator&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;For example, With 12V source into a 3.3V LP2985 and a 30mA load, we are dissipating (12V-3.3V) * 0.03A = 0.261W.  With a θJA of 206 °C/W, a TJ of 150°C, and 261mW we can safely use the chip without a heat sink up to 75°C (=147.1°C Junction Temperature).&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="VREG_SOT223_FIXED"/>
</gates>
<devices>
<device name="" package="SOT223-R">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2 4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-1X9" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD9"/>
</gates>
<devices>
<device name="" package="1X09_OVAL">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="76MIL" package="1X09_ROUND_76">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="70MIL" package="1X09_ROUND_70">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="antenna">
<packages>
<package name="DN007+5">
</package>
<package name="DN007+0">
</package>
<package name="DN007+1">
</package>
<package name="DN007+2">
</package>
<package name="DN007+3">
</package>
<package name="DN007+4">
</package>
<package name="DN007-1">
</package>
<package name="DN007-2">
</package>
<package name="DN007-3">
</package>
</packages>
<symbols>
<symbol name="INVERTED_F_ANTENNA">
<pin name="FEED"/>
<pin name="GND@1"/>
<pin name="GND"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="INVERTED_F_ANTENNA">
<description>&lt;b&gt;2.4GHz Inverted F Antenna&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
Based on TI Design Note DN007&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="INVERTED_F_ANTENNA"/>
</gates>
<devices>
<device name="+5" package="DN007+5">
<connects>
<connect gate="G$1" pin="FEED" pad="FEED"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="+0" package="DN007+0">
<connects>
<connect gate="G$1" pin="FEED" pad="FEED"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="+1" package="DN007+1">
<connects>
<connect gate="G$1" pin="FEED" pad="FEED"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="+2" package="DN007+2">
<connects>
<connect gate="G$1" pin="FEED" pad="FEED"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="+3" package="DN007+3">
<connects>
<connect gate="G$1" pin="FEED" pad="FEED"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="+4" package="DN007+4">
<connects>
<connect gate="G$1" pin="FEED" pad="FEED"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-1" package="DN007-1">
<connects>
<connect gate="G$1" pin="FEED" pad="FEED"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-2" package="DN007-2">
<connects>
<connect gate="G$1" pin="FEED" pad="FEED"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-3" package="DN007-3">
<connects>
<connect gate="G$1" pin="FEED" pad="FEED"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="fab">
<packages>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R1206W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="R1206FAB">
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1206FAB">
</package>
<package name="LED1206">
<description>LED 1206 pads (standard pattern)</description>
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="5MM">
<description>5mm round through hole part.</description>
</package>
</packages>
<symbols>
<symbol name="R-US">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="CAP-NONPOLARIZED">
<description>non-polarized capacitor</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="LED">
<description>LED</description>
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="RES-US" prefix="R" uservalue="yes">
<description>&lt;b&gt;Resistor (US Symbol)&lt;/b&gt;
&lt;p&gt;
Variants with postfix FAB are widened to allow the routing of internal traces</description>
<gates>
<gate name="G$1" symbol="R-US"/>
</gates>
<devices>
<device name="1206" package="R1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206W" package="R1206W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206FAB" package="R1206FAB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAP-UNPOLARIZED" prefix="C" uservalue="yes">
<gates>
<gate name="&gt;NAME" symbol="CAP-NONPOLARIZED"/>
</gates>
<devices>
<device name="" package="C1206">
<connects>
<connect gate="&gt;NAME" pin="1" pad="1"/>
<connect gate="&gt;NAME" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FAB" package="C1206FAB">
<connects>
<connect gate="&gt;NAME" pin="1" pad="1"/>
<connect gate="&gt;NAME" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED">
<description>LED</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="LED1206">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FAB1206" package="LED1206FAB">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5MM" package="5MM">
<connects>
<connect gate="G$1" pin="A" pad="IN"/>
<connect gate="G$1" pin="C" pad="OUT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<parts>
<part name="U2" library="microbuilder" deviceset="CC3000MOD" device="" value="CC3000MOD"/>
<part name="U$11" library="microbuilder" deviceset="GND" device=""/>
<part name="U$14" library="microbuilder" deviceset="GND" device=""/>
<part name="U$15" library="microbuilder" deviceset="GND" device=""/>
<part name="U$21" library="microbuilder" deviceset="GND" device=""/>
<part name="U$22" library="microbuilder" deviceset="GND" device=""/>
<part name="U$24" library="microbuilder" deviceset="GND" device=""/>
<part name="U$25" library="microbuilder" deviceset="VBAT" device=""/>
<part name="U$26" library="microbuilder" deviceset="GND" device=""/>
<part name="U$27" library="microbuilder" deviceset="GND" device=""/>
<part name="U$28" library="microbuilder" deviceset="GND" device=""/>
<part name="U$29" library="microbuilder" deviceset="GND" device=""/>
<part name="U$30" library="microbuilder" deviceset="GND" device=""/>
<part name="U$31" library="microbuilder" deviceset="GND" device=""/>
<part name="U$32" library="microbuilder" deviceset="GND" device=""/>
<part name="U$33" library="microbuilder" deviceset="GND" device=""/>
<part name="U$34" library="microbuilder" deviceset="VIN" device=""/>
<part name="U$35" library="microbuilder" deviceset="VBAT" device=""/>
<part name="U$36" library="microbuilder" deviceset="GND" device=""/>
<part name="U$37" library="microbuilder" deviceset="GND" device=""/>
<part name="U$38" library="microbuilder" deviceset="VIN" device=""/>
<part name="U3" library="microbuilder" deviceset="VREG_SOT223" device=""/>
<part name="U$39" library="microbuilder" deviceset="GND" device=""/>
<part name="U$40" library="microbuilder" deviceset="GND" device=""/>
<part name="U$41" library="microbuilder" deviceset="VBAT" device=""/>
<part name="U$44" library="microbuilder" deviceset="GND" device=""/>
<part name="U$45" library="microbuilder" deviceset="VBAT" device=""/>
<part name="U$46" library="microbuilder" deviceset="GND" device=""/>
<part name="JP3" library="microbuilder" deviceset="HEADER-1X9" device="70MIL"/>
<part name="U$50" library="microbuilder" deviceset="GND" device=""/>
<part name="U$51" library="microbuilder" deviceset="VBAT" device=""/>
<part name="JP2" library="microbuilder" deviceset="HEADER-1X3" device="ROUND"/>
<part name="U$47" library="antenna" deviceset="INVERTED_F_ANTENNA" device="-3"/>
<part name="U$48" library="microbuilder" deviceset="GND" device=""/>
<part name="R4" library="fab" deviceset="RES-US" device="1206FAB" value="470"/>
<part name="R5" library="fab" deviceset="RES-US" device="1206FAB" value="10k"/>
<part name="R6" library="fab" deviceset="RES-US" device="1206FAB" value="10k"/>
<part name="C1" library="fab" deviceset="CAP-UNPOLARIZED" device="FAB" value="1uf"/>
<part name="C3" library="fab" deviceset="CAP-UNPOLARIZED" device="FAB" value="1uf"/>
<part name="C4" library="fab" deviceset="CAP-UNPOLARIZED" device="FAB" value="10uf"/>
<part name="C5" library="fab" deviceset="CAP-UNPOLARIZED" device="FAB" value="10uf"/>
<part name="C12" library="fab" deviceset="CAP-UNPOLARIZED" device="FAB" value="10uf"/>
<part name="C6" library="fab" deviceset="CAP-UNPOLARIZED" device="FAB" value="10pf"/>
<part name="C7" library="fab" deviceset="CAP-UNPOLARIZED" device="FAB" value="10pf"/>
<part name="U$1" library="fab" deviceset="LED" device="FAB1206"/>
<part name="TP1" library="microbuilder" deviceset="TESTPOINT" device="PAD1MM" value="SDA"/>
<part name="TP2" library="microbuilder" deviceset="TESTPOINT" device="PAD1MM" value="SCL"/>
<part name="R1" library="fab" deviceset="RES-US" device="1206FAB" value="0k"/>
</parts>
<sheets>
<sheet>
<plain>
<text>Use internal 32K osc (EXT_32K to GND)</text>
<text>VIN = 5V</text>
<text>VBAT = 3.3V</text>
</plain>
<busses>
</busses>
<nets>
<net name="GND">
<segment>
<pinref part="U2" gate="G$1" pin="GND@14"/>
<pinref part="U$11" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="U2" gate="G$1" pin="GND@13"/>
<pinref part="U2" gate="G$1" pin="GND@10"/>
<pinref part="U2" gate="G$1" pin="GND@12"/>
<pinref part="U2" gate="G$1" pin="GND@11"/>
<pinref part="U$14" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="U2" gate="G$1" pin="GND@24"/>
<pinref part="U2" gate="G$1" pin="GND@19"/>
<pinref part="U2" gate="G$1" pin="GND@23"/>
<pinref part="U2" gate="G$1" pin="GND@22"/>
<pinref part="U2" gate="G$1" pin="GND@21"/>
<pinref part="U2" gate="G$1" pin="GND@20"/>
<pinref part="U$15" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="U2" gate="G$1" pin="GND@15"/>
<pinref part="U2" gate="G$1" pin="GND@18"/>
<pinref part="U2" gate="G$1" pin="GND@16"/>
<pinref part="U2" gate="G$1" pin="GND@17"/>
<pinref part="U$21" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="U$22" gate="G$1" pin="GND"/>
<pinref part="C3" gate="&gt;NAME" pin="1"/>
</segment>
<segment>
<pinref part="U$24" gate="G$1" pin="GND"/>
<pinref part="C1" gate="&gt;NAME" pin="1"/>
</segment>
<segment>
<pinref part="U2" gate="G$1" pin="GND@8"/>
<pinref part="U2" gate="G$1" pin="GND@7"/>
<pinref part="U2" gate="G$1" pin="EXT_32K"/>
<pinref part="U$26" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="U2" gate="G$1" pin="GND@9"/>
<pinref part="U$27" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="U2" gate="G$1" pin="GND@4"/>
<pinref part="U$30" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="U2" gate="G$1" pin="GND@5"/>
<pinref part="U$29" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="U2" gate="G$1" pin="GND@6"/>
<pinref part="U$28" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="U2" gate="G$1" pin="GND@3"/>
<pinref part="U$31" gate="G$1" pin="GND"/>
<pinref part="U2" gate="G$1" pin="GND@2"/>
</segment>
<segment>
<pinref part="U2" gate="G$1" pin="GND@1"/>
<pinref part="U$32" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="U$37" gate="G$1" pin="GND"/>
<pinref part="C12" gate="&gt;NAME" pin="1"/>
</segment>
<segment>
<pinref part="U$36" gate="G$1" pin="GND"/>
<pinref part="C4" gate="&gt;NAME" pin="1"/>
</segment>
<segment>
<pinref part="U$39" gate="G$1" pin="GND"/>
<pinref part="C5" gate="&gt;NAME" pin="1"/>
</segment>
<segment>
<pinref part="U3" gate="G$1" pin="GND"/>
<pinref part="U$40" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="U$33" gate="G$1" pin="GND"/>
<pinref part="JP3" gate="A" pin="9"/>
</segment>
<segment>
<pinref part="U$44" gate="G$1" pin="GND"/>
<pinref part="R5" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="U$46" gate="G$1" pin="GND"/>
<pinref part="JP2" gate="A" pin="1"/>
</segment>
<segment>
<pinref part="U$50" gate="G$1" pin="GND"/>
<pinref part="R4" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="U$48" gate="G$1" pin="GND"/>
<pinref part="U$47" gate="G$1" pin="GND"/>
<pinref part="U$47" gate="G$1" pin="GND@1"/>
</segment>
</net>
<net name="N$9">
<segment>
<pinref part="U2" gate="G$1" pin="RF_ANT"/>
<pinref part="C7" gate="&gt;NAME" pin="1"/>
</segment>
</net>
<net name="SCL_3V1">
<segment>
<pinref part="U2" gate="G$1" pin="SCL_CC3000"/>
<pinref part="U2" gate="G$1" pin="SCL_EEPROM"/>
<pinref part="TP2" gate="G$1" pin="P$1"/>
</segment>
</net>
<net name="SDA_3V1">
<segment>
<pinref part="U2" gate="G$1" pin="SDA_CC3000"/>
<pinref part="U2" gate="G$1" pin="SDA_EEPROM"/>
<pinref part="TP1" gate="G$1" pin="P$1"/>
</segment>
</net>
<net name="VBAT">
<segment>
<pinref part="U2" gate="G$1" pin="VBAT_IN"/>
<pinref part="U$25" gate="G$1" pin="VBAT"/>
<pinref part="U2" gate="G$1" pin="VIO_HOST"/>
<pinref part="C1" gate="&gt;NAME" pin="2"/>
<pinref part="C3" gate="&gt;NAME" pin="2"/>
</segment>
<segment>
<pinref part="U$35" gate="G$1" pin="VBAT"/>
<pinref part="U3" gate="G$1" pin="OUT"/>
<pinref part="C5" gate="&gt;NAME" pin="2"/>
<pinref part="C12" gate="&gt;NAME" pin="2"/>
</segment>
<segment>
<pinref part="U$41" gate="G$1" pin="VBAT"/>
<pinref part="JP3" gate="A" pin="8"/>
</segment>
<segment>
<pinref part="U$45" gate="G$1" pin="VBAT"/>
<pinref part="R6" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="U$51" gate="G$1" pin="VBAT"/>
<pinref part="U$1" gate="G$1" pin="A"/>
</segment>
</net>
<net name="VBAT_EN_3V">
<segment>
<pinref part="U2" gate="G$1" pin="VBAT_SW_EN"/>
</segment>
</net>
<net name="SPI_CLK_3V">
<segment>
<pinref part="U2" gate="G$1" pin="SPI_CLK"/>
<pinref part="JP3" gate="A" pin="6"/>
</segment>
</net>
<net name="SPI_MOSI_3V">
<segment>
<pinref part="U2" gate="G$1" pin="SPI_DIN"/>
<pinref part="JP3" gate="A" pin="4"/>
</segment>
</net>
<net name="SPI_IRQ_3V">
<segment>
<pinref part="U2" gate="G$1" pin="SPI_IRQ"/>
<pinref part="JP3" gate="A" pin="1"/>
</segment>
</net>
<net name="SPI_MISO_3V">
<segment>
<pinref part="U2" gate="G$1" pin="SPI_DOUT"/>
<pinref part="JP3" gate="A" pin="5"/>
</segment>
</net>
<net name="SPI_CS_3V">
<segment>
<pinref part="JP3" gate="A" pin="3"/>
<pinref part="R6" gate="G$1" pin="1"/>
<pinref part="R1" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$11">
<segment>
<pinref part="U2" gate="G$1" pin="WL_EN1"/>
<pinref part="U2" gate="G$1" pin="WL_EN2"/>
</segment>
</net>
<net name="RXD_3V">
<segment>
<pinref part="U2" gate="G$1" pin="WL_RS232_RX"/>
<pinref part="JP2" gate="A" pin="3"/>
</segment>
</net>
<net name="TXD_3V">
<segment>
<pinref part="U2" gate="G$1" pin="WL_RS232_TX"/>
<pinref part="JP2" gate="A" pin="2"/>
</segment>
</net>
<net name="VIN">
<segment>
<pinref part="U$38" gate="G$1" pin="VIN"/>
<pinref part="JP3" gate="A" pin="7"/>
</segment>
<segment>
<pinref part="U$34" gate="G$1" pin="VIN"/>
<pinref part="C4" gate="&gt;NAME" pin="2"/>
<pinref part="U3" gate="G$1" pin="IN"/>
</segment>
</net>
<net name="VBAT_EN_5V">
<segment>
<pinref part="JP3" gate="A" pin="2"/>
<pinref part="R5" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$13">
<segment>
<pinref part="R4" gate="G$1" pin="2"/>
<pinref part="U$1" gate="G$1" pin="C"/>
</segment>
</net>
<net name="N$14">
<segment>
<pinref part="U$47" gate="G$1" pin="FEED"/>
<pinref part="C6" gate="&gt;NAME" pin="1"/>
</segment>
</net>
<net name="N$15">
<segment>
<pinref part="C6" gate="&gt;NAME" pin="2"/>
<pinref part="C7" gate="&gt;NAME" pin="2"/>
</segment>
</net>
<net name="N$3">
<segment>
<pinref part="U2" gate="G$1" pin="SPI_CS"/>
<pinref part="R1" gate="G$1" pin="1"/>
</segment>
</net>
</nets>
</sheet>
</sheets>
</schematic>
</drawing>
</eagle>
