<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<board>
<plain>
<wire x1="-0.1016" y1="47.7522" x2="0" y2="-0.1016" width="0" layer="20"/>
<wire x1="0" y1="-0.1016" x2="49.3576" y2="-0.0508" width="0" layer="20"/>
<wire x1="49.3576" y1="-0.0508" x2="50.0688" y2="47.041" width="0" layer="20"/>
<wire x1="50.0688" y1="47.041" x2="-0.1016" y2="47.7522" width="0" layer="20"/>
<rectangle x1="2.0574" y1="1.397" x2="47.117" y2="45.3644" layer="20"/>
</plain>
<libraries>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-lstb">
<description>&lt;b&gt;Pin Headers&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
MA = male&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MA04-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="MA03-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="MA08-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="AVX_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/04/2012 16:26:10</description>
<packages>
<package name="CAPC3216X178N">
</package>
</packages>
</library>
<library name="01_SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
<package name="1X01">
</package>
</packages>
</library>
<library name="01_FAB_Hello">
<packages>
<package name="CSM-7X-DU">
<description>&lt;b&gt;SMD CRYSTAL&lt;/b&gt;&lt;p&gt;
Source: www.ecsxtal.com .. Crystal 3.6864MHz CSM_7X_DU.PDF</description>
</package>
</packages>
</library>
<library name="atmega8">
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="new">
<packages>
<package name="P-LCC-4-3">
<description>&lt;b&gt;Hyper TOPLED® &lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/</description>
</package>
</packages>
</library>
<library name="fab">
<packages>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ADC_1" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ADC_2" library="con-lstb" package="MA04-1" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="AVX_By_element14_Batch_1" package="CAPC3216X178N" value="22pF">
<attribute name="MPN" value="0612ZC225MAT2A"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="12N3209"/>
<attribute name="SUPPLIER" value="AVX"/>
<attribute name="TOLERANCE" value="±20%"/>
<attribute name="VALUE"/>
<attribute name="VOLTAGERATING" value="10V"/>
</element>
<element name="C2" library="AVX_By_element14_Batch_1" package="CAPC3216X178N" value="22pF">
<attribute name="MPN" value="0612ZC225MAT2A"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="12N3209"/>
<attribute name="SUPPLIER" value="AVX"/>
<attribute name="TOLERANCE" value="±20%"/>
<attribute name="VALUE"/>
<attribute name="VOLTAGERATING" value="10V"/>
</element>
<element name="C3" library="01_SparkFun" package="1206" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="01_SparkFun" package="1206" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="01_SparkFun" package="1206" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CRYSTAL" library="01_FAB_Hello" package="CSM-7X-DU" value="16Mhz">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="D13" library="01_SparkFun" package="1X01" value="M01PTH">
<attribute name="NAME"/>
</element>
<element name="DIGITAL1" library="con-lstb" package="MA03-1" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="DIGITAL_2" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MICRO" library="atmega8" package="TQFP32-08" value="ATMEGA328P-AU">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="POWER" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="01_SparkFun" package="1206" value="10k Ohm">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RST" library="01_SparkFun" package="1X01" value="M01PTH">
<attribute name="NAME"/>
</element>
<element name="DIGITAL_1" library="con-lstb" package="MA08-1" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="new" package="P-LCC-4-3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="fab" package="R1206" value="1k Ohm">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="fab" package="R1206" value="500 Ohm">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="fab" package="R1206" value="1k Ohm">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="fab" package="R1206" value="0 Ohm">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="MICRO" pad="4"/>
<contactref element="MICRO" pad="6"/>
<contactref element="MICRO" pad="18"/>
<contactref element="MICRO" pad="20"/>
<contactref element="R1" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="LED2" pad="A"/>
<contactref element="R5" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="POWER" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="C1" pad="2"/>
<contactref element="CRYSTAL" pad="1"/>
<contactref element="MICRO" pad="7"/>
</signal>
<signal name="GND">
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="MICRO" pad="3"/>
<contactref element="MICRO" pad="5"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="MICRO" pad="21"/>
<contactref element="POWER" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="2"/>
<contactref element="MICRO" pad="29"/>
<contactref element="RST" pad="1"/>
</signal>
<signal name="ADC3">
<contactref element="MICRO" pad="26"/>
<contactref element="ADC_2" pad="2"/>
</signal>
<signal name="ADC1">
<contactref element="MICRO" pad="24"/>
<contactref element="ADC_1" pad="1"/>
</signal>
<signal name="ADC4/SDA">
<contactref element="MICRO" pad="27"/>
<contactref element="ADC_2" pad="3"/>
</signal>
<signal name="ADC2">
<contactref element="MICRO" pad="25"/>
<contactref element="ADC_2" pad="1"/>
</signal>
<signal name="ADC0">
<contactref element="MICRO" pad="23"/>
<contactref element="ADC_1" pad="2"/>
</signal>
<signal name="D2">
<contactref element="MICRO" pad="32"/>
<contactref element="DIGITAL1" pad="3"/>
</signal>
<signal name="D4">
<contactref element="MICRO" pad="2"/>
<contactref element="DIGITAL_2" pad="2"/>
</signal>
<signal name="D3">
<contactref element="MICRO" pad="1"/>
<contactref element="DIGITAL_2" pad="1"/>
</signal>
<signal name="D5">
<contactref element="MICRO" pad="9"/>
<contactref element="DIGITAL_1" pad="1"/>
</signal>
<signal name="D6">
<contactref element="MICRO" pad="10"/>
<contactref element="DIGITAL_1" pad="2"/>
</signal>
<signal name="D7">
<contactref element="MICRO" pad="11"/>
<contactref element="DIGITAL_1" pad="3"/>
</signal>
<signal name="D9">
<contactref element="MICRO" pad="13"/>
</signal>
<signal name="D10">
<contactref element="MICRO" pad="14"/>
</signal>
<signal name="D11">
<contactref element="MICRO" pad="15"/>
</signal>
<signal name="D12">
<contactref element="MICRO" pad="16"/>
<contactref element="DIGITAL_1" pad="8"/>
</signal>
<signal name="D13">
<contactref element="MICRO" pad="17"/>
<contactref element="D13" pad="1"/>
</signal>
<signal name="D0/TX">
<contactref element="MICRO" pad="30"/>
<contactref element="DIGITAL1" pad="1"/>
</signal>
<signal name="D1/RX">
<contactref element="MICRO" pad="31"/>
<contactref element="DIGITAL1" pad="2"/>
</signal>
<signal name="ADC5/SCL">
<contactref element="MICRO" pad="28"/>
<contactref element="ADC_2" pad="4"/>
</signal>
<signal name="N$1">
<contactref element="C2" pad="2"/>
<contactref element="CRYSTAL" pad="2"/>
<contactref element="MICRO" pad="8"/>
</signal>
<signal name="D8">
<contactref element="MICRO" pad="12"/>
<contactref element="DIGITAL_1" pad="4"/>
</signal>
<signal name="N$4">
<contactref element="LED2" pad="R"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R2" pad="2"/>
<contactref element="DIGITAL_1" pad="7"/>
</signal>
<signal name="N$6">
<contactref element="LED2" pad="G"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="R4" pad="2"/>
<contactref element="DIGITAL_1" pad="6"/>
</signal>
<signal name="N$8">
<contactref element="LED2" pad="B"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="R3" pad="2"/>
<contactref element="DIGITAL_1" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
