<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<schematic>
<libraries>
<library name="fab">
<packages>
<package name="TQFP32-08THIN">
</package>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
<package name="1X06SMD">
</package>
<package name="2X03SMD">
</package>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="P-LCC-4">
<description>&lt;b&gt;Power TOPLED®&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LA_LO_LA_LY E67B.pdf</description>
</package>
<package name="P-LCC-4-FANCYFAB">
<description>&lt;b&gt;Power TOPLED®&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LA_LO_LA_LY E67B.pdf</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R1206W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="R1206FAB">
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1206FAB">
</package>
<package name="C2220">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="EFOBM">
</package>
</packages>
<symbols>
<symbol name="23-I/O">
<pin name="PB5(SCK)"/>
<pin name="PB7(XTAL2/TOSC2)"/>
<pin name="PB6(XTAL1/TOSC1)"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="AVCC" direction="pwr"/>
<pin name="PB4(MISO)"/>
<pin name="PB3(MOSI/OC2)"/>
<pin name="PB2(SS/OC1B)"/>
<pin name="PB1(OC1A)"/>
<pin name="PB0(ICP)"/>
<pin name="PD7(AIN1)"/>
<pin name="PD6(AIN0)"/>
<pin name="PD5(T1)"/>
<pin name="PD4(XCK/T0)"/>
<pin name="PD3(INT1)"/>
<pin name="PD2(INT0)"/>
<pin name="PD1(TXD)"/>
<pin name="PD0(RXD)"/>
<pin name="ADC7"/>
<pin name="ADC6"/>
<pin name="PC5(ADC5/SCL)"/>
<pin name="PC4(ADC4/SDA)"/>
<pin name="PC3(ADC3)"/>
<pin name="PC2(ADC2)"/>
<pin name="PC1(ADC1)"/>
<pin name="PC0(ADC0)"/>
<pin name="PC6(/RESET)" function="dot"/>
</symbol>
<symbol name="78ADJ">
<pin name="IN" direction="in"/>
<pin name="ADJ" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="OUT@1" direction="out"/>
</symbol>
<symbol name="FTDI">
<pin name="GND"/>
<pin name="CTS"/>
<pin name="VCC"/>
<pin name="TXD"/>
<pin name="RXD"/>
<pin name="RTS"/>
</symbol>
<symbol name="AVRISP">
<pin name="MISO" direction="pas" function="dot"/>
<pin name="VCC" direction="pas" function="dot"/>
<pin name="SCK" direction="pas" function="dot"/>
<pin name="MOSI" direction="pas" function="dot"/>
<pin name="RST" direction="pas" function="dot"/>
<pin name="GND" direction="pas" function="dot"/>
</symbol>
<symbol name="LED-RGB">
<pin name="CGREEN" direction="pas"/>
<pin name="CBLUE" direction="pas"/>
<pin name="CRED" direction="pas"/>
<pin name="A2" direction="pas"/>
</symbol>
<symbol name="R-US">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="CAP-NONPOLARIZED">
<description>non-polarized capacitor</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="CERAMIC_RESONATOR">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ATMEGA88-THIN" prefix="IC">
<gates>
<gate name="G$1" symbol="23-I/O"/>
</gates>
<devices>
<device name="" package="TQFP32-08THIN">
<connects>
<connect gate="G$1" pin="ADC6" pad="19"/>
<connect gate="G$1" pin="ADC7" pad="22"/>
<connect gate="G$1" pin="AREF" pad="20"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND" pad="21"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="PB0(ICP)" pad="12"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="13"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="14"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="15"/>
<connect gate="G$1" pin="PB4(MISO)" pad="16"/>
<connect gate="G$1" pin="PB5(SCK)" pad="17"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="7"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="8"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="29"/>
<connect gate="G$1" pin="PD0(RXD)" pad="30"/>
<connect gate="G$1" pin="PD1(TXD)" pad="31"/>
<connect gate="G$1" pin="PD2(INT0)" pad="32"/>
<connect gate="G$1" pin="PD3(INT1)" pad="1"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="2"/>
<connect gate="G$1" pin="PD5(T1)" pad="9"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="10"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="11"/>
<connect gate="G$1" pin="VCC@1" pad="4"/>
<connect gate="G$1" pin="VCC@2" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V_REG_LM1117" prefix="U" uservalue="yes">
<description>&lt;b&gt;Voltage Regulator LM1117&lt;/b&gt;
Standard adjustable voltage regulator but in SMD form. Spark Fun Electronics SKU : COM-00595</description>
<gates>
<gate name="G$1" symbol="78ADJ"/>
</gates>
<devices>
<device name="SOT223" package="SOT223">
<connects>
<connect gate="G$1" pin="ADJ" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2"/>
<connect gate="G$1" pin="OUT@1" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="VREG-08170"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FTDI-SMD-HEADER">
<gates>
<gate name="G$1" symbol="FTDI"/>
</gates>
<devices>
<device name="" package="1X06SMD">
<connects>
<connect gate="G$1" pin="CTS" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="RTS" pad="6"/>
<connect gate="G$1" pin="RXD" pad="5"/>
<connect gate="G$1" pin="TXD" pad="4"/>
<connect gate="G$1" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AVRISP">
<gates>
<gate name="G$1" symbol="AVRISP"/>
</gates>
<devices>
<device name="SMD" package="2X03SMD">
<connects>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="MISO" pad="1"/>
<connect gate="G$1" pin="MOSI" pad="4"/>
<connect gate="G$1" pin="RST" pad="5"/>
<connect gate="G$1" pin="SCK" pad="3"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="2X03">
<connects>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="MISO" pad="1"/>
<connect gate="G$1" pin="MOSI" pad="4"/>
<connect gate="G$1" pin="RST" pad="5"/>
<connect gate="G$1" pin="SCK" pad="3"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LEDRGBNEW" prefix="D">
<gates>
<gate name="G$1" symbol="LED-RGB"/>
</gates>
<devices>
<device name="" package="P-LCC-4">
<connects>
<connect gate="G$1" pin="A2" pad="A"/>
<connect gate="G$1" pin="CBLUE" pad="B"/>
<connect gate="G$1" pin="CGREEN" pad="G"/>
<connect gate="G$1" pin="CRED" pad="R"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FANCYFAB" package="P-LCC-4-FANCYFAB">
<connects>
<connect gate="G$1" pin="A2" pad="A"/>
<connect gate="G$1" pin="CBLUE" pad="B"/>
<connect gate="G$1" pin="CGREEN" pad="G"/>
<connect gate="G$1" pin="CRED" pad="R"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RES-US" prefix="R" uservalue="yes">
<description>&lt;b&gt;Resistor (US Symbol)&lt;/b&gt;
&lt;p&gt;
Variants with postfix FAB are widened to allow the routing of internal traces</description>
<gates>
<gate name="G$1" symbol="R-US"/>
</gates>
<devices>
<device name="1206" package="R1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206W" package="R1206W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206FAB" package="R1206FAB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAP-UNPOLARIZED" prefix="C" uservalue="yes">
<gates>
<gate name="&gt;NAME" symbol="CAP-NONPOLARIZED"/>
</gates>
<devices>
<device name="" package="C1206">
<connects>
<connect gate="&gt;NAME" pin="1" pad="1"/>
<connect gate="&gt;NAME" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FAB" package="C1206FAB">
<connects>
<connect gate="&gt;NAME" pin="1" pad="1"/>
<connect gate="&gt;NAME" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2220" package="C2220">
<connects>
<connect gate="&gt;NAME" pin="1" pad="1"/>
<connect gate="&gt;NAME" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RESONATOR">
<gates>
<gate name="G$1" symbol="CERAMIC_RESONATOR"/>
</gates>
<devices>
<device name="" package="EFOBM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="supply1">
<description>&lt;b&gt;Supply Symbols&lt;/b&gt;&lt;p&gt;
 GND, VCC, 0V, +5V, -5V, etc.&lt;p&gt;
 Please keep in mind, that these devices are necessary for the
 automatic wiring of the supply signals.&lt;p&gt;
 The pin name defined in the symbol is identical to the net which is to be wired automatically.&lt;p&gt;
 In this library the device names are the same as the pin names of the symbols, therefore the correct signal names appear next to the supply symbols in the schematic.&lt;p&gt;
 &lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
</packages>
<symbols>
<symbol name="VCC">
<pin name="VCC" direction="sup"/>
</symbol>
<symbol name="GND">
<pin name="GND" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="VCC" prefix="P+">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="VCC" symbol="VCC"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GND" prefix="GND">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="GND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X04/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X01">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="PINH2X4">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD1">
<pin name="1" direction="pas" function="dot"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="PINHD-2X4" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X4"/>
</gates>
<devices>
<device name="" package="2X04">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="2X04/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X1" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PINHD1"/>
</gates>
<devices>
<device name="" package="1X01">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="con-lstb">
<description>&lt;b&gt;Pin Headers&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
MA = male&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MA03-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="MA03-1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="MA03-1" prefix="SV" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MA03-1"/>
</gates>
<devices>
<device name="" package="MA03-1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<parts>
<part name="IC1" library="fab" deviceset="ATMEGA88-THIN" device=""/>
<part name="U1" library="fab" deviceset="V_REG_LM1117" device="SOT223"/>
<part name="U$1" library="fab" deviceset="FTDI-SMD-HEADER" device=""/>
<part name="U$2" library="fab" deviceset="AVRISP" device="SMD"/>
<part name="D1" library="fab" deviceset="LEDRGBNEW" device=""/>
<part name="R1" library="fab" deviceset="RES-US" device="1206FAB" value="220oh"/>
<part name="R2" library="fab" deviceset="RES-US" device="1206FAB" value="220oh"/>
<part name="R3" library="fab" deviceset="RES-US" device="1206FAB" value="220oh"/>
<part name="P+1" library="supply1" deviceset="VCC" device=""/>
<part name="GND1" library="supply1" deviceset="GND" device=""/>
<part name="GND2" library="supply1" deviceset="GND" device=""/>
<part name="C1" library="fab" deviceset="CAP-UNPOLARIZED" device="FAB" value="1uf"/>
<part name="R4" library="fab" deviceset="RES-US" device="1206FAB" value="10k"/>
<part name="P+2" library="supply1" deviceset="VCC" device=""/>
<part name="GND3" library="supply1" deviceset="GND" device=""/>
<part name="JP1" library="pinhead" deviceset="PINHD-2X4" device=""/>
<part name="U$3" library="fab" deviceset="RESONATOR" device=""/>
<part name="GND4" library="supply1" deviceset="GND" device=""/>
<part name="JP2" library="pinhead" deviceset="PINHD-1X1" device=""/>
<part name="JP3" library="pinhead" deviceset="PINHD-1X1" device=""/>
<part name="SV1" library="con-lstb" deviceset="MA03-1" device=""/>
</parts>
<sheets>
<sheet>
<plain>
</plain>
<busses>
</busses>
<nets>
<net name="MOSI">
<segment>
<pinref part="U$2" gate="G$1" pin="MOSI"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PB3(MOSI/OC2)"/>
</segment>
</net>
<net name="SCK">
<segment>
<pinref part="U$2" gate="G$1" pin="SCK"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PB5(SCK)"/>
</segment>
</net>
<net name="GND">
<segment>
<pinref part="U$1" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="U$2" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="U1" gate="G$1" pin="ADJ"/>
<pinref part="GND1" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="GND"/>
<pinref part="IC1" gate="G$1" pin="GND@1"/>
<pinref part="IC1" gate="G$1" pin="GND@2"/>
<pinref part="GND2" gate="1" pin="GND"/>
<pinref part="C1" gate="&gt;NAME" pin="1"/>
</segment>
<segment>
<pinref part="GND3" gate="1" pin="GND"/>
<pinref part="JP3" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="JP1" gate="A" pin="7"/>
</segment>
<segment>
<pinref part="U$3" gate="G$1" pin="2"/>
<pinref part="GND4" gate="1" pin="GND"/>
</segment>
</net>
<net name="N$10">
<segment>
<pinref part="U$1" gate="G$1" pin="TXD"/>
<pinref part="IC1" gate="G$1" pin="PD0(RXD)"/>
</segment>
</net>
<net name="N$11">
<segment>
<pinref part="IC1" gate="G$1" pin="PD1(TXD)"/>
<pinref part="U$1" gate="G$1" pin="RXD"/>
</segment>
</net>
<net name="RST">
<segment>
<pinref part="U$1" gate="G$1" pin="RTS"/>
</segment>
<segment>
<pinref part="U$2" gate="G$1" pin="RST"/>
</segment>
<segment>
<pinref part="R4" gate="G$1" pin="1"/>
<pinref part="IC1" gate="G$1" pin="PC6(/RESET)"/>
</segment>
</net>
<net name="N$13">
<segment>
<pinref part="R1" gate="G$1" pin="2"/>
<pinref part="D1" gate="G$1" pin="CRED"/>
</segment>
</net>
<net name="N$14">
<segment>
<pinref part="D1" gate="G$1" pin="CBLUE"/>
<pinref part="R2" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$15">
<segment>
<pinref part="D1" gate="G$1" pin="CGREEN"/>
<pinref part="R3" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$16">
<segment>
<pinref part="R1" gate="G$1" pin="1"/>
<pinref part="IC1" gate="G$1" pin="PB0(ICP)"/>
</segment>
</net>
<net name="N$17">
<segment>
<pinref part="R2" gate="G$1" pin="1"/>
<pinref part="IC1" gate="G$1" pin="PB1(OC1A)"/>
</segment>
</net>
<net name="N$18">
<segment>
<pinref part="R3" gate="G$1" pin="1"/>
<pinref part="IC1" gate="G$1" pin="PB2(SS/OC1B)"/>
</segment>
</net>
<net name="VCC">
<segment>
<pinref part="D1" gate="G$1" pin="A2"/>
<pinref part="P+1" gate="VCC" pin="VCC"/>
</segment>
<segment>
<pinref part="U$1" gate="G$1" pin="VCC"/>
</segment>
<segment>
<pinref part="U$2" gate="G$1" pin="VCC"/>
</segment>
<segment>
<pinref part="R4" gate="G$1" pin="2"/>
<pinref part="P+2" gate="VCC" pin="VCC"/>
</segment>
<segment>
<pinref part="JP1" gate="A" pin="2"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="VCC@2"/>
<pinref part="U1" gate="G$1" pin="OUT@1"/>
<pinref part="C1" gate="&gt;NAME" pin="2"/>
<pinref part="IC1" gate="G$1" pin="VCC@1"/>
<pinref part="U1" gate="G$1" pin="OUT"/>
</segment>
</net>
<net name="MISO">
<segment>
<pinref part="U$2" gate="G$1" pin="MISO"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PB4(MISO)"/>
</segment>
</net>
<net name="PANELSOLAR">
<segment>
<pinref part="U1" gate="G$1" pin="IN"/>
<pinref part="JP2" gate="G$1" pin="1"/>
</segment>
</net>
<net name="RX">
<segment>
<pinref part="JP1" gate="A" pin="1"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PD6(AIN0)"/>
</segment>
</net>
<net name="TX">
<segment>
<pinref part="JP1" gate="A" pin="8"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PD7(AIN1)"/>
</segment>
</net>
<net name="PB6">
<segment>
<pinref part="IC1" gate="G$1" pin="PB6(XTAL1/TOSC1)"/>
</segment>
<segment>
<pinref part="U$3" gate="G$1" pin="1"/>
</segment>
</net>
<net name="PB7">
<segment>
<pinref part="IC1" gate="G$1" pin="PB7(XTAL2/TOSC2)"/>
</segment>
<segment>
<pinref part="U$3" gate="G$1" pin="3"/>
</segment>
</net>
<net name="N$1">
<segment>
<pinref part="IC1" gate="G$1" pin="PD2(INT0)"/>
<pinref part="SV1" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$2">
<segment>
<pinref part="IC1" gate="G$1" pin="PD3(INT1)"/>
<pinref part="SV1" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$3">
<segment>
<pinref part="IC1" gate="G$1" pin="PD4(XCK/T0)"/>
<pinref part="SV1" gate="G$1" pin="3"/>
</segment>
</net>
</nets>
</sheet>
</sheets>
</schematic>
</drawing>
</eagle>
