<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<board>
<plain>
<wire x1="21.59" y1="15.24" x2="41.89" y2="15.24" width="0" layer="20"/>
<wire x1="41.89" y1="15.24" x2="41.89" y2="32.69" width="0" layer="20"/>
<wire x1="41.89" y1="32.69" x2="21.59" y2="32.69" width="0" layer="20"/>
<wire x1="21.59" y1="32.69" x2="21.59" y2="15.24" width="0" layer="20"/>
</plain>
<libraries>
<library name="fab_new">
<packages>
<package name="C1206FAB">
</package>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
<package name="1X06SMD">
</package>
</packages>
</library>
<library name="eagle_fab">
<packages>
<package name="SPDTSWITCH">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="fab_new" package="C1206FAB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$4" library="fab_new" package="SOIC8" value="UC_ATTINY412SI">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$5" library="fab_new" package="1X06SMD" value="CONN_06_FTDI-SMD-HEADER">
<attribute name="NAME"/>
</element>
<element name="U$1" library="eagle_fab" package="SPDTSWITCH" value="SPDTSWITCH">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="U$4" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="U$5" pad="3"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="U$4" pad="8"/>
<contactref element="U$5" pad="1"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="UPDI">
<contactref element="U$4" pad="6"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="SIGNAL">
<contactref element="U$4" pad="7"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="RXD">
<contactref element="U$4" pad="3"/>
<contactref element="U$5" pad="5"/>
</signal>
<signal name="TXD">
<contactref element="U$4" pad="2"/>
<contactref element="U$5" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
