Static Call Graph - [ejer3\ejer3.axf]

# Static Call Graph for image ejer3\ejer3.axf

#<CALLGRAPH># ARM Linker, 5060528: Last Updated: Sun Mar 18 19:49:36 2018

### Maximum Stack Usage = 192 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ SystemClock_Config ⇒ HAL_RCC_ClockConfig ⇒ HAL_RCC_GetSysClockFreq ⇒ __aeabi_uldivmod

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- SVC_Handler ⇒ SVC_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- PendSV_Handler ⇒ PendSV_Handler
- ADC_IRQHandler ⇒ ADC_IRQHandler

  ### Function Pointers

  - ADC_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - BusFault_Handler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA1_Stream0_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA1_Stream1_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA1_Stream2_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA1_Stream3_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA1_Stream4_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA1_Stream5_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA1_Stream6_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA1_Stream7_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA2_Stream0_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA2_Stream1_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA2_Stream2_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA2_Stream3_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA2_Stream4_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA2_Stream5_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA2_Stream6_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA2_Stream7_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DebugMon_Handler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - FLASH_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - FPU_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - HardFault_Handler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - I2C3_ER_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - I2C3_EV_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - MemManage_Handler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - NMI_Handler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - OTG_FS_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - OTG_FS_WKUP_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - PVD_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - PendSV_Handler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - RCC_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - RTC_Alarm_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - RTC_WKUP_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - Reset_Handler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - SDIO_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - SPI1_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - SPI2_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - SPI3_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - SPI4_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - SVC_Handler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - SysTick_Handler from stm32f4xx_it.o(i.SysTick_Handler) referenced from startup_stm32f401xe.o(RESET)
  - SystemInit from system_stm32f4xx.o(i.SystemInit) referenced from startup_stm32f401xe.o(.text)
  - TAMP_STAMP_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - TIM1_BRK_TIM9_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - TIM1_TRG_COM_TIM11_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - TIM1_UP_TIM10_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - TIM2_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - TIM3_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - TIM4_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - TIM5_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - USART1_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - USART2_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - USART6_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - UsageFault_Handler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - WWDG_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f401xe.o(.text)
  - main from main.o(i.main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_stm32f401xe.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f401xe.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f401xe.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f401xe.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f401xe.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - startup_stm32f401xe.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - startup_stm32f401xe.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup_stm32f401xe.o(RESET)

  ADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Calls]

  - >> ADC_IRQHandler
  [Called By]
  - >> ADC_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f401xe.o(RESET)

  DMA1_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA1_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA1_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA1_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA1_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA1_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA1_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA1_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA2_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA2_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA2_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA2_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA2_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA2_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA2_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA2_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  FPU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  I2C3_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  I2C3_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  OTG_FS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  OTG_FS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  RTC_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  SPI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  TAMP_STAMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  TIM1_BRK_TIM9_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  TIM1_TRG_COM_TIM11_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  TIM1_UP_TIM10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  USART6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  __aeabi_uldivmod (Thumb, 98 bytes, Stack size 40 bytes, uldiv.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = __aeabi_uldivmod
  [Calls]
  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> HAL_RCC_GetSysClockFreq

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text))
  [Called By]

  - >> __aeabi_uldivmod

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text))
  [Called By]

  - >> __aeabi_uldivmod

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  HAL_GPIO_Init (Thumb, 358 bytes, Stack size 40 bytes, stm32f4xx_hal_gpio.o(i.HAL_GPIO_Init))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_GPIO_Init
  [Called By]
  - >> main
  - >> MX_GPIO_Init
  - >> HAL_UART_MspInit

  HAL_GPIO_TogglePin (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_hal_gpio.o(i.HAL_GPIO_TogglePin))
  [Called By]

  - >> main

  HAL_GPIO_WritePin (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_hal_gpio.o(i.HAL_GPIO_WritePin))
  [Called By]

  - >> MX_GPIO_Init

  HAL_GetTick (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_hal.o(i.HAL_GetTick))
  [Called By]

  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_ClockConfig

  HAL_IncTick (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_hal.o(i.HAL_IncTick))
  [Called By]

  - >> SysTick_Handler

  HAL_Init (Thumb, 48 bytes, Stack size 8 bytes, stm32f4xx_hal.o(i.HAL_Init))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_Init ⇒ HAL_InitTick ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_InitTick
  - >> HAL_NVIC_SetPriorityGrouping
  - >> HAL_MspInit
  [Called By]
  - >> main

  HAL_InitTick (Thumb, 54 bytes, Stack size 16 bytes, stm32f4xx_hal.o(i.HAL_InitTick))
  [Stack]

  - Max Depth = 32
  - Call Chain = HAL_InitTick ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_SYSTICK_Config
  - >> HAL_NVIC_SetPriority
  [Called By]
  - >> HAL_RCC_ClockConfig
  - >> HAL_Init

  HAL_MspInit (Thumb, 88 bytes, Stack size 8 bytes, stm32f4xx_hal_msp.o(i.HAL_MspInit))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_MspInit ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_NVIC_SetPriorityGrouping
  - >> HAL_NVIC_SetPriority
  [Called By]
  - >> HAL_Init

  HAL_NVIC_SetPriority (Thumb, 60 bytes, Stack size 16 bytes, stm32f4xx_hal_cortex.o(i.HAL_NVIC_SetPriority))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_NVIC_SetPriority
  [Calls]
  - >> NVIC_SetPriority
  [Called By]
  - >> HAL_InitTick
  - >> SystemClock_Config
  - >> HAL_MspInit

  HAL_NVIC_SetPriorityGrouping (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_hal_cortex.o(i.HAL_NVIC_SetPriorityGrouping))
  [Called By]

  - >> HAL_Init
  - >> HAL_MspInit

  HAL_RCC_ClockConfig (Thumb, 286 bytes, Stack size 32 bytes, stm32f4xx_hal_rcc.o(i.HAL_RCC_ClockConfig))
  [Stack]

  - Max Depth = 80
  - Call Chain = HAL_RCC_ClockConfig ⇒ HAL_RCC_GetSysClockFreq ⇒ __aeabi_uldivmod
  [Calls]
  - >> HAL_InitTick
  - >> HAL_GetTick
  - >> HAL_RCC_GetSysClockFreq
  [Called By]
  - >> SystemClock_Config

  HAL_RCC_GetHCLKFreq (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_hal_rcc.o(i.HAL_RCC_GetHCLKFreq))
  [Called By]

  - >> SystemClock_Config

  HAL_RCC_GetPCLK1Freq (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_hal_rcc.o(i.HAL_RCC_GetPCLK1Freq))
  [Called By]

  - >> UART_SetConfig

  HAL_RCC_GetPCLK2Freq (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_hal_rcc.o(i.HAL_RCC_GetPCLK2Freq))
  [Called By]

  - >> UART_SetConfig

  HAL_RCC_GetSysClockFreq (Thumb, 88 bytes, Stack size 8 bytes, stm32f4xx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq))
  [Stack]

  - Max Depth = 48
  - Call Chain = HAL_RCC_GetSysClockFreq ⇒ __aeabi_uldivmod
  [Calls]
  - >> __aeabi_uldivmod
  [Called By]
  - >> HAL_RCC_ClockConfig

  HAL_RCC_OscConfig (Thumb, 770 bytes, Stack size 40 bytes, stm32f4xx_hal_rcc.o(i.HAL_RCC_OscConfig))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_RCC_OscConfig
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config

  HAL_SYSTICK_CLKSourceConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_hal_cortex.o(i.HAL_SYSTICK_CLKSourceConfig))
  [Called By]

  - >> SystemClock_Config

  HAL_SYSTICK_Callback (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_hal_cortex.o(i.HAL_SYSTICK_Callback))
  [Called By]

  - >> HAL_SYSTICK_IRQHandler

  HAL_SYSTICK_Config (Thumb, 40 bytes, Stack size 8 bytes, stm32f4xx_hal_cortex.o(i.HAL_SYSTICK_Config))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_SYSTICK_Config
  [Calls]
  - >> NVIC_SetPriority
  [Called By]
  - >> HAL_InitTick
  - >> SystemClock_Config

  HAL_SYSTICK_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, stm32f4xx_hal_cortex.o(i.HAL_SYSTICK_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_SYSTICK_IRQHandler
  [Calls]
  - >> HAL_SYSTICK_Callback
  [Called By]
  - >> SysTick_Handler

  HAL_UART_Init (Thumb, 98 bytes, Stack size 16 bytes, stm32f4xx_hal_uart.o(i.HAL_UART_Init))
  [Stack]

  - Max Depth = 88
  - Call Chain = HAL_UART_Init ⇒ HAL_UART_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_UART_MspInit
  - >> UART_SetConfig
  [Called By]
  - >> main

  HAL_UART_MspInit (Thumb, 60 bytes, Stack size 32 bytes, stm32f4xx_hal_msp.o(i.HAL_UART_MspInit))
  [Stack]

  - Max Depth = 72
  - Call Chain = HAL_UART_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  [Called By]
  - >> HAL_UART_Init

  SysTick_Handler (Thumb, 14 bytes, Stack size 8 bytes, stm32f4xx_it.o(i.SysTick_Handler))
  [Stack]

  - Max Depth = 16
  - Call Chain = SysTick_Handler ⇒ HAL_SYSTICK_IRQHandler
  [Calls]
  - >> HAL_SYSTICK_IRQHandler
  - >> HAL_IncTick
  [Address Reference Count : 1]
  - startup_stm32f401xe.o(RESET)

  SystemClock_Config (Thumb, 152 bytes, Stack size 88 bytes, main.o(i.SystemClock_Config))
  [Stack]

  - Max Depth = 168
  - Call Chain = SystemClock_Config ⇒ HAL_RCC_ClockConfig ⇒ HAL_RCC_GetSysClockFreq ⇒ __aeabi_uldivmod
  [Calls]
  - >> HAL_SYSTICK_Config
  - >> HAL_SYSTICK_CLKSourceConfig
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_GetHCLKFreq
  - >> HAL_RCC_ClockConfig
  - >> HAL_NVIC_SetPriority
  [Called By]
  - >> main

  SystemInit (Thumb, 66 bytes, Stack size 0 bytes, system_stm32f4xx.o(i.SystemInit))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(.text)

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  main (Thumb, 84 bytes, Stack size 24 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 192
  - Call Chain = main ⇒ SystemClock_Config ⇒ HAL_RCC_ClockConfig ⇒ HAL_RCC_GetSysClockFreq ⇒ __aeabi_uldivmod
  [Calls]
  - >> HAL_UART_Init
  - >> HAL_Init
  - >> HAL_GPIO_TogglePin
  - >> SystemClock_Config
  - >> MX_GPIO_Init
  - >> HAL_GPIO_Init
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  ### Local Symbols

  MX_GPIO_Init (Thumb, 130 bytes, Stack size 40 bytes, main.o(i.MX_GPIO_Init))
  [Stack]

  - Max Depth = 80
  - Call Chain = MX_GPIO_Init ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> HAL_GPIO_Init
  [Called By]
  - >> main

  NVIC_SetPriority (Thumb, 32 bytes, Stack size 0 bytes, stm32f4xx_hal_cortex.o(i.NVIC_SetPriority))
  [Called By]

  - >> HAL_SYSTICK_Config
  - >> HAL_NVIC_SetPriority

  UART_SetConfig (Thumb, 676 bytes, Stack size 24 bytes, stm32f4xx_hal_uart.o(i.UART_SetConfig))
  [Stack]

  - Max Depth = 24
  - Call Chain = UART_SetConfig
  [Calls]
  - >> HAL_RCC_GetPCLK1Freq
  - >> HAL_RCC_GetPCLK2Freq
  [Called By]
  - >> HAL_UART_Init

  ### Undefined Global Symbols