<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="43.688" y1="33.7312" x2="108.184" y2="33.6296" width="0" layer="20"/>
<wire x1="108.184" y1="33.6296" x2="108.0824" y2="73.1776" width="0" layer="20"/>
<wire x1="108.0824" y1="73.1776" x2="43.688" y2="73.076" width="0" layer="20"/>
<wire x1="43.688" y1="73.076" x2="43.688" y2="33.7312" width="0" layer="20"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="FAB_Hello">
<packages>
<package name="1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="con-amp-quick">
<description>&lt;b&gt;AMP Connectors, Type QUICK&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="03P">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
<package name="06P">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
<package name="04P">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="ESP8266-12E_ESP-12E">
<packages>
<package name="XCVR_ESP8266-12E/ESP-12E">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="PROG" library="fab" package="6MM_SWITCH" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="FAB_Hello" package="1206" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="FAB_Hello" package="1206" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="FAB_Hello" package="1206" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="FAB_Hello" package="1206" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="REGULATOR" library="con-amp-quick" package="03P" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="12"/>
<attribute name="VALUE"/>
</element>
<element name="RST" library="fab" package="6MM_SWITCH" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SL1" library="con-amp-quick" package="06P" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="5"/>
<attribute name="VALUE"/>
</element>
<element name="SL2" library="con-amp-quick" package="06P" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="5"/>
<attribute name="VALUE"/>
</element>
<element name="SL3" library="con-amp-quick" package="03P" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="12"/>
<attribute name="VALUE"/>
</element>
<element name="SL4" library="con-amp-quick" package="04P" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="19"/>
<attribute name="VALUE"/>
</element>
<element name="U4" library="ESP8266-12E_ESP-12E" package="XCVR_ESP8266-12E/ESP-12E" value="ESP8266-12E/ESP-12E">
<attribute name="AVAILABILITY" value="No availability data"/>
<attribute name="DESCRIPTION" value=" This WiFi module has a 32-bit MCU micro and clock speeds supporting 80 MHz or 160 MHz. Supports the RTOS and integrated Wi-Fi MAC/BB/RF/PA/LNA, and has an on-board antenna. "/>
<attribute name="MF" value="AI-Thinker"/>
<attribute name="MP" value="ESP8266-12E/ESP-12E"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="FAB_Hello" package="1206" value="499">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="FAB_Hello" package="1206" value="GREEN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="FAB_Hello" package="1206" value="10UF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="FAB_Hello" package="1206" value="10UF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U4" pad="15"/>
<contactref element="R7" pad="1"/>
<contactref element="PROG" pad="2"/>
<contactref element="RST" pad="1"/>
<contactref element="RST" pad="2"/>
<contactref element="SL1" pad="1"/>
<contactref element="REGULATOR" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="U4" pad="8"/>
<contactref element="R12" pad="2"/>
<contactref element="R11" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="REGULATOR" pad="2"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="TX">
<contactref element="U4" pad="22"/>
<contactref element="SL1" pad="4"/>
</signal>
<signal name="IO15">
<contactref element="U4" pad="16"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="RST">
<contactref element="U4" pad="1"/>
<contactref element="RST" pad="4"/>
<contactref element="RST" pad="3"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="CH_PD">
<contactref element="U4" pad="3"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="RX">
<contactref element="U4" pad="21"/>
<contactref element="SL1" pad="5"/>
</signal>
<signal name="IO0">
<contactref element="U4" pad="18"/>
<contactref element="PROG" pad="3"/>
<contactref element="PROG" pad="4"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="IO4">
<contactref element="U4" pad="19"/>
<contactref element="SL3" pad="2"/>
</signal>
<signal name="IO5">
<contactref element="U4" pad="20"/>
<contactref element="SL3" pad="1"/>
</signal>
<signal name="5V">
<contactref element="SL1" pad="3"/>
<contactref element="REGULATOR" pad="3"/>
<contactref element="LED1" pad="1"/>
<contactref element="C9" pad="2"/>
</signal>
<signal name="IO14">
<contactref element="U4" pad="5"/>
<contactref element="SL4" pad="2"/>
</signal>
<signal name="IO13">
<contactref element="U4" pad="7"/>
<contactref element="SL4" pad="4"/>
</signal>
<signal name="IO12">
<contactref element="U4" pad="6"/>
<contactref element="SL4" pad="3"/>
</signal>
<signal name="N$11">
<contactref element="U4" pad="2"/>
</signal>
<signal name="IO16">
<contactref element="U4" pad="4"/>
<contactref element="SL4" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="U4" pad="14"/>
<contactref element="SL2" pad="1"/>
</signal>
<signal name="CS0">
<contactref element="U4" pad="9"/>
<contactref element="SL2" pad="6"/>
</signal>
<signal name="MOSI">
<contactref element="U4" pad="13"/>
<contactref element="SL2" pad="2"/>
</signal>
<signal name="MISO">
<contactref element="U4" pad="10"/>
<contactref element="SL2" pad="5"/>
</signal>
<signal name="IO10">
<contactref element="U4" pad="12"/>
<contactref element="SL2" pad="3"/>
</signal>
<signal name="IO9">
<contactref element="U4" pad="11"/>
<contactref element="SL2" pad="4"/>
</signal>
<signal name="IO2">
<contactref element="U4" pad="17"/>
<contactref element="SL3" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="R2" pad="2"/>
<contactref element="LED1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
