<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="100" y2="0" width="0" layer="20"/>
<wire x1="100" y1="0" x2="100" y2="80" width="0" layer="20"/>
<wire x1="100" y1="80" x2="0" y2="80" width="0" layer="20"/>
<wire x1="0" y1="80" x2="0" y2="0" width="0" layer="20"/>
<text>Hanis board</text>
<wire x1="53.34" y1="71.12" x2="73.66" y2="71.12" width="0.4064" layer="20"/>
<wire x1="73.66" y1="71.12" x2="83.82" y2="63.5" width="0.4064" layer="20"/>
<wire x1="83.82" y1="63.5" x2="86.36" y2="46.99" width="0.4064" layer="20"/>
<wire x1="86.36" y1="46.99" x2="76.2" y2="31.75" width="0.4064" layer="20"/>
<wire x1="76.2" y1="31.75" x2="53.34" y2="31.75" width="0.4064" layer="20"/>
<wire x1="53.34" y1="31.75" x2="48.26" y2="36.83" width="0.4064" layer="20"/>
<wire x1="48.26" y1="36.83" x2="48.26" y2="66.04" width="0.4064" layer="20"/>
<wire x1="48.26" y1="66.04" x2="53.34" y2="71.12" width="0.4064" layer="20"/>
</plain>
<libraries>
<library name="eagle_fab">
<packages>
<package name="C1206FAB">
</package>
<package name="SOIC14">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="R1206FAB">
</package>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="EFOBM">
</package>
<package name="2X03SMD">
</package>
<package name="1X06SMD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="eagle_fab" package="C1206FAB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="eagle_fab" package="SOIC14" value="UC_ATTINY44-SSU">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="eagle_fab" package="R1206FAB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="eagle_fab" package="R1206FAB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="eagle_fab" package="R1206FAB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="eagle_fab" package="6MM_SWITCH" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="eagle_fab" package="LED1206FAB" value="LEDFAB1206">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="eagle_fab" package="EFOBM" value="XTAL_RESONATOR"/>
<element name="U$3" library="eagle_fab" package="2X03SMD" value="CONN_03X2_AVRISPSMD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$4" library="eagle_fab" package="1X06SMD" value="CONN_06_FTDI-SMD-HEADER">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="R1" pad="1"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="1"/>
<contactref element="U$3" pad="2"/>
<contactref element="U$4" pad="3"/>
<contactref element="R3" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="14"/>
<contactref element="U$3" pad="6"/>
<contactref element="U$4" pad="1"/>
<contactref element="U$2" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="S1" pad="2"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U$3" pad="1"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="N$2">
<contactref element="U$3" pad="4"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="N$5">
<contactref element="U$4" pad="4"/>
<contactref element="IC1" pad="13"/>
</signal>
<signal name="N$4">
<contactref element="U$4" pad="5"/>
<contactref element="IC1" pad="12"/>
</signal>
<signal name="N$6">
<contactref element="U$3" pad="3"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="N$9">
<contactref element="U$2" pad="1"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="U$2" pad="3"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="N$13">
<contactref element="R2" pad="1"/>
<contactref element="U$3" pad="5"/>
<contactref element="IC1" pad="4"/>
</signal>
<signal name="N$7">
<contactref element="R1" pad="2"/>
<contactref element="IC1" pad="11"/>
</signal>
<signal name="N$8">
<contactref element="R3" pad="2"/>
<contactref element="S1" pad="4"/>
<contactref element="IC1" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
