<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.0">
<drawing>
<board>
<plain>
<wire x1="55.88" y1="25.4" x2="118.09" y2="25.4" width="0" layer="20"/>
<wire x1="118.09" y1="25.4" x2="118.09" y2="75.87" width="0" layer="20"/>
<wire x1="118.09" y1="75.87" x2="55.88" y2="75.87" width="0" layer="20"/>
<wire x1="55.88" y1="75.87" x2="55.88" y2="25.4" width="0" layer="20"/>
<text>H A N I   W 10</text>
<wire x1="83.82" y1="73.66" x2="110.49" y2="73.66" width="0.4064" layer="20"/>
<wire x1="110.49" y1="73.66" x2="115.57" y2="68.58" width="0.4064" layer="20" curve="-90"/>
<wire x1="115.57" y1="68.58" x2="115.57" y2="35.56" width="0.4064" layer="20"/>
<wire x1="115.57" y1="35.56" x2="109.22" y2="29.21" width="0.4064" layer="20" curve="-90"/>
<wire x1="109.22" y1="29.21" x2="73.66" y2="29.21" width="0.4064" layer="20"/>
<wire x1="73.66" y1="29.21" x2="59.69" y2="43.18" width="0.4064" layer="20" curve="-90"/>
<wire x1="59.69" y1="43.18" x2="59.69" y2="60.96" width="0.4064" layer="20"/>
<wire x1="59.69" y1="60.96" x2="72.39" y2="73.66" width="0.4064" layer="20" curve="-90"/>
<wire x1="72.39" y1="73.66" x2="83.82" y2="73.66" width="0.4064" layer="20"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="C1206FAB">
</package>
<package name="R1206FAB">
</package>
<package name="2X03SMD">
</package>
<package name="1X06SMD">
</package>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
<package name="MIC_MEMS_ANALOG_SPU0414HR5H">
<description>http://www.digikey.com/product-search/en?keywords=423-1134-1-ND%09</description>
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
</packages>
</library>
<library name="eagle_fab">
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT 23&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C30" library="fab" package="C1206FAB" value="10UF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="fab" package="C1206FAB" value="1UF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C40" library="fab" package="C1206FAB" value="10UF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="fab" package="C1206FAB" value="10UF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="eagle_fab" package="SOT23" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="fab" package="R1206FAB" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="fab" package="R1206FAB" value="10 K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="fab" package="2X03SMD" value="AVRISPSMD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="fab" package="1X06SMD" value="FTDI-SMD-HEADER">
<attribute name="NAME"/>
</element>
<element name="U$3" library="fab" package="SOIC8" value="ATTINY45SI">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$4" library="fab" package="MIC_MEMS_ANALOG_SPU0414HR5H" value="MIC_MEMS_ANALOG_SPU0414HR5H">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="fab" package="R1206FAB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$6" library="fab" package="LED1206FAB" value="LEDFAB1206">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="6"/>
<contactref element="U$3" pad="4"/>
<contactref element="U$2" pad="1"/>
<contactref element="U$4" pad="2"/>
<contactref element="IC1" pad="3"/>
<contactref element="C2" pad="2"/>
<contactref element="C40" pad="2"/>
<contactref element="C30" pad="1"/>
<contactref element="C10" pad="2"/>
<contactref element="U$6" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="U$1" pad="2"/>
<contactref element="U$3" pad="8"/>
<contactref element="U$2" pad="3"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="PB1">
<contactref element="U$1" pad="1"/>
<contactref element="U$3" pad="6"/>
</signal>
<signal name="PB0">
<contactref element="U$3" pad="5"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="PB2">
<contactref element="U$3" pad="7"/>
<contactref element="U$1" pad="3"/>
<contactref element="U$2" pad="5"/>
</signal>
<signal name="RST">
<contactref element="U$3" pad="1"/>
<contactref element="U$1" pad="5"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U$4" pad="3"/>
<contactref element="C30" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U$4" pad="4"/>
<contactref element="R20" pad="1"/>
</signal>
<signal name="PB4">
<contactref element="R20" pad="2"/>
<contactref element="U$3" pad="3"/>
<contactref element="C40" pad="1"/>
</signal>
<signal name="OUT">
<contactref element="C2" pad="1"/>
<contactref element="U$4" pad="1"/>
<contactref element="R10" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="1"/>
<contactref element="U$6" pad="1"/>
</signal>
<signal name="PB3">
<contactref element="R1" pad="2"/>
<contactref element="U$3" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
