<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.0">
<drawing>
<board>
<plain>
<wire x1="21.59" y1="13.97" x2="77.45" y2="13.97" width="0" layer="20"/>
<wire x1="77.45" y1="13.97" x2="77.45" y2="70.79" width="0" layer="20"/>
<wire x1="77.45" y1="70.79" x2="21.59" y2="70.79" width="0" layer="20"/>
<wire x1="21.59" y1="70.79" x2="21.59" y2="13.97" width="0" layer="20"/>
<wire x1="31.75" y1="58.42" x2="55.88" y2="58.42" width="0.3048" layer="20"/>
<wire x1="55.88" y1="58.42" x2="71.12" y2="43.18" width="0.3048" layer="20" curve="-90"/>
<wire x1="71.12" y1="43.18" x2="71.12" y2="26.67" width="0.3048" layer="20"/>
<wire x1="71.12" y1="26.67" x2="69.85" y2="25.4" width="0.3048" layer="20" curve="-90"/>
<wire x1="69.85" y1="25.4" x2="39.37" y2="25.4" width="0.3048" layer="20"/>
<wire x1="31.75" y1="58.42" x2="27.94" y2="54.61" width="0.3048" layer="20" curve="90"/>
<wire x1="27.94" y1="54.61" x2="27.94" y2="36.83" width="0.3048" layer="20"/>
<wire x1="27.94" y1="36.83" x2="39.37" y2="25.4" width="0.3048" layer="20" curve="90"/>
<text>H A N I  W 12</text>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="C1206FAB">
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT 23&lt;/b&gt;</description>
</package>
<package name="R1206FAB">
</package>
<package name="SOT-23">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
<package name="2X02SMD">
</package>
<package name="2X03SMD">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="fab" package="C1206FAB" value="1UF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="fab" package="SOT23" value="5V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="fab" package="R1206FAB" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="fab" package="R1206FAB" value="500">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T1" library="fab" package="SOT-23" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="fab" package="SOIC8" value="ATTINY45SI">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2/POWER" library="fab" package="2X02SMD" value="PINHD-2X2-SMD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3/SPEAKER" library="fab" package="2X02SMD" value="PINHD-2X2-SMD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ISP" library="fab" package="2X03SMD" value="AVRISPSMD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$5" library="fab" package="LED1206FAB" value="LEDFAB1206">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="U$1" pad="8"/>
<contactref element="ISP" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="IC1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="U$5" pad="2"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="4"/>
<contactref element="ISP" pad="6"/>
<contactref element="T1" pad="2"/>
<contactref element="IC1" pad="3"/>
<contactref element="J2/POWER" pad="1"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="PB1">
<contactref element="U$1" pad="6"/>
<contactref element="ISP" pad="1"/>
<contactref element="T1" pad="3"/>
</signal>
<signal name="RST">
<contactref element="U$1" pad="1"/>
<contactref element="ISP" pad="5"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="PB2">
<contactref element="ISP" pad="3"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="PB0">
<contactref element="ISP" pad="4"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="N$1">
<contactref element="T1" pad="1"/>
<contactref element="J3/SPEAKER" pad="1"/>
</signal>
<signal name="V">
<contactref element="J3/SPEAKER" pad="4"/>
<contactref element="J3/SPEAKER" pad="3"/>
<contactref element="J2/POWER" pad="4"/>
<contactref element="J2/POWER" pad="3"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="U$5" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R2" pad="2"/>
<contactref element="U$1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
