<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.0">
<drawing>
<board>
<plain>
<wire x1="53.34" y1="25.4" x2="123.17" y2="25.4" width="0" layer="20"/>
<wire x1="123.17" y1="25.4" x2="123.17" y2="70.79" width="0" layer="20"/>
<wire x1="123.17" y1="70.79" x2="53.34" y2="70.79" width="0" layer="20"/>
<wire x1="53.34" y1="70.79" x2="53.34" y2="25.4" width="0" layer="20"/>
<text>H A N I     W 15</text>
<wire x1="63.5" y1="62.23" x2="66.04" y2="64.77" width="0.4064" layer="20" curve="-90"/>
<wire x1="66.04" y1="64.77" x2="99.06" y2="64.77" width="0.4064" layer="20"/>
<wire x1="99.06" y1="64.77" x2="114.3" y2="49.53" width="0.4064" layer="20" curve="-90"/>
<wire x1="114.3" y1="49.53" x2="114.3" y2="31.75" width="0.4064" layer="20"/>
<wire x1="113.03" y1="30.48" x2="78.74" y2="30.48" width="0.4064" layer="20"/>
<wire x1="78.74" y1="30.48" x2="63.5" y2="48.26" width="0.4064" layer="20" curve="-90"/>
<wire x1="63.5" y1="48.26" x2="63.5" y2="62.23" width="0.4064" layer="20"/>
<wire x1="113.03" y1="30.48" x2="114.3" y2="31.75" width="0.4064" layer="20" curve="90"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="C1206FAB">
</package>
</packages>
</library>
<library name="eagle_fab">
<packages>
<package name="SOIC14">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="R1206FAB">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="EFOBM">
</package>
<package name="2X03SMD">
</package>
<package name="1X06SMD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="fab" package="C1206FAB" value="1UF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="eagle_fab" package="SOIC14" value="UC_ATTINY44-SSU">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="eagle_fab" package="R1206FAB" value="500">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="eagle_fab" package="R1206FAB" value="1OK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="eagle_fab" package="R1206FAB" value="500">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="eagle_fab" package="LED1206FAB" value="LEDFAB1206">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="eagle_fab" package="EFOBM" value="XTAL_RESONATOR"/>
<element name="U$3" library="eagle_fab" package="2X03SMD" value="CONN_03X2_AVRISPSMD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$4" library="eagle_fab" package="1X06SMD" value="CONN_06_FTDI-SMD-HEADER">
<attribute name="NAME"/>
</element>
<element name="U$5" library="eagle_fab" package="LED1206FAB" value="LEDFAB1206">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="R1" pad="1"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="1"/>
<contactref element="U$3" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="U$4" pad="2"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="14"/>
<contactref element="U$1" pad="2"/>
<contactref element="U$2" pad="2"/>
<contactref element="U$3" pad="6"/>
<contactref element="U$5" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="U$4" pad="3"/>
</signal>
<signal name="PA5">
<contactref element="U$3" pad="1"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="PA4">
<contactref element="U$3" pad="3"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="PB3">
<contactref element="U$3" pad="5"/>
<contactref element="R2" pad="2"/>
<contactref element="IC1" pad="4"/>
</signal>
<signal name="PA6">
<contactref element="U$3" pad="4"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="PA0">
<contactref element="U$4" pad="4"/>
<contactref element="IC1" pad="13"/>
</signal>
<signal name="PA1">
<contactref element="U$4" pad="5"/>
<contactref element="IC1" pad="12"/>
</signal>
<signal name="N$13">
<contactref element="IC1" pad="5"/>
</signal>
<signal name="PA2">
<contactref element="IC1" pad="11"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="PA3">
<contactref element="IC1" pad="10"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="IC1" pad="6"/>
</signal>
<signal name="PB0">
<contactref element="U$2" pad="1"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="PB1">
<contactref element="U$2" pad="3"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="U$5" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
