<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.0">
<drawing>
<schematic>
<libraries>
<library name="fab">
<packages>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R1206W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="R1206FAB">
</package>
<package name="LED1206">
<description>LED 1206 pads (standard pattern)</description>
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="5MM">
<description>5mm round through hole part.</description>
</package>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="EFOBM">
</package>
<package name="EFOS">
</package>
<package name="2X02SMD">
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1206FAB">
</package>
<package name="TQFP32-08THIN">
</package>
<package name="2X03SMD">
</package>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="R-US">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="LED">
<description>LED</description>
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="TS2">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="P1" direction="pas"/>
</symbol>
<symbol name="CERAMIC_RESONATOR">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="PINH2X2">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
</symbol>
<symbol name="CAP-NONPOLARIZED">
<description>non-polarized capacitor</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="23-I/O">
<pin name="PB5(SCK)"/>
<pin name="PB7(XTAL2/TOSC2)"/>
<pin name="PB6(XTAL1/TOSC1)"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="AVCC" direction="pwr"/>
<pin name="PB4(MISO)"/>
<pin name="PB3(MOSI/OC2)"/>
<pin name="PB2(SS/OC1B)"/>
<pin name="PB1(OC1A)"/>
<pin name="PB0(ICP)"/>
<pin name="PD7(AIN1)"/>
<pin name="PD6(AIN0)"/>
<pin name="PD5(T1)"/>
<pin name="PD4(XCK/T0)"/>
<pin name="PD3(INT1)"/>
<pin name="PD2(INT0)"/>
<pin name="PD1(TXD)"/>
<pin name="PD0(RXD)"/>
<pin name="ADC7"/>
<pin name="ADC6"/>
<pin name="PC5(ADC5/SCL)"/>
<pin name="PC4(ADC4/SDA)"/>
<pin name="PC3(ADC3)"/>
<pin name="PC2(ADC2)"/>
<pin name="PC1(ADC1)"/>
<pin name="PC0(ADC0)"/>
<pin name="PC6(/RESET)" function="dot"/>
</symbol>
<symbol name="AVRISP">
<pin name="MISO" direction="pas" function="dot"/>
<pin name="VCC" direction="pas" function="dot"/>
<pin name="SCK" direction="pas" function="dot"/>
<pin name="MOSI" direction="pas" function="dot"/>
<pin name="RST" direction="pas" function="dot"/>
<pin name="GND" direction="pas" function="dot"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="RES-US" prefix="R" uservalue="yes">
<description>&lt;b&gt;Resistor (US Symbol)&lt;/b&gt;
&lt;p&gt;
Variants with postfix FAB are widened to allow the routing of internal traces</description>
<gates>
<gate name="G$1" symbol="R-US"/>
</gates>
<devices>
<device name="1206" package="R1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206W" package="R1206W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206FAB" package="R1206FAB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED">
<description>LED</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="LED1206">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FAB1206" package="LED1206FAB">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5MM" package="5MM">
<connects>
<connect gate="G$1" pin="A" pad="IN"/>
<connect gate="G$1" pin="C" pad="OUT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6MM_SWITCH" prefix="S" uservalue="yes">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
<gates>
<gate name="2" symbol="TS2"/>
</gates>
<devices>
<device name="6MM_SWITCH" package="6MM_SWITCH">
<connects>
<connect gate="2" pin="P" pad="1"/>
<connect gate="2" pin="P1" pad="2"/>
<connect gate="2" pin="S" pad="3"/>
<connect gate="2" pin="S1" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RESONATOR">
<gates>
<gate name="G$1" symbol="CERAMIC_RESONATOR"/>
</gates>
<devices>
<device name="EFOB" package="EFOBM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="VARIANT" value=""/>
</technology>
</technologies>
</device>
<device name="" package="EFOS">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
<connect gate="G$1" pin="3" pad="P$3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X2-SMD">
<gates>
<gate name="G$1" symbol="PINH2X2"/>
</gates>
<devices>
<device name="" package="2X02SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAP-UNPOLARIZED" prefix="C" uservalue="yes">
<gates>
<gate name="&gt;NAME" symbol="CAP-NONPOLARIZED"/>
</gates>
<devices>
<device name="" package="C1206">
<connects>
<connect gate="&gt;NAME" pin="1" pad="1"/>
<connect gate="&gt;NAME" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FAB" package="C1206FAB">
<connects>
<connect gate="&gt;NAME" pin="1" pad="1"/>
<connect gate="&gt;NAME" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA88-THIN" prefix="IC">
<gates>
<gate name="G$1" symbol="23-I/O"/>
</gates>
<devices>
<device name="" package="TQFP32-08THIN">
<connects>
<connect gate="G$1" pin="ADC6" pad="19"/>
<connect gate="G$1" pin="ADC7" pad="22"/>
<connect gate="G$1" pin="AREF" pad="20"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND" pad="21"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="PB0(ICP)" pad="12"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="13"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="14"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="15"/>
<connect gate="G$1" pin="PB4(MISO)" pad="16"/>
<connect gate="G$1" pin="PB5(SCK)" pad="17"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="7"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="8"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="29"/>
<connect gate="G$1" pin="PD0(RXD)" pad="30"/>
<connect gate="G$1" pin="PD1(TXD)" pad="31"/>
<connect gate="G$1" pin="PD2(INT0)" pad="32"/>
<connect gate="G$1" pin="PD3(INT1)" pad="1"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="2"/>
<connect gate="G$1" pin="PD5(T1)" pad="9"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="10"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="11"/>
<connect gate="G$1" pin="VCC@1" pad="4"/>
<connect gate="G$1" pin="VCC@2" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AVRISP">
<gates>
<gate name="G$1" symbol="AVRISP"/>
</gates>
<devices>
<device name="SMD" package="2X03SMD">
<connects>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="MISO" pad="1"/>
<connect gate="G$1" pin="MOSI" pad="4"/>
<connect gate="G$1" pin="RST" pad="5"/>
<connect gate="G$1" pin="SCK" pad="3"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="2X03">
<connects>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="MISO" pad="1"/>
<connect gate="G$1" pin="MOSI" pad="4"/>
<connect gate="G$1" pin="RST" pad="5"/>
<connect gate="G$1" pin="SCK" pad="3"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X06/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X03/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X05">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X05/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1_05X2MM">
<description>CON-M-1X5-200</description>
</package>
</packages>
<symbols>
<symbol name="PINHD6">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD3">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD5">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="PINHD-1X6" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD6"/>
</gates>
<devices>
<device name="" package="1X06">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X06/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X3" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD3"/>
</gates>
<devices>
<device name="" package="1X03">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X03/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X5" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD5"/>
</gates>
<devices>
<device name="" package="1X05">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X05/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5X2MM" package="1_05X2MM">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="eagle_fab">
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT 23&lt;/b&gt;</description>
</package>
<package name="PJ-002AH-SMT">
</package>
</packages>
<symbols>
<symbol name="REGULATOR">
<pin name="IN"/>
<pin name="GND"/>
<pin name="OUT"/>
</symbol>
<symbol name="DC-POWER-JACK">
<pin name="PIN1" direction="pwr"/>
<pin name="SHUNT" direction="pwr"/>
<pin name="CONTACT" direction="pwr"/>
<pin name="PIN2" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="VR_REGULATOR-SOT23" prefix="IC" uservalue="yes">
<gates>
<gate name="G$1" symbol="REGULATOR"/>
</gates>
<devices>
<device name="SOT23" package="SOT23">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_JACK-2.1MM" prefix="J">
<description>SMD DC power jack PJ-002AH-SMT As found in the fablab inventory.

&lt;p&gt;Made by Zaerc.</description>
<gates>
<gate name="G$1" symbol="DC-POWER-JACK"/>
</gates>
<devices>
<device name="" package="PJ-002AH-SMT">
<connects>
<connect gate="G$1" pin="CONTACT" pad="CONTACT"/>
<connect gate="G$1" pin="PIN1" pad="PIN1"/>
<connect gate="G$1" pin="PIN2" pad="PIN2"/>
<connect gate="G$1" pin="SHUNT" pad="SHUNT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<parts>
<part name="JP2" library="pinhead" deviceset="PINHD-1X6" device=""/>
<part name="JP8" library="pinhead" deviceset="PINHD-1X6" device=""/>
<part name="JP7" library="pinhead" deviceset="PINHD-1X3" device=""/>
<part name="JP9" library="pinhead" deviceset="PINHD-1X3" device=""/>
<part name="JP1" library="pinhead" deviceset="PINHD-1X5" device=""/>
<part name="S1" library="fab" deviceset="6MM_SWITCH" device="6MM_SWITCH"/>
<part name="R4" library="fab" deviceset="RES-US" device="1206FAB" value="499 ohm"/>
<part name="U$5" library="fab" deviceset="LED" device="FAB1206"/>
<part name="U$7" library="fab" deviceset="RESONATOR" device="EFOB"/>
<part name="VCC" library="fab" deviceset="PINHD-2X2-SMD" device=""/>
<part name="GND" library="fab" deviceset="PINHD-2X2-SMD" device=""/>
<part name="C1" library="fab" deviceset="CAP-UNPOLARIZED" device="FAB" value="10UF"/>
<part name="C5" library="fab" deviceset="CAP-UNPOLARIZED" device="FAB" value="1UF"/>
<part name="C6" library="fab" deviceset="CAP-UNPOLARIZED" device="FAB" value="1UF"/>
<part name="IC1" library="fab" deviceset="ATMEGA88-THIN" device=""/>
<part name="U$1" library="fab" deviceset="AVRISP" device="SMD"/>
<part name="IC2" library="eagle_fab" deviceset="VR_REGULATOR-SOT23" device="SOT23"/>
<part name="12V" library="fab" deviceset="PINHD-2X2-SMD" device=""/>
<part name="C2" library="fab" deviceset="CAP-UNPOLARIZED" device="FAB" value="1UF"/>
<part name="12V1" library="fab" deviceset="PINHD-2X2-SMD" device=""/>
<part name="R1" library="fab" deviceset="RES-US" device="1206FAB" value="0ohm"/>
<part name="J2" library="eagle_fab" deviceset="CONN_JACK-2.1MM" device=""/>
</parts>
<sheets>
<sheet>
<plain>
</plain>
<busses>
</busses>
<nets>
<net name="VCC">
<segment>
<pinref part="VCC" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="VCC" gate="G$1" pin="3"/>
</segment>
<segment>
<pinref part="VCC" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="VCC" gate="G$1" pin="4"/>
</segment>
<segment>
<pinref part="C1" gate="&gt;NAME" pin="2"/>
</segment>
<segment>
<pinref part="C5" gate="&gt;NAME" pin="2"/>
</segment>
<segment>
<pinref part="C6" gate="&gt;NAME" pin="2"/>
</segment>
<segment>
<pinref part="R4" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="JP1" gate="A" pin="1"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="VCC@1"/>
<pinref part="IC1" gate="G$1" pin="VCC@2"/>
<pinref part="IC1" gate="G$1" pin="AVCC"/>
</segment>
<segment>
<pinref part="U$1" gate="G$1" pin="VCC"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="OUT"/>
</segment>
<segment>
<pinref part="C2" gate="&gt;NAME" pin="2"/>
</segment>
<segment>
<pinref part="R1" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="R1" gate="G$1" pin="1"/>
</segment>
</net>
<net name="GND">
<segment>
<pinref part="GND" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="GND" gate="G$1" pin="3"/>
</segment>
<segment>
<pinref part="GND" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="GND" gate="G$1" pin="4"/>
</segment>
<segment>
<pinref part="U$7" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="C6" gate="&gt;NAME" pin="1"/>
</segment>
<segment>
<pinref part="C5" gate="&gt;NAME" pin="1"/>
</segment>
<segment>
<pinref part="C1" gate="&gt;NAME" pin="1"/>
</segment>
<segment>
<pinref part="U$5" gate="G$1" pin="C"/>
</segment>
<segment>
<pinref part="JP1" gate="A" pin="4"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="GND@1"/>
<pinref part="IC1" gate="G$1" pin="GND@2"/>
<pinref part="IC1" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="U$1" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="C2" gate="&gt;NAME" pin="1"/>
</segment>
<segment>
<pinref part="J2" gate="G$1" pin="CONTACT"/>
</segment>
<segment>
<pinref part="J2" gate="G$1" pin="SHUNT"/>
</segment>
<segment>
<pinref part="JP7" gate="A" pin="3"/>
</segment>
</net>
<net name="XTAL2">
<segment>
<pinref part="U$7" gate="G$1" pin="3"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PB7(XTAL2/TOSC2)"/>
</segment>
</net>
<net name="XTAL1">
<segment>
<pinref part="U$7" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PB6(XTAL1/TOSC1)"/>
</segment>
</net>
<net name="SCK">
<segment>
<pinref part="IC1" gate="G$1" pin="PB5(SCK)"/>
</segment>
<segment>
<pinref part="U$1" gate="G$1" pin="SCK"/>
</segment>
</net>
<net name="MOSI">
<segment>
<pinref part="IC1" gate="G$1" pin="PB3(MOSI/OC2)"/>
</segment>
<segment>
<pinref part="U$1" gate="G$1" pin="MOSI"/>
</segment>
</net>
<net name="MISO">
<segment>
<pinref part="IC1" gate="G$1" pin="PB4(MISO)"/>
</segment>
<segment>
<pinref part="U$1" gate="G$1" pin="MISO"/>
</segment>
</net>
<net name="AREF">
<segment>
<pinref part="JP1" gate="A" pin="3"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="AREF"/>
</segment>
</net>
<net name="ADC6">
<segment>
<pinref part="JP1" gate="A" pin="2"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="ADC6"/>
</segment>
</net>
<net name="ADC7">
<segment>
<pinref part="JP1" gate="A" pin="5"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="ADC7"/>
</segment>
</net>
<net name="A0">
<segment>
<pinref part="JP2" gate="A" pin="1"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PC0(ADC0)"/>
</segment>
</net>
<net name="A1">
<segment>
<pinref part="JP2" gate="A" pin="2"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PC1(ADC1)"/>
</segment>
</net>
<net name="A2">
<segment>
<pinref part="JP2" gate="A" pin="3"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PC2(ADC2)"/>
</segment>
</net>
<net name="A3">
<segment>
<pinref part="JP2" gate="A" pin="4"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PC3(ADC3)"/>
</segment>
</net>
<net name="A4">
<segment>
<pinref part="JP2" gate="A" pin="5"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PC4(ADC4/SDA)"/>
</segment>
</net>
<net name="A5">
<segment>
<pinref part="JP2" gate="A" pin="6"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PC5(ADC5/SCL)"/>
</segment>
</net>
<net name="D2">
<segment>
<pinref part="IC1" gate="G$1" pin="PD2(INT0)"/>
</segment>
<segment>
<pinref part="JP9" gate="A" pin="1"/>
</segment>
</net>
<net name="D3">
<segment>
<pinref part="IC1" gate="G$1" pin="PD3(INT1)"/>
</segment>
<segment>
<pinref part="JP9" gate="A" pin="2"/>
</segment>
</net>
<net name="D4">
<segment>
<pinref part="IC1" gate="G$1" pin="PD4(XCK/T0)"/>
</segment>
<segment>
<pinref part="JP9" gate="A" pin="3"/>
</segment>
</net>
<net name="D5">
<segment>
<pinref part="IC1" gate="G$1" pin="PD5(T1)"/>
</segment>
<segment>
<pinref part="JP8" gate="A" pin="1"/>
</segment>
</net>
<net name="D6">
<segment>
<pinref part="JP8" gate="A" pin="2"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PD6(AIN0)"/>
</segment>
</net>
<net name="D7">
<segment>
<pinref part="JP8" gate="A" pin="3"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PD7(AIN1)"/>
</segment>
</net>
<net name="D8">
<segment>
<pinref part="JP8" gate="A" pin="4"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PB0(ICP)"/>
</segment>
</net>
<net name="D9">
<segment>
<pinref part="JP8" gate="A" pin="5"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PB1(OC1A)"/>
</segment>
</net>
<net name="D10">
<segment>
<pinref part="JP8" gate="A" pin="6"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PB2(SS/OC1B)"/>
</segment>
</net>
<net name="N$6">
<segment>
<pinref part="S1" gate="2" pin="P"/>
<pinref part="U$5" gate="G$1" pin="A"/>
</segment>
</net>
<net name="RST">
<segment>
<pinref part="R4" gate="G$1" pin="1"/>
<pinref part="S1" gate="2" pin="S"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PC6(/RESET)"/>
</segment>
<segment>
<pinref part="U$1" gate="G$1" pin="RST"/>
</segment>
</net>
<net name="RX">
<segment>
<pinref part="JP7" gate="A" pin="1"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PD0(RXD)"/>
</segment>
</net>
<net name="TX">
<segment>
<pinref part="JP7" gate="A" pin="2"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PD1(TXD)"/>
</segment>
</net>
<net name="12V">
<segment>
<pinref part="IC2" gate="G$1" pin="IN"/>
</segment>
<segment>
<pinref part="12V" gate="G$1" pin="3"/>
</segment>
<segment>
<pinref part="12V" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="12V" gate="G$1" pin="4"/>
</segment>
<segment>
<pinref part="12V1" gate="G$1" pin="3"/>
</segment>
<segment>
<pinref part="12V1" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="12V1" gate="G$1" pin="4"/>
</segment>
<segment>
<pinref part="J2" gate="G$1" pin="PIN1"/>
</segment>
</net>
<net name="12V\">
<segment>
<pinref part="12V" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="12V1" gate="G$1" pin="1"/>
</segment>
</net>
</nets>
</sheet>
</sheets>
</schematic>
</drawing>
</eagle>
