<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.6.3">
<drawing>
<board>
<plain>
<wire x1="18.6508" y1="0.8061" x2="20.3974" y2="1.7757" width="0.254" layer="20" curve="28.79673"/>
<wire x1="20.3974" y1="1.7757" x2="21.6981" y2="5.8635" width="0.254" layer="20" curve="65.224797"/>
<wire x1="21.6981" y1="5.8635" x2="28.0731" y2="9.4378" width="0.254" layer="20"/>
<wire x1="28.0731" y1="9.4378" x2="33.8838" y2="9.4378" width="0.254" layer="20" curve="89.08981"/>
<wire x1="33.8838" y1="9.4378" x2="40.5392" y2="5.3838" width="0.254" layer="20"/>
<wire x1="40.5392" y1="5.3838" x2="43.4581" y2="0.1777" width="0.254" layer="20" curve="97.267996"/>
<wire x1="43.4581" y1="0.1777" x2="43.4581" y2="0" width="0.254" layer="20"/>
<wire x1="43.4581" y1="0" x2="45.3027" y2="0" width="0.254" layer="20"/>
<wire x1="45.3027" y1="0" x2="45.3027" y2="0.2216" width="0.254" layer="20"/>
<wire x1="45.3027" y1="0.2216" x2="47.7419" y2="1.9919" width="0.254" layer="20" curve="44.10637"/>
<wire x1="47.7419" y1="1.9919" x2="47.8669" y2="2.198" width="0.254" layer="20"/>
<wire x1="47.8669" y1="2.198" x2="48.252" y2="5.1878" width="0.254" layer="20" curve="44.591106"/>
<wire x1="48.252" y1="5.1878" x2="54.7858" y2="8.8905" width="0.254" layer="20"/>
<wire x1="54.7858" y1="8.8905" x2="58.6101" y2="15.5661" width="0.254" layer="20" curve="212.492902"/>
<wire x1="58.6101" y1="15.5661" x2="58.6101" y2="23.4343" width="0.254" layer="20"/>
<wire x1="58.6101" y1="23.4343" x2="54.7351" y2="30.0357" width="0.254" layer="20" curve="214.424216"/>
<wire x1="54.7351" y1="30.0357" x2="48.0459" y2="34.0897" width="0.254" layer="20"/>
<wire x1="48.0459" y1="34.0897" x2="40.5088" y2="34.1336" width="0.254" layer="20" curve="219.704191"/>
<wire x1="40.5088" y1="34.1336" x2="34.198" y2="30.5931" width="0.254" layer="20"/>
<wire x1="34.198" y1="30.5931" x2="28.8906" y2="31.3059" width="0.254" layer="20" curve="84.039397"/>
<wire x1="28.8906" y1="31.3059" x2="28.0866" y2="30.6303" width="0.254" layer="20" curve="14.885059"/>
<wire x1="28.0866" y1="30.6303" x2="21.3974" y2="34.6843" width="0.254" layer="20"/>
<wire x1="21.3974" y1="34.6843" x2="13.8603" y2="34.7282" width="0.254" layer="20" curve="219.704191"/>
<wire x1="13.8603" y1="34.7282" x2="7.5597" y2="30.9642" width="0.254" layer="20"/>
<wire x1="7.5597" y1="30.9642" x2="3.5428" y2="24.4811" width="0.254" layer="20" curve="215.750779"/>
<wire x1="3.5428" y1="24.4811" x2="3.5428" y2="16.8263" width="0.254" layer="20"/>
<wire x1="3.5428" y1="16.8263" x2="0.4786" y2="11.5324" width="0.254" layer="20" curve="97.946112"/>
<wire x1="0.4786" y1="11.5324" x2="0" y2="11.2625" width="0.254" layer="20"/>
<wire x1="0" y1="11.2625" x2="0" y2="9.6927" width="0.254" layer="20"/>
<wire x1="0" y1="9.6927" x2="1.1543" y2="10.3432" width="0.254" layer="20"/>
<wire x1="1.1543" y1="10.3432" x2="7.1745" y2="10.0932" width="0.254" layer="20" curve="97.73354"/>
<wire x1="7.1745" y1="10.0932" x2="13.884" y2="5.9986" width="0.254" layer="20"/>
<wire x1="13.884" y1="5.9986" x2="16.8029" y2="0.7926" width="0.254" layer="20" curve="97.268045"/>
<wire x1="16.8029" y1="0.7926" x2="16.8029" y2="0" width="0.254" layer="20"/>
<wire x1="16.8029" y1="0" x2="18.6508" y2="0" width="0.254" layer="20"/>
<wire x1="18.6508" y1="0" x2="18.6508" y2="0.8061" width="0.254" layer="20"/>
<wire x1="31.9649" y1="16.1844" x2="31.9649" y2="24.0222" width="0.254" layer="20"/>
<wire x1="31.9649" y1="24.0222" x2="33.0967" y2="24.4918" width="0.254" layer="20" curve="17.516351"/>
<wire x1="33.0967" y1="24.4918" x2="34.9007" y2="29.3938" width="0.254" layer="20" curve="81.60954"/>
<wire x1="34.9007" y1="29.3938" x2="41.1777" y2="32.9309" width="0.254" layer="20"/>
<wire x1="41.1777" y1="32.9309" x2="47.2317" y2="32.7721" width="0.254" layer="20" curve="98.291856"/>
<wire x1="47.2317" y1="32.7721" x2="53.9209" y2="28.7181" width="0.254" layer="20"/>
<wire x1="53.9209" y1="28.7181" x2="56.7722" y2="23.4445" width="0.254" layer="20" curve="97.849626"/>
<wire x1="56.7722" y1="23.4445" x2="56.7722" y2="15.5932" width="0.254" layer="20"/>
<wire x1="56.7722" y1="15.5932" x2="53.8026" y2="10.5864" width="0.254" layer="20" curve="93.379013"/>
<wire x1="53.8026" y1="10.5864" x2="47.2892" y2="6.904" width="0.254" layer="20"/>
<wire x1="47.2892" y1="6.904" x2="41.4075" y2="6.8838" width="0.254" layer="20" curve="94.757408"/>
<wire x1="41.4075" y1="6.8838" x2="34.7892" y2="10.8973" width="0.254" layer="20"/>
<wire x1="34.7892" y1="10.8973" x2="33.519" y2="15.3939" width="0.254" layer="20" curve="72.465083"/>
<wire x1="33.519" y1="15.3939" x2="33.4818" y2="15.4243" width="0.254" layer="20"/>
<wire x1="33.4818" y1="15.4243" x2="33.3163" y2="15.5459" width="0.254" layer="20"/>
<wire x1="33.3163" y1="15.5459" x2="31.9649" y2="16.1844" width="0.254" layer="20" curve="21.646213"/>
</plain>
<libraries>
<library name="fablibrary">
<packages>
<package name="C1206FAB">
</package>
<package name="1X06SMD">
</package>
<package name="2X02SMD">
</package>
<package name="2X03SMD">
</package>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
<package name="R1206FAB">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="fablibrary" package="C1206FAB" value="1uF"/>
<element name="FTDI" library="fablibrary" package="1X06SMD" value="FTDI-SMD-HEADER"/>
<element name="I2C" library="fablibrary" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="ISP" library="fablibrary" package="2X03SMD" value=""/>
<element name="MASTERBRIDGE" library="fablibrary" package="SOIC8" value="ATTINY45SI"/>
<element name="R3" library="fablibrary" package="R1206FAB" value="10K"/>
<element name="R2" library="fablibrary" package="R1206FAB" value="10K"/>
<element name="R1" library="fablibrary" package="R1206FAB" value="10K"/>
</elements>
<signals>
<signal name="GND">
<contactref element="FTDI" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="MASTERBRIDGE" pad="4"/>
<contactref element="I2C" pad="2"/>
<contactref element="ISP" pad="1"/>
</signal>
<signal name="RST">
<contactref element="ISP" pad="2"/>
<contactref element="MASTERBRIDGE" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="ISP" pad="5"/>
<contactref element="R3" pad="1"/>
<contactref element="I2C" pad="4"/>
<contactref element="FTDI" pad="3"/>
<contactref element="MASTERBRIDGE" pad="8"/>
<contactref element="R1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="MISO">
<contactref element="ISP" pad="6"/>
<contactref element="MASTERBRIDGE" pad="6"/>
</signal>
<signal name="SCK">
<contactref element="ISP" pad="4"/>
<contactref element="MASTERBRIDGE" pad="7"/>
<contactref element="I2C" pad="1"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="TXD">
<contactref element="MASTERBRIDGE" pad="2"/>
<contactref element="FTDI" pad="4"/>
</signal>
<signal name="RXD">
<contactref element="FTDI" pad="5"/>
<contactref element="MASTERBRIDGE" pad="3"/>
</signal>
<signal name="SDA">
<contactref element="I2C" pad="3"/>
<contactref element="ISP" pad="3"/>
<contactref element="MASTERBRIDGE" pad="5"/>
<contactref element="R2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
