<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="37.826" y2="0.254" width="0" layer="20"/>
<wire x1="37.826" y1="0.254" x2="37.826" y2="27.61" width="0" layer="20"/>
<wire x1="37.826" y1="27.61" x2="0" y2="27.356" width="0" layer="20"/>
<wire x1="0" y1="27.356" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
<description>&lt;p&gt;&lt;b&gt;Generic 3216 (1206) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="fab">
<packages>
<package name="2X03SMD">
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="2X02SMD">
</package>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
<package name="LED1206">
<description>LED 1206 pads (standard pattern)</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="1206" value="1.0uF">
<attribute name="PROD_ID" value="CAP-09822"/>
</element>
<element name="J1ISP" library="fab" package="2X03SMD" value="AVRISPSMD"/>
<element name="R4" library="fab" package="R1206" value=""/>
<element name="SERIAL2" library="fab" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="U$1" library="fab" package="SOIC8" value="ATTINY45SI"/>
<element name="U$2" library="fab" package="LED1206" value="LED"/>
<element name="R1" library="fab" package="R1206" value=""/>
</elements>
<signals>
<signal name="RST">
<contactref element="J1ISP" pad="5"/>
<contactref element="R4" pad="1"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="J1ISP" pad="4"/>
<contactref element="U$1" pad="5"/>
<contactref element="U$2" pad="2"/>
</signal>
<signal name="GND">
<contactref element="J1ISP" pad="6"/>
<contactref element="U$1" pad="4"/>
<contactref element="C1" pad="1"/>
<contactref element="SERIAL2" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="J1ISP" pad="2"/>
<contactref element="U$1" pad="8"/>
<contactref element="C1" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="SERIAL2" pad="3"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="SCK">
<contactref element="J1ISP" pad="3"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="MISO">
<contactref element="J1ISP" pad="1"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="TX">
<contactref element="SERIAL2" pad="2"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="RX">
<contactref element="SERIAL2" pad="4"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="U$2" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$1">
</signal>
</signals>
</board>
</drawing>
</eagle>
