<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<board>
<plain>
</plain>
<libraries>
<library name="esp12e">
<packages>
<package name="ESP8266-ESP12E">
<description>
&lt;b&gt;ESP8266-12E Library for Eagle CAD&lt;/b&gt;&lt;p&gt;
The author not responsible for any damages or errors!.&lt;p&gt;
&lt;author&gt;Created by Suhail jr.lt;/author&gt;
</description>
</package>
</packages>
</library>
<library name="fab">
<packages>
<package name="1X06SMD">
</package>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT 23&lt;/b&gt;</description>
</package>
<package name="C1206FAB">
</package>
<package name="R1206FAB">
</package>
<package name="SOT-23">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="JACK_2.1MM">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
</packages>
</library>
<library name="Seeed-OPL-Relay">
<packages>
<package name="REY5-19.0X15.0X15.0MM">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="MOLEX-1X2_LOCK">
</package>
</packages>
</library>
<library name="con-amp-quick">
<description>&lt;b&gt;AMP Connectors, Type QUICK&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="03P">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="v-reg">
<description>&lt;b&gt;Voltage Regulators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;Small Outline Transistor 223&lt;/b&gt;&lt;p&gt;
PLASTIC PACKAGE CASE 318E-04&lt;br&gt;
Source: http://www.onsemi.co.jp .. LM137M-D.PDF</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="SJR1" library="esp12e" package="ESP8266-ESP12E" value="">
<attribute name="NAME"/>
</element>
<element name="U$7" library="fab" package="1X06SMD" value="FTDI-SMD-HEADER">
<attribute name="NAME"/>
</element>
<element name="S1" library="fab" package="6MM_SWITCH" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="fab" package="SOT23" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S2" library="fab" package="6MM_SWITCH" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="fab" package="C1206FAB" value="10uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="fab" package="R1206FAB" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="fab" package="R1206FAB" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="fab" package="R1206FAB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="K1" library="Seeed-OPL-Relay" package="REY5-19.0X15.0X15.0MM" value="HLS8L-DC5V-S-C">
<attribute name="MPN" value="HLS8L-DC5V-S-C"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="MOLEX-1X2_LOCK" value=""/>
<element name="T1" library="fab" package="SOT-23" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="fab" package="R1206FAB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="K2" library="Seeed-OPL-Relay" package="REY5-19.0X15.0X15.0MM" value="HLS8L-DC5V-S-C">
<attribute name="MPN" value="HLS8L-DC5V-S-C"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="MOLEX-1X2_LOCK" value=""/>
<element name="T2" library="fab" package="SOT-23" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="fab" package="JACK_2.1MM" value="JACK2.1MM"/>
<element name="R3" library="fab" package="R1206FAB" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="fab" package="R1206FAB" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SL1" library="con-amp-quick" package="03P" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="fab" package="R1206FAB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="v-reg" package="SOT223" value="LD117AS12TR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="fab" package="LED1206FAB" value="LEDFAB1206">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="fab" package="LED1206FAB" value="LEDFAB1206">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="fab" package="R1206FAB" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="fab" package="R1206FAB" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="fab" package="R1206FAB" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="fab" package="R1206FAB" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="fab" package="R1206FAB" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="fab" package="R1206FAB" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="fab" package="R1206FAB" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="SJR1" pad="9"/>
<contactref element="U$7" pad="1"/>
<contactref element="IC1" pad="3"/>
<contactref element="S2" pad="1"/>
<contactref element="S2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="S1" pad="4"/>
<contactref element="S1" pad="3"/>
<contactref element="T1" pad="2"/>
<contactref element="T2" pad="2"/>
<contactref element="J4" pad="CONTACT"/>
<contactref element="SL1" pad="1"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="SJR1" pad="16"/>
<contactref element="U$7" pad="5"/>
</signal>
<signal name="N$4">
<contactref element="SJR1" pad="15"/>
<contactref element="U$7" pad="4"/>
</signal>
<signal name="N$8">
<contactref element="S1" pad="1"/>
<contactref element="SJR1" pad="12"/>
<contactref element="S1" pad="2"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="3V3">
<contactref element="R7" pad="1"/>
<contactref element="IC1" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="SJR1" pad="8"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="S2" pad="3"/>
<contactref element="S2" pad="4"/>
<contactref element="C1" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="SJR1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R8" pad="1"/>
<contactref element="SJR1" pad="10"/>
</signal>
<signal name="N$2">
<contactref element="K1" pad="3"/>
<contactref element="T1" pad="1"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="K1" pad="2"/>
<contactref element="U$7" pad="3"/>
<contactref element="IC1" pad="2"/>
<contactref element="K2" pad="2"/>
<contactref element="IC2" pad="4"/>
<contactref element="U$1" pad="2"/>
<contactref element="U$2" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="2"/>
<contactref element="T1" pad="3"/>
</signal>
<signal name="CONTROL">
<contactref element="R2" pad="1"/>
<contactref element="SJR1" pad="14"/>
</signal>
<signal name="N$6">
<contactref element="K1" pad="4"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="K1" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="K2" pad="3"/>
<contactref element="T2" pad="1"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="R2" pad="2"/>
<contactref element="T2" pad="3"/>
</signal>
<signal name="N$13">
<contactref element="K2" pad="4"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="K2" pad="1"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="12V">
<contactref element="J4" pad="PIN"/>
<contactref element="IC2" pad="3"/>
<contactref element="SL1" pad="3"/>
</signal>
<signal name="CONTROL02">
<contactref element="R1" pad="1"/>
<contactref element="SJR1" pad="13"/>
</signal>
<signal name="N$15">
<contactref element="SJR1" pad="3"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="SJR1" pad="5"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="R5" pad="1"/>
<contactref element="SL1" pad="2"/>
</signal>
<signal name="N$16">
</signal>
<signal name="N$18">
</signal>
<signal name="N$20">
</signal>
<signal name="N$21">
</signal>
<signal name="N$22">
</signal>
</signals>
</board>
</drawing>
</eagle>
