<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.0">
<drawing>
<schematic>
<libraries>
<library name="fab">
<packages>
<package name="SOT-23">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="TO252">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
TS-003</description>
</package>
</packages>
<symbols>
<symbol name="N_MOSFET">
<pin name="D" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="G" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="NMOSFET" prefix="T" uservalue="yes">
<description>&lt;b&gt;MOS FET&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="N_MOSFET"/>
</gates>
<devices>
<device name="SOT23" package="SOT-23">
<connects>
<connect gate="A" pin="D" pad="1"/>
<connect gate="A" pin="G" pad="3"/>
<connect gate="A" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO252" package="TO252">
<connects>
<connect gate="A" pin="D" pad="3"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="supply1">
<description>&lt;b&gt;Supply Symbols&lt;/b&gt;&lt;p&gt;
 GND, VCC, 0V, +5V, -5V, etc.&lt;p&gt;
 Please keep in mind, that these devices are necessary for the
 automatic wiring of the supply signals.&lt;p&gt;
 The pin name defined in the symbol is identical to the net which is to be wired automatically.&lt;p&gt;
 In this library the device names are the same as the pin names of the symbols, therefore the correct signal names appear next to the supply symbols in the schematic.&lt;p&gt;
 &lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
</packages>
<symbols>
<symbol name="GND">
<pin name="GND" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="GND" prefix="GND">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="GND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X03/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="PINHD3">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="PINHD-1X3" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD3"/>
</gates>
<devices>
<device name="" package="1X03">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X03/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<parts>
<part name="GND1" library="supply1" deviceset="GND" device=""/>
<part name="JP1" library="pinhead" deviceset="PINHD-1X3" device=""/>
<part name="T2" library="fab" deviceset="NMOSFET" device="SOT23"/>
</parts>
<sheets>
<sheet>
<plain>
</plain>
<busses>
</busses>
<nets>
<net name="GND">
<segment>
<pinref part="GND1" gate="1" pin="GND"/>
<pinref part="T2" gate="A" pin="S"/>
</segment>
<segment>
<pinref part="JP1" gate="A" pin="3"/>
</segment>
</net>
<net name="BMX">
<segment>
<pinref part="JP1" gate="A" pin="2"/>
</segment>
<segment>
<pinref part="T2" gate="A" pin="D"/>
</segment>
</net>
<net name="CONTROL">
<segment>
<pinref part="JP1" gate="A" pin="1"/>
</segment>
<segment>
<pinref part="T2" gate="A" pin="G"/>
</segment>
</net>
</nets>
</sheet>
</sheets>
</schematic>
</drawing>
</eagle>
