<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<board>
<plain>
<wire x1="38.1" y1="10.16" x2="72.37" y2="10.16" width="0" layer="20"/>
<wire x1="72.37" y1="10.16" x2="72.37" y2="32.69" width="0" layer="20"/>
<wire x1="72.37" y1="32.69" x2="38.1" y2="32.69" width="0" layer="20"/>
<wire x1="38.1" y1="32.69" x2="38.1" y2="10.16" width="0" layer="20"/>
</plain>
<libraries>
<library name="fab_new">
<packages>
<package name="C1206FAB">
</package>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
<package name="1X06SMD">
</package>
</packages>
</library>
<library name="eagle_fab">
<packages>
<package name="R1206FAB">
</package>
</packages>
</library>
<library name="ADXL343BCCZ">
<packages>
<package name="LGA_CC-14-1">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="fab_new" package="C1206FAB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="eagle_fab" package="R1206FAB" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="eagle_fab" package="R1206FAB" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="fab_new" package="SOIC8" value="UC_ATTINY412SI">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="fab_new" package="1X06SMD" value="CONN_06_FTDI-SMD-HEADER">
<attribute name="NAME"/>
</element>
<element name="U1" library="ADXL343BCCZ" package="LGA_CC-14-1" value="ADXL343BCCZ">
<attribute name="MANUFACTURER_PART_NUMBER" value="ADXL343BCCZ"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="Analog Devices Inc"/>
</element>
<element name="R3" library="eagle_fab" package="R1206FAB" value="0k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="eagle_fab" package="R1206FAB" value="0k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="eagle_fab" package="R1206FAB" value="0k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="SCL">
<contactref element="U1" pad="14"/>
<contactref element="R2" pad="1"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="SDA">
<contactref element="R1" pad="1"/>
<contactref element="U$1" pad="4"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="2"/>
<contactref element="U$2" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="U$1" pad="8"/>
</signal>
<signal name="VCC">
<contactref element="U$2" pad="3"/>
<contactref element="U$1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="7"/>
<contactref element="U1" pad="6"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="U1" pad="1"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="RXD">
<contactref element="U$2" pad="5"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="UPDI">
<contactref element="U$1" pad="6"/>
<contactref element="U$2" pad="6"/>
</signal>
<signal name="TXD">
<contactref element="U$1" pad="2"/>
<contactref element="U$2" pad="4"/>
</signal>
<signal name="ALT">
<contactref element="U1" pad="12"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="13"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
