<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<board>
<plain>
<wire x1="64.77" y1="22.86" x2="93.96" y2="22.86" width="0" layer="20"/>
<wire x1="93.96" y1="22.86" x2="93.96" y2="64.44" width="0" layer="20"/>
<wire x1="93.96" y1="64.44" x2="64.77" y2="64.44" width="0" layer="20"/>
<wire x1="64.77" y1="64.44" x2="64.77" y2="22.86" width="0" layer="20"/>
</plain>
<libraries>
<library name="fab_new">
<packages>
<package name="C1206FAB">
</package>
<package name="1X06SMD">
</package>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOLDER_PAD_2">
<description>&lt;h3&gt;LuMini Ring Solder Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: .8 in&lt;/li&gt;
&lt;li&gt;Area: .4 x 1 in.&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="eagle_fab">
<packages>
<package name="R1206FAB">
</package>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="fab_new" package="C1206FAB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="SOLDER_PAD_2" value="SOLDER_PAD_2"/>
<element name="R1" library="eagle_fab" package="R1206FAB" value="120 ohms">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="eagle_fab" package="R1206FAB" value="0 ohms">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="eagle_fab" package="6MM_SWITCH" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="fab_new" package="1X06SMD" value="CONN_06_FTDI-SMD-HEADER">
<attribute name="NAME"/>
</element>
<element name="U$2" library="fab_new" package="SOIC8" value="UC_ATTINY412SI">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="eagle_fab" package="LED1206FAB" value="LEDFAB1206">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="eagle_fab" package="R1206FAB" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="eagle_fab" package="R1206FAB" value="0k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="eagle_fab" package="R1206FAB" value="0k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$3">
<contactref element="R1" pad="2"/>
<contactref element="U$3" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="U$2" pad="5"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="GRD">
<contactref element="J1" pad="P$2"/>
<contactref element="U$2" pad="8"/>
<contactref element="U$1" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="U$3" pad="1"/>
<contactref element="U$2" pad="2"/>
</signal>
<signal name="UPDI">
<contactref element="J1" pad="P$1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="1">
<contactref element="U$2" pad="3"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="S1" pad="4"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="U$2" pad="4"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="C1" pad="1"/>
<contactref element="U$1" pad="3"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="5"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="S1" pad="2"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="R3" pad="2"/>
<contactref element="U$2" pad="6"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
