<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<schematic>
<libraries>
<library name="ESP8266-12E_ESP-12E">
<packages>
<package name="XCVR_ESP8266-12E/ESP-12E">
</package>
</packages>
<symbols>
<symbol name="ESP8266-12E/ESP-12E">
<pin name="RESET" direction="in"/>
<pin name="ADC" direction="pas"/>
<pin name="IO16"/>
<pin name="IO14"/>
<pin name="IO12"/>
<pin name="IO13"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="IO15"/>
<pin name="IO2"/>
<pin name="IO0"/>
<pin name="IO5"/>
<pin name="IO4"/>
<pin name="RXD" direction="in"/>
<pin name="TXD" direction="out"/>
<pin name="MISO"/>
<pin name="EN" direction="in"/>
<pin name="CS0" direction="in"/>
<pin name="IO9"/>
<pin name="IO10"/>
<pin name="MOSI"/>
<pin name="SCLK" direction="in" function="clk"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ESP8266-12E/ESP-12E" prefix="U">
<description>ESP-12E WiFi Module &lt;a href="https://pricing.snapeda.com/parts/ESP8266-12E/ESP-12E/AI-Thinker/view-part?ref=eda"&gt;Check prices&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="ESP8266-12E/ESP-12E"/>
</gates>
<devices>
<device name="" package="XCVR_ESP8266-12E/ESP-12E">
<connects>
<connect gate="G$1" pin="ADC" pad="2"/>
<connect gate="G$1" pin="CS0" pad="9"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="IO0" pad="18"/>
<connect gate="G$1" pin="IO10" pad="12"/>
<connect gate="G$1" pin="IO12" pad="6"/>
<connect gate="G$1" pin="IO13" pad="7"/>
<connect gate="G$1" pin="IO14" pad="5"/>
<connect gate="G$1" pin="IO15" pad="16"/>
<connect gate="G$1" pin="IO16" pad="4"/>
<connect gate="G$1" pin="IO2" pad="17"/>
<connect gate="G$1" pin="IO4" pad="19"/>
<connect gate="G$1" pin="IO5" pad="20"/>
<connect gate="G$1" pin="IO9" pad="11"/>
<connect gate="G$1" pin="MISO" pad="10"/>
<connect gate="G$1" pin="MOSI" pad="13"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="RXD" pad="21"/>
<connect gate="G$1" pin="SCLK" pad="14"/>
<connect gate="G$1" pin="TXD" pad="22"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="AVAILABILITY" value="No availability data"/>
<attribute name="DESCRIPTION" value=" This WiFi module has a 32-bit MCU micro and clock speeds supporting 80 MHz or 160 MHz. Supports the RTOS and integrated Wi-Fi MAC/BB/RF/PA/LNA, and has an on-board antenna. "/>
<attribute name="MF" value="AI-Thinker"/>
<attribute name="MP" value="ESP8266-12E/ESP-12E"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="fab">
<packages>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="TS2">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="P1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="6MM_SWITCH" prefix="S" uservalue="yes">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
<gates>
<gate name="2" symbol="TS2"/>
</gates>
<devices>
<device name="6MM_SWITCH" package="6MM_SWITCH">
<connects>
<connect gate="2" pin="P" pad="1"/>
<connect gate="2" pin="P1" pad="2"/>
<connect gate="2" pin="S" pad="3"/>
<connect gate="2" pin="S1" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="FAB_Hello">
<packages>
<package name="1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="0402">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="5MM">
<description>5 mm, round</description>
</package>
<package name="0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="RESISTOR">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="LED">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="CAP-NP">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="RESISTOR" prefix="R" uservalue="yes">
<gates>
<gate name="G$1" symbol="RESISTOR"/>
</gates>
<devices>
<device name="1206" package="1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0402" package="0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED" uservalue="yes">
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="1206" package="1206">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0402" package="0402">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5MM" package="5MM">
<connects>
<connect gate="G$1" pin="A" pad="IN"/>
<connect gate="G$1" pin="C" pad="OUT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603" package="0603">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UNPOLARIZED_CAPACITOR" prefix="C" uservalue="yes">
<description>unpolarized_capacitor</description>
<gates>
<gate name="1" symbol="CAP-NP"/>
</gates>
<devices>
<device name="1206" package="1206">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="con-amp-quick">
<description>&lt;b&gt;AMP Connectors, Type QUICK&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="06P">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
<package name="03P">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
<package name="04P">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="M06">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="M03">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="M04">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="M06" prefix="SL" uservalue="yes">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="M06"/>
</gates>
<devices>
<device name="" package="06P">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="5"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M03" prefix="SL" uservalue="yes">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="M03"/>
</gates>
<devices>
<device name="" package="03P">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="12"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M04" prefix="SL" uservalue="yes">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="M04"/>
</gates>
<devices>
<device name="" package="04P">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="19"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<parts>
<part name="U4" library="ESP8266-12E_ESP-12E" deviceset="ESP8266-12E/ESP-12E" device=""/>
<part name="RST" library="fab" deviceset="6MM_SWITCH" device="6MM_SWITCH"/>
<part name="PROG" library="fab" deviceset="6MM_SWITCH" device="6MM_SWITCH"/>
<part name="R6" library="FAB_Hello" deviceset="RESISTOR" device="1206" value="10k"/>
<part name="R7" library="FAB_Hello" deviceset="RESISTOR" device="1206" value="10k"/>
<part name="R12" library="FAB_Hello" deviceset="RESISTOR" device="1206" value="10k"/>
<part name="R11" library="FAB_Hello" deviceset="RESISTOR" device="1206" value="10k"/>
<part name="SL1" library="con-amp-quick" deviceset="M06" device=""/>
<part name="SL2" library="con-amp-quick" deviceset="M06" device=""/>
<part name="REGULATOR" library="con-amp-quick" deviceset="M03" device=""/>
<part name="SL4" library="con-amp-quick" deviceset="M04" device=""/>
<part name="SL3" library="con-amp-quick" deviceset="M03" device=""/>
<part name="R2" library="FAB_Hello" deviceset="RESISTOR" device="1206" value="499"/>
<part name="LED1" library="FAB_Hello" deviceset="LED" device="1206" value="GREEN"/>
<part name="C9" library="FAB_Hello" deviceset="UNPOLARIZED_CAPACITOR" device="1206" value="10UF"/>
<part name="C1" library="FAB_Hello" deviceset="UNPOLARIZED_CAPACITOR" device="1206" value="10UF"/>
</parts>
<sheets>
<sheet>
<plain>
</plain>
<busses>
</busses>
<nets>
<net name="GND">
<segment>
<pinref part="U4" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="R7" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="PROG" gate="2" pin="P1"/>
</segment>
<segment>
<pinref part="RST" gate="2" pin="P"/>
<pinref part="RST" gate="2" pin="P1"/>
</segment>
<segment>
<pinref part="SL1" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="R2" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="C9" gate="1" pin="1"/>
</segment>
<segment>
<pinref part="C1" gate="1" pin="2"/>
</segment>
<segment>
<pinref part="REGULATOR" gate="G$1" pin="1"/>
</segment>
</net>
<net name="VCC">
<segment>
<pinref part="U4" gate="G$1" pin="VCC"/>
</segment>
<segment>
<pinref part="R12" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="R11" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="R6" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="REGULATOR" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="C1" gate="1" pin="1"/>
</segment>
</net>
<net name="TX">
<segment>
<pinref part="U4" gate="G$1" pin="TXD"/>
</segment>
<segment>
<pinref part="SL1" gate="G$1" pin="4"/>
</segment>
</net>
<net name="IO15">
<segment>
<pinref part="U4" gate="G$1" pin="IO15"/>
</segment>
<segment>
<pinref part="R7" gate="G$1" pin="2"/>
</segment>
</net>
<net name="RST">
<segment>
<pinref part="U4" gate="G$1" pin="RESET"/>
</segment>
<segment>
<pinref part="RST" gate="2" pin="S1"/>
<pinref part="RST" gate="2" pin="S"/>
<pinref part="R12" gate="G$1" pin="1"/>
</segment>
<segment>
</segment>
</net>
<net name="CH_PD">
<segment>
<pinref part="U4" gate="G$1" pin="EN"/>
</segment>
<segment>
<pinref part="R6" gate="G$1" pin="1"/>
</segment>
</net>
<net name="RX">
<segment>
<pinref part="U4" gate="G$1" pin="RXD"/>
</segment>
<segment>
<pinref part="SL1" gate="G$1" pin="5"/>
</segment>
</net>
<net name="IO0">
<segment>
<pinref part="U4" gate="G$1" pin="IO0"/>
</segment>
<segment>
<pinref part="PROG" gate="2" pin="S"/>
<pinref part="PROG" gate="2" pin="S1"/>
<pinref part="R11" gate="G$1" pin="2"/>
</segment>
</net>
<net name="IO4">
<segment>
<pinref part="U4" gate="G$1" pin="IO4"/>
</segment>
<segment>
<pinref part="SL3" gate="G$1" pin="2"/>
</segment>
</net>
<net name="IO5">
<segment>
<pinref part="U4" gate="G$1" pin="IO5"/>
</segment>
<segment>
<pinref part="SL3" gate="G$1" pin="1"/>
</segment>
</net>
<net name="5V">
<segment>
<pinref part="SL1" gate="G$1" pin="3"/>
</segment>
<segment>
<pinref part="REGULATOR" gate="G$1" pin="3"/>
<pinref part="LED1" gate="G$1" pin="A"/>
<pinref part="C9" gate="1" pin="2"/>
</segment>
</net>
<net name="IO14">
<segment>
<pinref part="U4" gate="G$1" pin="IO14"/>
</segment>
<segment>
<pinref part="SL4" gate="G$1" pin="2"/>
</segment>
</net>
<net name="IO13">
<segment>
<pinref part="U4" gate="G$1" pin="IO13"/>
</segment>
<segment>
<pinref part="SL4" gate="G$1" pin="4"/>
</segment>
</net>
<net name="IO12">
<segment>
<pinref part="U4" gate="G$1" pin="IO12"/>
</segment>
<segment>
<pinref part="SL4" gate="G$1" pin="3"/>
</segment>
</net>
<net name="N$11">
<segment>
<pinref part="U4" gate="G$1" pin="ADC"/>
</segment>
</net>
<net name="IO16">
<segment>
<pinref part="U4" gate="G$1" pin="IO16"/>
</segment>
<segment>
<pinref part="SL4" gate="G$1" pin="1"/>
</segment>
</net>
<net name="SCL">
<segment>
<pinref part="U4" gate="G$1" pin="SCLK"/>
</segment>
<segment>
<pinref part="SL2" gate="G$1" pin="1"/>
</segment>
</net>
<net name="CS0">
<segment>
<pinref part="U4" gate="G$1" pin="CS0"/>
</segment>
<segment>
<pinref part="SL2" gate="G$1" pin="6"/>
</segment>
</net>
<net name="MOSI">
<segment>
<pinref part="U4" gate="G$1" pin="MOSI"/>
</segment>
<segment>
<pinref part="SL2" gate="G$1" pin="2"/>
</segment>
</net>
<net name="MISO">
<segment>
<pinref part="U4" gate="G$1" pin="MISO"/>
</segment>
<segment>
<pinref part="SL2" gate="G$1" pin="5"/>
</segment>
</net>
<net name="IO10">
<segment>
<pinref part="U4" gate="G$1" pin="IO10"/>
</segment>
<segment>
<pinref part="SL2" gate="G$1" pin="3"/>
</segment>
</net>
<net name="IO9">
<segment>
<pinref part="U4" gate="G$1" pin="IO9"/>
</segment>
<segment>
<pinref part="SL2" gate="G$1" pin="4"/>
</segment>
</net>
<net name="IO2">
<segment>
<pinref part="U4" gate="G$1" pin="IO2"/>
</segment>
<segment>
<pinref part="SL3" gate="G$1" pin="3"/>
</segment>
</net>
<net name="N$1">
<segment>
<pinref part="R2" gate="G$1" pin="2"/>
<pinref part="LED1" gate="G$1" pin="C"/>
</segment>
</net>
</nets>
</sheet>
</sheets>
</schematic>
</drawing>
</eagle>
